(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "ICP-20100"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 33.02 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "ICP-20100"
				(at 33.02 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "ICP-20100"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://product.tdk.com/system/files/dam/doc/product/sensor/pressure/capacitive-pressure/data_sheet/ds-000416-icp-20100.pdf"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Board Mount High Accuracy, Low Power, Barometric Pressure and Temperature Sensor"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "ICP-20100"
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "TDK"
				(at 33.02 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "DIGITAL, SENSOR, I2C, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "ICP-20100_1_1"
				(pin input line
					(at 0 -11.43 0)
					(length 2.54)
					(name "CSB")
					(number "1")
				)
				(pin input line
					(at 0 -8.89 0)
					(length 2.54)
					(name "SCL")
					(number "2")
				)
				(pin power_in line
					(at 19.05 -13.97 180)
					(length 2.54)
					(name "VSS")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 2.54)
					(name "SDA")
					(number "4")
					(alternate "SDI" bidirectional line)
					(alternate "SDIO" bidirectional line)
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDD")
					(number "5")
				)
				(pin output line
					(at 0 -13.97 0)
					(length 2.54)
					(name "SDO")
					(number "6")
					(alternate "AD0" input line)
				)
				(pin output line
					(at 19.05 0 180)
					(length 2.54)
					(name "INT")
					(number "7")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 2.54)
					(name "RESV")
					(number "8")
				)
				(pin passive line
					(at 19.05 -11.43 180)
					(length 2.54)
					(name "RESV")
					(number "9")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDDIO")
					(number "10")
				)
			)
			(embedded_fonts no)
		)
)
