(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "IM69D130"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "MK"
				(at 30.48 -1.27 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "IM69D130"
				(at 30.48 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "IM69D130"
				(at 30.48 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IM69D130-DS-v01_00-EN.pdf?fileId=5546d462602a9dc801607a0e46511a2e"
				(at 30.48 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Audio Control, MEMS Microphone, 1.62V to 3.6V, LGA, 5 Pins, -40 °C"
				(at 30.48 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "IM69D130"
				(at 30.48 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Infineon"
				(at 30.48 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 30.48 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 30.48 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MEMS, SENSOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "IM69D130_1_1"
				(pin output line
					(at 0 0 0)
					(length 2.54)
					(name "DATA")
					(number "1")
				)
				(pin power_in line
					(at 19.05 0 180)
					(length 2.54)
					(name "VDD")
					(number "2")
				)
				(pin input clock
					(at 0 -2.54 0)
					(length 2.54)
					(name "CLOCK")
					(number "3")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "SELECT")
					(number "4")
				)
				(pin power_in line
					(at 19.05 -5.08 180)
					(length 2.54)
					(name "GND")
					(number "5")
				)
			)
			(embedded_fonts no)
		)
)
