(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MK_IM73A135V01XTSA1"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "MK"
				(at 15.24 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MK_IM73A135V01XTSA1"
				(at 15.24 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MK_IM73A135V01XTSA1"
				(at 15.24 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-IM73A135-DataSheet-v01_00-EN.pdf?fileId=8ac78c8c7f2a768a017fadec36b84500"
				(at 15.24 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "MEMS Microphone, 2.3 V to 3 V, -40 C, LGA-5"
				(at 15.24 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Infineon"
				(at 15.24 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "IM73A135V01XTSA1"
				(at 15.24 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 15.24 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 15.24 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MEMS, SENSOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MK_IM73A135V01XTSA1_1_1"
				(pin output line
					(at 0 -5.08 180)
					(length 2.54)
					(name "OUTPUT+")
					(number "1")
				)
				(pin power_in line
					(at 0 0 180)
					(length 2.54)
					(name "VDD")
					(number "2")
				)
				(pin output line
					(at 0 -7.62 180)
					(length 2.54)
					(name "OUTPUT-")
					(number "3")
				)
				(pin power_in line
					(at 0 -12.7 180)
					(length 2.54)
					(name "GND")
					(number "4")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "5")
				)
			)
			(embedded_fonts no)
		)
)
