(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LM335AM"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 33.02 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LM335AM"
				(at 33.02 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LM335AM"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm135.pdf?HQS=dis-dk-null-digikeymode-dsf-pf-null-wwe&ts=1705317147743&ref_url=https%253A%252F%252Fwww.ti.com%252Fgeneral%252Fdocs%252Fsuppproductinfo.tsp%253FdistId%253D10%2526gotoUrl%253Dhttps%253A%252F%252Fwww.ti.com%252Flit%252Fgpn%252Flm135"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Temperature sensor, analog, local -40°C ~ 100°C 10mV/°K 8-SOIC"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LM335AM"
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 33.02 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "ANALOG, SENSOR, SMT, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LM335AM_1_1"
				(pin no_connect line
					(at 2.54 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "2")
				)
				(pin no_connect line
					(at 13.97 -2.54 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "3")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "V-")
					(number "4")
				)
				(pin input line
					(at 16.51 0 180)
					(length 2.54)
					(name "ADJ")
					(number "5")
				)
				(pin no_connect line
					(at 13.97 -3.81 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "6")
				)
				(pin no_connect line
					(at 13.97 -5.08 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "7")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V+")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
