(footprint "QSOP-16_3.9x4.9mm_P0.635mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "16-Lead Plastic Shrink Small Outline Narrow Body (QR)-.150\" Body [QSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
	(tags "SSOP 0.635")
	(property "Reference" "REF**"
		(at -1.55 -3.07 0)
		(layer "F.SilkS")
	)
	(property "Value" "QSOP-16_3.9x4.9mm_P0.635mm"
		(at -8.22 3.67 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -8.22 5.67 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -8.22 6.87 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -8.22 8.07 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -2.656 -2.223)
		(size 1.6 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -2.656 -1.589)
		(size 1.6 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -2.656 -0.954)
		(size 1.6 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -2.656 -0.318)
		(size 1.6 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -2.656 0.315)
		(size 1.6 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -2.656 0.951)
		(size 1.6 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -2.656 1.586)
		(size 1.6 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -2.656 2.221)
		(size 1.6 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 2.652 2.221)
		(size 1.6 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 2.652 1.586)
		(size 1.6 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 2.652 0.951)
		(size 1.6 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 2.652 0.315)
		(size 1.6 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 2.652 -0.318)
		(size 1.6 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 2.652 -0.954)
		(size 1.6 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 2.652 -1.589)
		(size 1.6 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 2.652 -2.223)
		(size 1.6 0.41)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_max1617amee_t.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
