(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MAX1617AMEE+T"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MAX1617AMEE+T"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MAX1617AMEE+T"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX1617.pdf"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Temperature sensor"
				(at 35.56 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MAX1617AMEE+T"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Maxim Integrated Products"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, SENSOR, IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MAX1617AMEE+T_1_1"
				(pin no_connect line
					(at 20.32 -21.59 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "1")
				)
				(pin power_in line
					(at 10.16 0 270)
					(length 2.54)
					(name "VCC")
					(number "2")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "DXP")
					(number "3")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "DXN")
					(number "4")
				)
				(pin no_connect line
					(at 20.32 -21.59 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "5")
				)
				(pin input line
					(at 0 -19.05 0)
					(length 2.54)
					(name "ADD1")
					(number "6")
				)
				(pin power_in line
					(at 10.16 -26.67 90)
					(length 2.54)
					(name "GND")
					(number "7")
				)
				(pin passive line
					(at 10.16 -26.67 90)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "8")
				)
				(pin no_connect line
					(at 20.32 -21.59 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "9")
				)
				(pin input line
					(at 0 -16.51 0)
					(length 2.54)
					(name "ADD0")
					(number "10")
				)
				(pin output line
					(at 20.32 -16.51 180)
					(length 2.54)
					(name "~{ALERT}")
					(number "11")
				)
				(pin bidirectional line
					(at 20.32 -10.16 180)
					(length 2.54)
					(name "SMBDATA")
					(number "12")
				)
				(pin no_connect line
					(at 20.32 -21.59 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "13")
				)
				(pin input clock
					(at 20.32 -12.7 180)
					(length 2.54)
					(name "SMBCLK")
					(number "14")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 2.54)
					(name "STBY")
					(number "15")
				)
				(pin no_connect line
					(at 20.32 -21.59 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "16")
				)
			)
			(embedded_fonts no)
		)
)
