(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MAX31730AUB+"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MAX31730AUB+"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MAX31730AUB+"
				(at 38.1 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX31730.pdf"
				(at 38.1 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "3-Channel remote temperature sensor, 3-3.6V, I2C"
				(at 38.1 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MAX31730AUB+"
				(at 38.1 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Analog Devices"
				(at 38.1 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "I2C, SENSOR, IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MAX31730AUB+_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 2.54)
					(name "DXP1")
					(number "2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "DXN")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "DXP2")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "DXP3")
					(number "5")
				)
				(pin passive line
					(at 25.4 -10.16 180)
					(length 2.54)
					(name "GND")
					(number "6")
				)
				(pin passive line
					(at 25.4 -7.62 180)
					(length 2.54)
					(name "~{THERM}")
					(number "7")
				)
				(pin passive line
					(at 25.4 -5.08 180)
					(length 2.54)
					(name "ADD")
					(number "8")
				)
				(pin passive line
					(at 25.4 -2.54 180)
					(length 2.54)
					(name "SDA")
					(number "9")
				)
				(pin passive line
					(at 25.4 0 180)
					(length 2.54)
					(name "SCL")
					(number "10")
				)
			)
			(embedded_fonts no)
		)
)
