(footprint "TDFN-8-1EP_2x3x0.75mm_P0.5mm_EP1.75x1.63mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "8-Lead Plastic Dual Flat, 2x3mm Body")
	(tags "DFN 0.5")
	(property "Reference" "REF**"
		(at -1 -1.3 0)
		(layer "F.SilkS")
	)
	(property "Value" "TDFN-8-1EP_2x3x0.75mm_P0.5mm_EP1.75x1.63mm"
		(at -2.1 3 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "License: Apache-2.0"
		(at -2.12 5 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -2.12 6.2 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -2.12 7.4 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.5 -0.75 90)
		(size 0.3 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.5 -0.25 90)
		(size 0.3 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.5 0.25 90)
		(size 0.3 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.5 0.75 90)
		(size 0.3 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1.5 0.75 90)
		(size 0.3 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 1.5 0.25 90)
		(size 0.3 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 1.5 -0.25 90)
		(size 0.3 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 1.5 -0.75 90)
		(size 0.3 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 0 0 90)
		(size 1.63 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_max31740ata_t.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
