(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MAX31740ATA+T"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MAX31740ATA+T"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MAX31740ATA+T"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/max31740.pdf"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Pwm fan speed controller, temperature measurement, Control speed of 2-, 3-, 4- Wire Fans"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MAX31740ATA+T"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Analog Devices"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SENSOR, IC, SMT, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MAX31740ATA+T_1_1"
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "DMIN")
					(number "1")
				)
				(pin passive line
					(at 22.86 -7.62 180)
					(length 2.54)
					(name "SLOPE")
					(number "2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "SENSE")
					(number "3")
				)
				(pin power_in line
					(at 22.86 -15.24 180)
					(length 2.54)
					(name "GND")
					(number "4")
				)
				(pin passive line
					(at 22.86 -5.08 180)
					(length 2.54)
					(name "FREQ")
					(number "5")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "D0")
					(number "6")
				)
				(pin output line
					(at 22.86 0 180)
					(length 2.54)
					(name "PWM_OUT")
					(number "7")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "8")
				)
				(pin power_in line
					(at 22.86 -12.7 180)
					(length 2.54)
					(name "EP")
					(number "9")
				)
			)
			(embedded_fonts no)
		)
)
