(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MAX6643_QSOP"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MAX6643_QSOP"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MAX6643_QSOP"
				(at 38.1 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX6643-MAX6645.pdf"
				(at 38.1 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "PWM Controller, Overtemperature Output, 3V to 5.5V Supply, 32Hz, QSOP-16"
				(at 38.1 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Analog Devices"
				(at 38.1 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MAX6643LBBAEE+"
				(at 38.1 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "CONTROLLER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MAX6643_QSOP_1_1"
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "TH1")
					(number "1")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "TL2")
					(number "2")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "TL1")
					(number "3")
				)
				(pin output line
					(at 24.13 -5.08 180)
					(length 2.54)
					(name "~{FANFAIL}")
					(number "4")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "TACHSET")
					(number "5")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "FULLSPD")
					(number "6")
				)
				(pin power_in line
					(at 24.13 -27.94 180)
					(length 2.54)
					(name "GND")
					(number "7")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "DXP")
					(number "8")
				)
				(pin output line
					(at 24.13 -2.54 180)
					(length 2.54)
					(name "~{OT}")
					(number "9")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "FAN_IN2")
					(number "10")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "FAN_IN1")
					(number "11")
				)
				(pin output line
					(at 24.13 0 180)
					(length 2.54)
					(name "PWM_OUT")
					(number "12")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "OT2")
					(number "13")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "OT1")
					(number "14")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "TH2")
					(number "15")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "16")
				)
			)
			(embedded_fonts no)
		)
)
