(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MC3635"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 34.29 -1.27 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MC3635"
				(at 34.29 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MC3635"
				(at 34.29 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/821/MEMSIC_MC3635_Datasheet-1878925.pdf"
				(at 34.29 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Accelerometers Digital Output 3 Axis Acceleronmeter"
				(at 34.29 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MC3635"
				(at 34.29 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "MEMSIC"
				(at 34.29 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 34.29 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 34.29 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, SENSOR, IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MC3635_1_1"
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "DOUT_A1")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "DIN_SDA")
					(number "2")
				)
				(pin no_connect line
					(at 19.05 -5.08 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "3")
				)
				(pin power_in line
					(at 21.59 -7.62 180)
					(length 2.54)
					(name "VPP")
					(number "4")
				)
				(pin output line
					(at 0 -2.54 0)
					(length 2.54)
					(name "INTN")
					(number "5")
				)
				(pin power_in line
					(at 21.59 -2.54 180)
					(length 2.54)
					(name "VDDIO")
					(number "6")
				)
				(pin power_in line
					(at 21.59 0 180)
					(length 2.54)
					(name "VDD")
					(number "7")
				)
				(pin power_in line
					(at 21.59 -10.16 180)
					(length 2.54)
					(name "GND")
					(number "8")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "CSN")
					(number "9")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "SCK_SCL")
					(number "10")
				)
			)
			(embedded_fonts no)
		)
)
