(footprint "OV5640"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -3.37 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "OV5640"
		(at 0 4.27 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0.5 -0.58 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0.5 -0.58 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -3.25 5.8 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -3.25 7 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -3.25 8.2 0)
		(layer "F.Fab")
	)
	(pad "A2" smd circle
		(at -1.99 -2.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd circle
		(at -1.49 -2.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd circle
		(at -0.99 -2.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A5" smd circle
		(at -0.49 -2.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A6" smd circle
		(at 0.005 -2.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A7" smd circle
		(at 0.505 -2.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A8" smd circle
		(at 1.005 -2.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A9" smd circle
		(at 1.505 -2.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A10" smd circle
		(at 2.005 -2.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A11" smd circle
		(at 2.505 -2.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd circle
		(at -2.49 -2)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B2" smd circle
		(at -1.99 -2)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B3" smd circle
		(at -1.49 -2)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B4" smd circle
		(at -0.99 -2)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B5" smd circle
		(at -0.49 -2)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B6" smd circle
		(at 0.005 -2)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B7" smd circle
		(at 0.505 -2)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B8" smd circle
		(at 1.005 -2)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B9" smd circle
		(at 1.505 -2)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B10" smd circle
		(at 2.005 -2)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B11" smd circle
		(at 2.505 -2)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C1" smd circle
		(at -2.49 -1.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C2" smd circle
		(at -1.99 -1.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C3" smd circle
		(at -1.49 -1.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C10" smd circle
		(at 2.005 -1.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C11" smd circle
		(at 2.505 -1.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D1" smd circle
		(at -2.49 -1)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D2" smd circle
		(at -1.99 -1)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D10" smd circle
		(at 2.005 -1)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D11" smd circle
		(at 2.505 -1)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E1" smd circle
		(at -2.49 -0.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E2" smd circle
		(at -1.99 -0.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E10" smd circle
		(at 2.005 -0.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E11" smd circle
		(at 2.505 -0.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F1" smd circle
		(at -2.49 0)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F2" smd circle
		(at -1.99 0)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F10" smd circle
		(at 2.005 0)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F11" smd circle
		(at 2.505 0)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G1" smd circle
		(at -2.49 0.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G2" smd circle
		(at -1.99 0.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G10" smd circle
		(at 2.005 0.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G11" smd circle
		(at 2.505 0.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H1" smd circle
		(at -2.49 1)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H2" smd circle
		(at -1.99 1)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H10" smd circle
		(at 2.005 1)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H11" smd circle
		(at 2.505 1)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "I1" smd circle
		(at -2.49 1.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "I2" smd circle
		(at -1.99 1.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "I8" smd circle
		(at 1.005 1.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "I9" smd circle
		(at 1.505 1.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "I10" smd circle
		(at 2.005 1.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "I11" smd circle
		(at 2.505 1.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J1" smd circle
		(at -2.49 2)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J2" smd circle
		(at -1.99 2)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J3" smd circle
		(at -1.49 2)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J4" smd circle
		(at -0.99 2)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J5" smd circle
		(at -0.49 2)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J6" smd circle
		(at 0.005 2)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J7" smd circle
		(at 0.505 2)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J9" smd circle
		(at 1.505 2)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J10" smd circle
		(at 2.005 2)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J11" smd circle
		(at 2.505 2)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K1" smd circle
		(at -2.49 2.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K2" smd circle
		(at -1.99 2.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K3" smd circle
		(at -1.49 2.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K4" smd circle
		(at -0.99 2.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K5" smd circle
		(at -0.49 2.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K6" smd circle
		(at 0.005 2.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K7" smd circle
		(at 0.505 2.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K8" smd circle
		(at 1.005 2.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K11" smd circle
		(at 2.505 2.5)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_ov5640.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
