(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "OV5640"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 64.77 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "OV5640"
				(at 64.77 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Footprint" "OV5640"
				(at 64.77 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://cdn.sparkfun.com/datasheets/Sensors/LightImaging/OV5640_datasheet.pdf"
				(at 64.77 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Color CMOS QSXGA 5 megapixel image sensor with OmniBSI technology"
				(at 64.77 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "OV5640"
				(at 64.77 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "OmniVision"
				(at 64.77 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 64.77 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 64.77 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SENSOR, CMOS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "OV5640_1_1"
				(text "1/4\""
					(at 20.32 -13.97 0)
				)
				(text "CMOS"
					(at 20.32 -16.51 0)
				)
				(text "QSXGA"
					(at 20.32 -19.05 0)
				)
				(pin input line
					(at 48.26 -34.29 180)
					(length 3.81)
					(name "VCMSINK")
					(number "A2")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "AVDD")
					(number "A3")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "A4")
				)
				(pin power_in line
					(at 0 -39.37 0)
					(length 3.81)
					(name "DGND")
					(number "A5")
				)
				(pin no_connect line
					(at 3.81 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "A6")
					(number "A6")
				)
				(pin no_connect line
					(at 3.81 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "A7")
					(number "A7")
				)
				(pin no_connect line
					(at 3.81 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "A8")
					(number "A8")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(name "DVDD")
					(number "A9")
				)
				(pin power_in line
					(at 0 -36.83 0)
					(length 3.81)
					(name "AGND")
					(number "A10")
				)
				(pin no_connect line
					(at 3.81 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "A11")
					(number "A11")
				)
				(pin passive line
					(at 0 -39.37 0)
					(length 3.81)
					(hide yes)
					(name "DGND")
					(number "B1")
				)
				(pin passive line
					(at 48.26 -34.29 180)
					(length 3.81)
					(hide yes)
					(name "VCMSINK")
					(number "B2")
				)
				(pin power_in line
					(at 0 -41.91 0)
					(length 3.81)
					(name "VCMGND")
					(number "B3")
				)
				(pin passive line
					(at 0 -41.91 0)
					(length 3.81)
					(hide yes)
					(name "VCMGND")
					(number "B4")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "DVDD")
					(number "B5")
				)
				(pin no_connect line
					(at 3.81 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "B6")
					(number "B6")
				)
				(pin no_connect line
					(at 3.81 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "B7")
					(number "B7")
				)
				(pin no_connect line
					(at 3.81 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "B8")
					(number "B8")
				)
				(pin passive line
					(at 0 -39.37 0)
					(length 3.81)
					(hide yes)
					(name "DGND")
					(number "B9")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "AVDD")
					(number "B10")
				)
				(pin passive line
					(at 48.26 -40.64 180)
					(length 3.81)
					(name "VN")
					(number "B11")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "DVDD")
					(number "C1")
				)
				(pin passive line
					(at 0 -39.37 0)
					(length 3.81)
					(hide yes)
					(name "DGND")
					(number "C2")
				)
				(pin no_connect line
					(at 3.81 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "C3")
					(number "C3")
				)
				(pin passive line
					(at 48.26 -38.1 180)
					(length 3.81)
					(name "VH")
					(number "C10")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "AVDD")
					(number "C11")
				)
				(pin input line
					(at 0 -13.97 0)
					(length 3.81)
					(name "PWDN")
					(number "D1")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "DVDD")
					(number "D2")
				)
				(pin no_connect line
					(at 3.81 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "D10")
					(number "D10")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 3.81)
					(hide yes)
					(name "AGND")
					(number "D11")
				)
				(pin output line
					(at 48.26 -31.75 180)
					(length 3.81)
					(name "STROBE")
					(number "E1")
				)
				(pin input line
					(at 0 -16.51 0)
					(length 3.81)
					(name "RESETB")
					(number "E2")
				)
				(pin no_connect line
					(at 3.81 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "E10")
					(number "E10")
				)
				(pin no_connect line
					(at 3.81 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "E11")
					(number "E11")
				)
				(pin bidirectional line
					(at 48.26 0 180)
					(length 3.81)
					(name "GPIO0")
					(number "F1")
				)
				(pin output line
					(at 48.26 -44.45 180)
					(length 3.81)
					(name "FREX")
					(number "F2")
				)
				(pin no_connect line
					(at 3.81 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "F10")
					(number "F10")
				)
				(pin power_in line
					(at 0 -46.99 0)
					(length 3.81)
					(name "SGND")
					(number "F11")
				)
				(pin bidirectional line
					(at 48.26 -2.54 180)
					(length 3.81)
					(name "GPIO1")
					(number "G1")
				)
				(pin power_in line
					(at 0 -44.45 0)
					(length 3.81)
					(name "DOGND")
					(number "G2")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 3.81)
					(name "SCL")
					(number "G10")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "SDA")
					(number "G11")
				)
				(pin output line
					(at 48.26 -49.53 180)
					(length 3.81)
					(name "VSYNC")
					(number "H1")
				)
				(pin output line
					(at 48.26 -46.99 180)
					(length 3.81)
					(name "HREF")
					(number "H2")
				)
				(pin output line
					(at 48.26 -12.7 180)
					(length 3.81)
					(name "D3")
					(number "H10")
				)
				(pin input line
					(at 0 -26.67 0)
					(length 3.81)
					(name "XVCLK")
					(number "H11")
				)
				(pin output line
					(at 0 -29.21 0)
					(length 3.81)
					(name "PCLK")
					(number "I1")
				)
				(pin passive line
					(at 0 -39.37 0)
					(length 3.81)
					(hide yes)
					(name "DGND")
					(number "I2")
				)
				(pin bidirectional line
					(at 48.26 -20.32 180)
					(length 3.81)
					(name "D6")
					(number "I8")
					(alternate "MCN" passive line)
				)
				(pin bidirectional line
					(at 48.26 -22.86 180)
					(length 3.81)
					(name "D7")
					(number "I9")
					(alternate "MCP" passive line)
				)
				(pin input line
					(at 0 -10.16 0)
					(length 3.81)
					(name "PVDD")
					(number "I10")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "DVDD")
					(number "I11")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "DVDD")
					(number "J1")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(name "DOVDD")
					(number "J2")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "DOVDD")
					(number "J3")
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 3.81)
					(hide yes)
					(name "DOGND")
					(number "J4")
				)
				(pin output line
					(at 48.26 -10.16 180)
					(length 3.81)
					(name "D2")
					(number "J5")
				)
				(pin no_connect line
					(at 3.81 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "J6")
					(number "J6")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 3.81)
					(name "EVDD")
					(number "J7")
				)
				(pin output line
					(at 48.26 -25.4 180)
					(length 3.81)
					(name "D8")
					(number "J9")
					(alternate "MDN1" passive line)
				)
				(pin output line
					(at 48.26 -27.94 180)
					(length 3.81)
					(name "D9")
					(number "J10")
					(alternate "MDP1" passive line)
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 3.81)
					(hide yes)
					(name "DOGND")
					(number "J11")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "DVDD")
					(number "K1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "DOVDD")
					(number "K2")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "DOVDD")
					(number "K3")
				)
				(pin bidirectional line
					(at 48.26 -7.62 180)
					(length 3.81)
					(name "D1")
					(number "K4")
					(alternate "GPIO3" passive line)
				)
				(pin bidirectional line
					(at 48.26 -5.08 180)
					(length 3.81)
					(name "D0")
					(number "K5")
					(alternate "GPIO2" passive line)
				)
				(pin output line
					(at 48.26 -15.24 180)
					(length 3.81)
					(name "D4")
					(number "K6")
					(alternate "MDN0" passive line)
				)
				(pin output line
					(at 48.26 -17.78 180)
					(length 3.81)
					(name "D5")
					(number "K7")
					(alternate "MDP0" passive line)
				)
				(pin passive line
					(at 0 -49.53 0)
					(length 3.81)
					(hide yes)
					(name "EGND")
					(number "K8")
				)
				(pin power_in line
					(at 0 -49.53 0)
					(length 3.81)
					(name "EGND")
					(number "K11")
				)
			)
			(embedded_fonts no)
		)
)
