(footprint "OV9281"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr " B&W CMOS 1 Megapixel (1280x800) Image Sensor with OmniPixel®3‑GS Technology ")
	(tags "CMOS, Sensor, Image")
	(property "Reference" "REF**"
		(at -1.8 -2.575 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "ImageSensor_OV9281"
		(at -3.2475 3.164 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Sensor offset:"
		(at -1.9 -0.5 0)
		(layer "Cmts.User")
	)
	(fp_text user "X: 247,5 um, Y: -36 um"
		(at -1.9 0.4 0)
		(layer "Cmts.User")
	)
	(fp_text user "Author: Antmicro"
		(at -3.2575 5.164 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -3.2575 6.364 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -3.2575 7.564 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -2.4875 -1.786)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "A2" smd circle
		(at -1.8475 -1.786)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "A3" smd circle
		(at -1.2075 -1.786)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "A4" smd circle
		(at -0.5675 -1.786)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "A5" smd circle
		(at 0.0725 -1.786)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "A6" smd circle
		(at 0.7125 -1.786)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "A7" smd circle
		(at 1.3525 -1.786)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "A8" smd circle
		(at 1.9925 -1.786)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "B1" smd circle
		(at -2.4875 -1.286)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "B2" smd circle
		(at -1.8475 -1.286)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "B3" smd circle
		(at -1.2075 -1.286)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "B4" smd circle
		(at -0.5675 -1.286)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "B5" smd circle
		(at 0.0725 -1.286)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "B6" smd circle
		(at 0.7125 -1.286)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "B7" smd circle
		(at 1.3525 -1.286)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "B8" smd circle
		(at 1.9925 -1.286)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "C1" smd circle
		(at -2.4875 -0.786)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "C2" smd circle
		(at -1.8475 -0.786)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "C3" smd circle
		(at -1.2075 -0.786)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "C4" smd circle
		(at -0.5675 -0.786)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "C5" smd circle
		(at 0.0725 -0.786)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "C6" smd circle
		(at 0.7125 -0.786)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "C7" smd circle
		(at 1.3525 -0.786)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "C8" smd circle
		(at 1.9925 -0.786)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "D1" smd circle
		(at -2.4875 -0.286)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "D2" smd circle
		(at -1.8475 -0.286)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "D3" smd circle
		(at -1.2075 -0.286)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "D4" smd circle
		(at -0.5675 -0.286)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "D5" smd circle
		(at 0.0725 -0.286)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "D6" smd circle
		(at 0.7125 -0.286)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "D7" smd circle
		(at 1.3525 -0.286)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "D8" smd circle
		(at 1.9925 -0.286)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "E1" smd circle
		(at -2.4875 0.214)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "E2" smd circle
		(at -1.8475 0.214)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "E3" smd circle
		(at -1.2075 0.214)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "E4" smd circle
		(at -0.5675 0.214)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "E5" smd circle
		(at 0.0725 0.214)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "E6" smd circle
		(at 0.7125 0.214)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "E7" smd circle
		(at 1.3525 0.214)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "E8" smd circle
		(at 1.9925 0.214)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "F1" smd circle
		(at -2.4875 0.714)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "F2" smd circle
		(at -1.8475 0.714)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "F3" smd circle
		(at -1.2075 0.714)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "F4" smd circle
		(at -0.5675 0.714)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "F5" smd circle
		(at 0.0725 0.714)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "F6" smd circle
		(at 0.7125 0.714)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "F7" smd circle
		(at 1.3525 0.714)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "F8" smd circle
		(at 1.9925 0.714)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "G1" smd circle
		(at -2.4875 1.214)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "G2" smd circle
		(at -1.8475 1.214)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "G3" smd circle
		(at -1.2075 1.214)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "G4" smd circle
		(at -0.5675 1.214)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "G5" smd circle
		(at 0.0725 1.214)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "G6" smd circle
		(at 0.7125 1.214)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "G7" smd circle
		(at 1.3525 1.214)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "G8" smd circle
		(at 1.9925 1.214)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "H1" smd circle
		(at -2.4875 1.714)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "H2" smd circle
		(at -1.8475 1.714)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "H3" smd circle
		(at -1.2075 1.714)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "H4" smd circle
		(at -0.5675 1.714)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "H5" smd circle
		(at 0.0725 1.714)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "H6" smd circle
		(at 0.7125 1.714)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "H7" smd circle
		(at 1.3525 1.714)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(pad "H8" smd circle
		(at 1.9925 1.714)
		(size 0.2 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin 0.05)
	)
	(embedded_fonts no)
	(model "antmicro_ov9281.glb"
		(offset
			(xyz -0.2475 0.036 0.68)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 -180 0)
		)
	)
)
