(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "OV9281"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 48.895 -3.175 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "OV9281"
				(at 48.895 -15.875 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "OV9281"
				(at 48.895 -18.415 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ovt.com/wp-content/uploads/2022/01/OV9281-OV9282-PB-v1.3-WEB.pdf"
				(at 48.895 -20.955 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "B&W CMOS 1 Megapixel (1280x800) Image Sensor with OmniPixel®3‑GS Technology"
				(at 48.895 -23.495 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "OV9281"
				(at 48.895 -5.715 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "OmniVision"
				(at 48.895 -8.255 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 48.895 -10.795 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 48.895 -13.335 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SENSOR, CMOS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "OV9281_1_1"
				(pin no_connect line
					(at 2.54 -49.53 0)
					(length 2.54)
					(hide yes)
					(name "")
					(number "A1")
				)
				(pin passive line
					(at 0 -3.81 0)
					(length 2.54)
					(name "DVDD")
					(number "A2")
				)
				(pin power_in line
					(at 0 -67.31 0)
					(length 2.54)
					(name "DOGND")
					(number "A3")
				)
				(pin passive line
					(at 36.83 -20.32 180)
					(length 2.54)
					(name "SDA")
					(number "A4")
				)
				(pin passive line
					(at 36.83 -31.75 180)
					(length 2.54)
					(name "XSHUTDOWN")
					(number "A5")
				)
				(pin passive line
					(at 36.83 -67.31 180)
					(length 2.54)
					(name "ILPWM")
					(number "A6")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 2.54)
					(hide yes)
					(name "DOGND")
					(number "A7")
				)
				(pin no_connect line
					(at 2.54 -50.8 0)
					(length 2.54)
					(hide yes)
					(name "")
					(number "A8")
				)
				(pin passive line
					(at 0 -3.81 0)
					(length 2.54)
					(hide yes)
					(name "DVDD")
					(number "B1")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 2.54)
					(hide yes)
					(name "DOGND")
					(number "B2")
				)
				(pin passive line
					(at 0 -3.81 0)
					(length 2.54)
					(hide yes)
					(name "DVDD")
					(number "B3")
				)
				(pin passive line
					(at 36.83 -52.07 180)
					(length 2.54)
					(name "D8")
					(number "B4")
				)
				(pin passive line
					(at 36.83 -36.83 180)
					(length 2.54)
					(name "FSIN/VSYNC")
					(number "B5")
				)
				(pin passive line
					(at 36.83 -34.29 180)
					(length 2.54)
					(name "STROBE")
					(number "B6")
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 2.54)
					(name "DOVDD")
					(number "B7")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "AVDD")
					(number "B8")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "AVDD")
					(number "C1")
				)
				(pin passive line
					(at 36.83 -25.4 180)
					(length 2.54)
					(name "PCLK")
					(number "C2")
				)
				(pin passive line
					(at 36.83 -44.45 180)
					(length 2.54)
					(name "GPIO1")
					(number "C3")
				)
				(pin passive line
					(at 36.83 -49.53 180)
					(length 2.54)
					(name "D9")
					(number "C4")
				)
				(pin passive line
					(at 0 -3.81 0)
					(length 2.54)
					(hide yes)
					(name "DVDD")
					(number "C5")
				)
				(pin passive line
					(at 36.83 -54.61 180)
					(length 2.54)
					(name "ULPM")
					(number "C6")
				)
				(pin passive line
					(at 36.83 -64.77 180)
					(length 2.54)
					(name "TEST")
					(number "C7")
				)
				(pin passive line
					(at 0 -64.77 0)
					(length 2.54)
					(name "AGND")
					(number "C8")
				)
				(pin passive line
					(at 36.83 -59.69 180)
					(length 2.54)
					(name "HREF")
					(number "D1")
				)
				(pin passive line
					(at 0 -64.77 0)
					(length 2.54)
					(hide yes)
					(name "AGND")
					(number "D2")
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 2.54)
					(hide yes)
					(name "DOVDD")
					(number "D3")
				)
				(pin passive line
					(at 36.83 -46.99 180)
					(length 2.54)
					(name "GPIO0")
					(number "D4")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "PVDD")
					(number "D5")
				)
				(pin passive line
					(at 36.83 -41.91 180)
					(length 2.54)
					(name "GPIO2")
					(number "D6")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 2.54)
					(name "VN1")
					(number "D7")
				)
				(pin passive line
					(at 0 -3.81 0)
					(length 2.54)
					(hide yes)
					(name "DVDD")
					(number "D8")
				)
				(pin passive line
					(at 36.83 -62.23 180)
					(length 2.54)
					(name "SID")
					(number "E1")
				)
				(pin passive line
					(at 36.83 -27.94 180)
					(length 2.54)
					(name "XVCLK")
					(number "E2")
				)
				(pin passive line
					(at 0 -62.23 0)
					(length 2.54)
					(name "EGND")
					(number "E3")
				)
				(pin passive line
					(at 36.83 -17.78 180)
					(length 2.54)
					(name "SCL")
					(number "E4")
				)
				(pin passive line
					(at 0 -62.23 0)
					(length 2.54)
					(hide yes)
					(name "EGND")
					(number "E5")
				)
				(pin passive line
					(at 36.83 -57.15 180)
					(length 2.54)
					(name "TM")
					(number "E6")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 2.54)
					(name "VN2")
					(number "E7")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(name "VH")
					(number "E8")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 2.54)
					(hide yes)
					(name "DOGND")
					(number "F1")
				)
				(pin passive line
					(at 0 -3.81 0)
					(length 2.54)
					(hide yes)
					(name "DVDD")
					(number "F2")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 2.54)
					(name "EVDD")
					(number "F3")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 2.54)
					(hide yes)
					(name "DOGND")
					(number "F4")
				)
				(pin passive line
					(at 36.83 -7.62 180)
					(length 2.54)
					(name "MD1N")
					(number "F5")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 2.54)
					(hide yes)
					(name "DOGND")
					(number "F6")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(name "VN3")
					(number "F7")
				)
				(pin passive line
					(at 0 -64.77 0)
					(length 2.54)
					(hide yes)
					(name "AGND")
					(number "F8")
				)
				(pin passive line
					(at 0 -3.81 0)
					(length 2.54)
					(hide yes)
					(name "DVDD")
					(number "G1")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 2.54)
					(hide yes)
					(name "DOGND")
					(number "G2")
				)
				(pin passive line
					(at 36.83 -10.16 180)
					(length 2.54)
					(name "MDP0")
					(number "G3")
				)
				(pin passive line
					(at 36.83 0 180)
					(length 2.54)
					(name "MDCP")
					(number "G4")
				)
				(pin passive line
					(at 36.83 -5.08 180)
					(length 2.54)
					(name "MDP1")
					(number "G5")
				)
				(pin passive line
					(at 0 -3.81 0)
					(length 2.54)
					(hide yes)
					(name "DVDD")
					(number "G6")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "AVDD")
					(number "G7")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "AVDD")
					(number "G8")
				)
				(pin no_connect line
					(at 2.54 -52.07 0)
					(length 2.54)
					(hide yes)
					(name "")
					(number "H1")
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 2.54)
					(hide yes)
					(name "DOVDD")
					(number "H2")
				)
				(pin passive line
					(at 36.83 -12.7 180)
					(length 2.54)
					(name "MDN0")
					(number "H3")
				)
				(pin passive line
					(at 36.83 -2.54 180)
					(length 2.54)
					(name "MDCN")
					(number "H4")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 2.54)
					(hide yes)
					(name "EVDD")
					(number "H5")
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 2.54)
					(hide yes)
					(name "DOVDD")
					(number "H6")
				)
				(pin passive line
					(at 0 -64.77 0)
					(length 2.54)
					(hide yes)
					(name "AGND")
					(number "H7")
				)
				(pin no_connect line
					(at 2.54 -53.34 0)
					(length 2.54)
					(hide yes)
					(name "")
					(number "H8")
				)
			)
			(embedded_fonts no)
		)
)
