(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "P3T1085UK"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 33.02 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "P3T1085UK"
				(at 33.02 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "P3T1085UK"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/P3T1085UK.pdf"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "1.4V-Capable ±0.5°C Temperature Sensor, I2C, I3C"
				(at 33.02 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "P3T1085UKZ"
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "NXP"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "DIGITAL, SENSOR, I2C, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "P3T1085UK_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V+")
					(number "A1")
				)
				(pin power_in line
					(at 17.78 -7.62 180)
					(length 2.54)
					(name "GND")
					(number "A2")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "A0")
					(number "B1")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "SCL")
					(number "B2")
				)
				(pin output line
					(at 17.78 -5.08 180)
					(length 2.54)
					(name "~{ALERT}")
					(number "C1")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "SDA")
					(number "C2")
				)
			)
			(embedded_fonts no)
		)
)
