(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "PAC1934T_WLCSP"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 50.8 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "PAC1934T_WLCSP"
				(at 50.8 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "PAC1934T_WLCSP"
				(at 50.8 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/268/PAC1931_Family_Data_Sheet_DS20005850E-1519053.pdf"
				(at 50.8 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "DC Power/Energy Monitor With Accumulator, Quad High-side current Sensor, 2.7V to 5.5V, WLCSP-16"
				(at 50.8 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 50.8 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "PAC1934T-I/J6CX"
				(at 50.8 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 50.8 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 50.8 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, PMIC, SMT, MONITOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "PAC1934T_WLCSP_1_1"
				(pin input line
					(at 27.94 -5.08 180)
					(length 2.54)
					(name "SENSE2+")
					(number "A1")
				)
				(pin input line
					(at 27.94 -2.54 180)
					(length 2.54)
					(name "SENSE1-")
					(number "A2")
				)
				(pin input line
					(at 27.94 0 180)
					(length 2.54)
					(name "SENSE1+")
					(number "A3")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDD")
					(number "A4")
				)
				(pin input line
					(at 27.94 -7.62 180)
					(length 2.54)
					(name "SENSE2-")
					(number "B1")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD_I/O")
					(number "B2")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "~{PWRDN}")
					(number "B3")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 2.54)
					(name "GND")
					(number "B4")
				)
				(pin input line
					(at 27.94 -12.7 180)
					(length 2.54)
					(name "SENSE3-")
					(number "C1")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "ADDRSEL")
					(number "C2")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "SLOW/~{ALERT}")
					(number "C3")
				)
				(pin input clock
					(at 0 -5.08 0)
					(length 2.54)
					(name "SM_CLK")
					(number "C4")
				)
				(pin input line
					(at 27.94 -10.16 180)
					(length 2.54)
					(name "SENSE3+")
					(number "D1")
				)
				(pin input line
					(at 27.94 -17.78 180)
					(length 2.54)
					(name "SENSE4-")
					(number "D2")
				)
				(pin input line
					(at 27.94 -15.24 180)
					(length 2.54)
					(name "SENSE4+")
					(number "D3")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "SM_DATA")
					(number "D4")
				)
			)
			(embedded_fonts no)
		)
)
