(footprint "Sensirion_DFN-4-1.5x1.5x0.5mm_P0.8mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Sensiron's 4-pin 1.5mm x 1.5mm Dual Flat No-Lead, used for SHT4x series I²C Humidity & Temperature Sensors, 0.5mm Height. Based on \"Recommended land pattern\" from SHT4x Datasheet V3: https://sensirion.com/media/documents/33FD6951/624C4357/Datasheet_SHT4x.pdf")
	(tags "dfn4 DFN-4 sensirion sht4x SHT40 SHT41 SHT45")
	(property "Reference" "REF**"
		(at 0.001 1.499 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Sensirion_DFN-4-1.5x1.5x0.5mm_P0.8mm"
		(at 0.001 -2.202 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Author: Antmicro"
		(at -1.258 3.499 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -1.258 4.699 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -1.258 5.899 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.701 -0.403)
		(size 0.5 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -0.701 0.401)
		(size 0.5 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at 0.699 0.401)
		(size 0.5 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at 0.699 -0.403)
		(size 0.5 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "antmicro_sht45_ad1b_r2.glb"
		(offset
			(xyz 0.001 -0.001 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
