(footprint "VQFN-48_7x7mm_P0.5mm_EP4.1x4.1mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -4.6 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "VQFN-48_7x7mm_P0.5mm_EP4.1x4.1mm"
		(at 0 5.3 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -5.13 6.78 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -5.13 7.98 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -5.13 9.18 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -3.475 -2.75 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "2" smd roundrect
		(at -3.475 -2.25 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "3" smd roundrect
		(at -3.475 -1.75 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "4" smd roundrect
		(at -3.475 -1.25 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "5" smd roundrect
		(at -3.475 -0.75 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "6" smd roundrect
		(at -3.475 -0.25 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "7" smd roundrect
		(at -3.475 0.25 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "8" smd roundrect
		(at -3.475 0.75 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "9" smd roundrect
		(at -3.475 1.25 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "10" smd roundrect
		(at -3.475 1.75 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "11" smd roundrect
		(at -3.475 2.25 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "12" smd roundrect
		(at -3.475 2.75 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "13" smd roundrect
		(at -2.75 3.475 180)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "14" smd roundrect
		(at -2.25 3.475 180)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "15" smd roundrect
		(at -1.75 3.475 180)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "16" smd roundrect
		(at -1.25 3.475 180)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "17" smd roundrect
		(at -0.75 3.475 180)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "18" smd roundrect
		(at -0.25 3.475 180)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "19" smd roundrect
		(at 0.25 3.475 180)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "20" smd roundrect
		(at 0.75 3.475 180)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "21" smd roundrect
		(at 1.25 3.475 180)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "22" smd roundrect
		(at 1.75 3.475 180)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "23" smd roundrect
		(at 2.25 3.475 180)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "24" smd roundrect
		(at 2.75 3.475 180)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "25" smd roundrect
		(at 3.475 2.75 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "26" smd roundrect
		(at 3.475 2.25 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "27" smd roundrect
		(at 3.475 1.75 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "28" smd roundrect
		(at 3.475 1.25 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "29" smd roundrect
		(at 3.475 0.75 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "30" smd roundrect
		(at 3.475 0.25 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "31" smd roundrect
		(at 3.475 -0.25 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "32" smd roundrect
		(at 3.475 -0.75 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "33" smd roundrect
		(at 3.475 -1.25 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "34" smd roundrect
		(at 3.475 -1.75 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "35" smd roundrect
		(at 3.475 -2.25 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "36" smd roundrect
		(at 3.475 -2.75 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "37" smd roundrect
		(at 2.75 -3.475 180)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "38" smd roundrect
		(at 2.25 -3.475 180)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "39" smd roundrect
		(at 1.75 -3.475 180)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "40" smd roundrect
		(at 1.25 -3.475 180)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "41" smd roundrect
		(at 0.75 -3.475 180)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "42" smd roundrect
		(at 0.25 -3.475 180)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "43" smd roundrect
		(at -0.25 -3.475 180)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "44" smd roundrect
		(at -0.75 -3.475 180)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "45" smd roundrect
		(at -1.25 -3.475 180)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "46" smd roundrect
		(at -1.75 -3.475 180)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "47" smd roundrect
		(at -2.25 -3.475 180)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "48" smd roundrect
		(at -2.75 -3.475 180)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1785714286)
	)
	(pad "49" smd roundrect
		(at 0 0)
		(size 4.1 4.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.01219512195)
		(solder_paste_margin_ratio -0.1)
	)
	(embedded_fonts no)
	(model "antmicro_sn75dp159rgzr.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
