(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SN75DP159_VQFN"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 43.18 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SN75DP159_VQFN"
				(at 43.18 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SN75DP159_VQFN"
				(at 43.18 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn75dp159.pdf?HQS=dis-mous-null-mousermode-dsf-pf-null-wwe&ts=1703065719267&ref_url=https%253A%252F%252Feu.mouser.com%252F"
				(at 43.18 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Interface - Signal Buffers, Repeaters 6-Gbps DP++ 1.1 to HDMI 2.0 retimer -40 to 85C operating temperature 48-VQFN 0 to 85"
				(at 43.18 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SN75DP159RGZR"
				(at 43.18 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 43.18 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 43.18 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 43.18 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, SMT, BUFFER, HDMI"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SN75DP159_VQFN_1_1"
				(pin passive line
					(at 29.21 -36.83 180)
					(length 2.54)
					(name "SWAP/POL")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 2.54)
					(name "IN_D2p")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 2.54)
					(name "IN_D2n")
					(number "3")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 2.54)
					(name "HPD_SRC")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 2.54)
					(name "IN_D1p")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 2.54)
					(name "IN_D1n")
					(number "6")
				)
				(pin passive line
					(at 29.21 -58.42 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 2.54)
					(name "IN_D0p")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 2.54)
					(name "IN_D0n")
					(number "9")
				)
				(pin passive line
					(at 29.21 -39.37 180)
					(length 2.54)
					(name "I2C_EN/PIN")
					(number "10")
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 2.54)
					(name "IN_CLKp")
					(number "11")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 2.54)
					(name "IN_CLKn")
					(number "12")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VCC_3P3")
					(number "13")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD_1P1")
					(number "14")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 2.54)
					(name "SCL_CTL")
					(number "15")
				)
				(pin passive line
					(at 0 -39.37 0)
					(length 2.54)
					(name "SDA_CTL")
					(number "16")
				)
				(pin no_connect line
					(at 26.67 -2.54 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "17")
				)
				(pin passive line
					(at 29.21 0 180)
					(length 2.54)
					(name "CEC_EN")
					(number "18")
				)
				(pin passive line
					(at 29.21 -58.42 180)
					(length 2.54)
					(name "GND")
					(number "19")
				)
				(pin passive line
					(at 29.21 -41.91 180)
					(length 2.54)
					(name "PRE_SEL")
					(number "20")
				)
				(pin passive line
					(at 29.21 -44.45 180)
					(length 2.54)
					(name "EQ_SEL/A0")
					(number "21")
				)
				(pin passive line
					(at 0 -46.99 0)
					(length 2.54)
					(name "VSADJ")
					(number "22")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD_1P1")
					(number "23")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD_1P1")
					(number "24")
				)
				(pin output line
					(at 29.21 -8.89 180)
					(length 2.54)
					(name "OUT_CLKn")
					(number "25")
				)
				(pin output line
					(at 29.21 -6.35 180)
					(length 2.54)
					(name "OUT_CLKp")
					(number "26")
				)
				(pin passive line
					(at 29.21 -46.99 180)
					(length 2.54)
					(name "~{HDMI_SEL/A1}")
					(number "27")
				)
				(pin output line
					(at 29.21 -13.97 180)
					(length 2.54)
					(name "OUT_D0n")
					(number "28")
				)
				(pin output line
					(at 29.21 -11.43 180)
					(length 2.54)
					(name "OUT_D0p")
					(number "29")
				)
				(pin passive line
					(at 29.21 -58.42 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "30")
				)
				(pin output line
					(at 29.21 -19.05 180)
					(length 2.54)
					(name "OUT_D1n")
					(number "31")
				)
				(pin output line
					(at 29.21 -16.51 180)
					(length 2.54)
					(name "OUT_D1p")
					(number "32")
				)
				(pin passive line
					(at 29.21 -27.94 180)
					(length 2.54)
					(name "HPD_SNK")
					(number "33")
				)
				(pin output line
					(at 29.21 -24.13 180)
					(length 2.54)
					(name "OUT_D2n")
					(number "34")
				)
				(pin output line
					(at 29.21 -21.59 180)
					(length 2.54)
					(name "OUT_D2p")
					(number "35")
				)
				(pin passive line
					(at 29.21 -49.53 180)
					(length 2.54)
					(name "TX_TERM_CTL")
					(number "36")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD_1P1")
					(number "37")
				)
				(pin passive line
					(at 29.21 -30.48 180)
					(length 2.54)
					(name "SCL_SNK")
					(number "38")
				)
				(pin passive line
					(at 29.21 -33.02 180)
					(length 2.54)
					(name "SDA_SNK")
					(number "39")
				)
				(pin passive line
					(at 29.21 -52.07 180)
					(length 2.54)
					(name "SLEW_CTL")
					(number "40")
				)
				(pin passive line
					(at 29.21 -58.42 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "41")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(name "OE")
					(number "42")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VCC_3P3")
					(number "43")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 2.54)
					(name "AUX_SRCn")
					(number "44")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(name "AUX_SRCp")
					(number "45")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 2.54)
					(name "SCL_SRC")
					(number "46")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 2.54)
					(name "SDA_SRC")
					(number "47")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD_1P1")
					(number "48")
				)
				(pin passive line
					(at 29.21 -55.88 180)
					(length 2.54)
					(name "EPAD")
					(number "49")
				)
			)
			(embedded_fonts no)
		)
)
