(footprint "MK_SPH0645LM4H-B"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Footprint based on: https://eu.mouser.com/datasheet/2/218/ph0645lm4h_b_datasheet_rev_c-1525723.pdf")
	(property "Reference" "REF**"
		(at 0.27 -3.15 0)
		(layer "F.SilkS")
	)
	(property "Value" "MK_SPH0645LM4H-B"
		(at 3.490845 1.742302 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 3.490845 3.17 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at 4.12 4.38 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at 5.14 5.53 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 0 0)
		(size 0.77 0.77)
		(drill 0.77)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd rect
		(at -0.9 -2.074)
		(size 0.6 0.522)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -0.9 -1.252)
		(size 0.6 0.522)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd custom
		(at 0.662 0)
		(size 0.1 0.1)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_circle
				(center -0.662 0)
				(end 0 0)
				(width 0.3)
				(fill no)
			)
		)
	)
	(pad "4" smd rect
		(at 0.9 -1.252)
		(size 0.6 0.522)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 0.9 -2.074)
		(size 0.6 0.522)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 0 -2.074)
		(size 0.6 0.522)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_sph0645lm4h_b.glb"
		(offset
			(xyz 0 0.7 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 -180)
		)
	)
)
