(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MK_SPH0645LM4H-B"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "MK"
				(at 15.24 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MK_SPH0645LM4H-B"
				(at 15.24 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MK_SPH0645LM4H-B"
				(at 15.24 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/218/ph0645lm4h_b_datasheet_rev_c-1525723.pdf"
				(at 15.24 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "MEMS Microphones, BP, I2S output, 1.62V - 3.6V"
				(at 15.24 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Knowles"
				(at 15.24 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SPH0645LM4H-B"
				(at 15.24 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 15.24 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 15.24 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MEMS, SENSOR, AUDIO, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MK_SPH0645LM4H-B_1_1"
				(pin input line
					(at 0 -5.08 180)
					(length 2.54)
					(name "WS")
					(number "1")
				)
				(pin input line
					(at 0 -15.24 180)
					(length 2.54)
					(name "SELECT")
					(number "2")
				)
				(pin power_in line
					(at 0 -17.78 180)
					(length 2.54)
					(name "GND")
					(number "3")
				)
				(pin input clock
					(at 0 -7.62 180)
					(length 2.54)
					(name "BCLK")
					(number "4")
				)
				(pin power_in line
					(at 0 0 180)
					(length 2.54)
					(name "VDD")
					(number "5")
				)
				(pin output line
					(at 0 -10.16 180)
					(length 2.54)
					(name "DATA")
					(number "6")
				)
			)
			(embedded_fonts no)
		)
)
