(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TMCS1100A2-Q1"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 33.02 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TMCS1100A2-Q1"
				(at 33.02 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TMCS1100A2-Q1"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmcs1100-q1.pdf?ts=1647195769204&ref_url=https%253A%252F%252Fwww.mouser.de%252F"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Hall current Sensor/transducer"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TMCS1100A2QDRQ1"
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 33.02 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, SENSOR, IC, POWER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TMCS1100A2-Q1_0_1")
			(symbol "TMCS1100A2-Q1_1_1"
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "IN+")
					(number "1")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "IN+")
					(number "2")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "IN-")
					(number "3")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(hide yes)
					(name "IN-")
					(number "4")
				)
				(pin power_in line
					(at 17.78 -5.08 180)
					(length 2.54)
					(name "GND")
					(number "5")
				)
				(pin input line
					(at 17.78 -2.54 180)
					(length 2.54)
					(name "VREF")
					(number "6")
				)
				(pin output line
					(at 17.78 0 180)
					(length 2.54)
					(name "VOUT")
					(number "7")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
