(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TMP451AIDQFR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 27.94 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TMP451AIDQFR"
				(at 27.94 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TMP451AIDQFR"
				(at 27.94 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmp451.pdf?ts=1727409102766"
				(at 27.94 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Board Mount Temperature Sensors AC +/-1degC Remote & Local Temp sensor"
				(at 27.94 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TMP451AIDQFR"
				(at 27.94 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 27.94 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 27.94 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 27.94 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "DIGITAL, SENSOR, I2C, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TMP451AIDQFR_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V+")
					(number "1")
				)
				(pin input line
					(at 17.78 -2.54 180)
					(length 2.54)
					(name "D+")
					(number "2")
				)
				(pin input line
					(at 17.78 -5.08 180)
					(length 2.54)
					(name "D-")
					(number "3")
				)
				(pin output line
					(at 0 -12.7 0)
					(length 2.54)
					(name "~{THERM}")
					(number "4")
				)
				(pin power_in line
					(at 17.78 -12.7 180)
					(length 2.54)
					(name "GND")
					(number "5")
				)
				(pin output line
					(at 0 -10.16 0)
					(length 2.54)
					(name "~{ALERT}")
					(number "6")
					(alternate "~{THERM2}" output line)
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "SDA")
					(number "7")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "SCL")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
