(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TMP461AIRUNR-S"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 53.34 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TMP461AIRUNR-S"
				(at 53.34 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TMP461AIRUNR-S"
				(at 53.34 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmp461.pdf"
				(at 53.34 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "TMP461 High-Accuracy Remote and Local Temperature Sensor with Pin-Programmable Bus Address"
				(at 53.34 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TMP461AIRUNR-S"
				(at 53.34 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 53.34 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 53.34 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 53.34 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, DIGITAL, SENSOR, I2C"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TMP461AIRUNR-S_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V+")
					(number "1")
				)
				(pin input line
					(at 19.05 -3.81 180)
					(length 2.54)
					(name "D+")
					(number "2")
				)
				(pin input line
					(at 19.05 -6.35 180)
					(length 2.54)
					(name "D-")
					(number "3")
				)
				(pin output line
					(at 0 -12.7 0)
					(length 2.54)
					(name "~{THERM}")
					(number "4")
				)
				(pin input line
					(at 0 -19.05 0)
					(length 2.54)
					(name "A0")
					(number "5")
				)
				(pin power_in line
					(at 19.05 -19.05 180)
					(length 2.54)
					(name "GND")
					(number "6")
				)
				(pin output line
					(at 0 -10.16 0)
					(length 2.54)
					(name "~{ALERT}")
					(number "7")
					(alternate "~{THERM2}" output line)
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 2.54)
					(name "SDA")
					(number "8")
				)
				(pin input line
					(at 0 -3.81 0)
					(length 2.54)
					(name "SCL")
					(number "9")
				)
				(pin input line
					(at 0 -16.51 0)
					(length 2.54)
					(name "A1")
					(number "10")
				)
			)
			(embedded_fonts no)
		)
)
