(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "UT8SD4MQ2G72RMLH"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "UT8SD4MQ2G72RMLH"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "UT8SD4MQ2G72RMLH"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.frontgrade.com/sites/default/files/documents/adv_datasheet-ut8sd4mq2g72_0-0-2.pdf"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "DDR4 DRAM 18GB (16GB + 2GB ECC), Radiation Harness Assurance 100krad(Si), Temperature Range: -55°C to 125°C"
				(at 45.72 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "UT8SD4MQ2G72RMLH"
				(at 45.72 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Frontgrade"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "SMT, DRAM, IC"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "266BGA_FTG"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "UT8SD4MQ2G72RMLH_1_1"
				(pin no_connect line
					(at 3.81 -53.34 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "C2")
				)
				(pin no_connect line
					(at 3.81 -53.34 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "C4")
				)
				(pin no_connect line
					(at 3.81 -53.34 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "D2")
				)
				(pin no_connect line
					(at 3.81 -53.34 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "D4")
				)
				(pin no_connect line
					(at 3.81 -53.34 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "E4")
				)
				(pin no_connect line
					(at 3.81 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "H2")
					(alternate "A17" passive line)
				)
				(pin input line
					(at 0 -10.16 0)
					(length 3.81)
					(name "CS0_N")
					(number "J11")
				)
				(pin bidirectional line
					(at 31.75 -48.26 180)
					(length 3.81)
					(name "A13")
					(number "K1")
				)
				(pin bidirectional line
					(at 31.75 -38.1 180)
					(length 3.81)
					(name "A9")
					(number "K2")
				)
				(pin input line
					(at 31.75 -2.54 180)
					(length 3.81)
					(name "ALERT_N")
					(number "K3")
				)
				(pin bidirectional line
					(at 31.75 -30.48 180)
					(length 3.81)
					(name "A6")
					(number "K4")
				)
				(pin input line
					(at 31.75 -10.16 180)
					(length 3.81)
					(name "TEN")
					(number "K5")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 3.81)
					(name "BA1")
					(number "K6")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "BG0")
					(number "K7")
				)
				(pin bidirectional line
					(at 31.75 -45.72 180)
					(length 3.81)
					(name "A12")
					(number "K8")
					(alternate "BC_N" passive line)
				)
				(pin input line
					(at 31.75 0 180)
					(length 3.81)
					(name "ACT_N")
					(number "K9")
				)
				(pin bidirectional line
					(at 31.75 -50.8 180)
					(length 3.81)
					(name "A14")
					(number "K10")
					(alternate "WE_N" passive line)
				)
				(pin bidirectional line
					(at 31.75 -43.18 180)
					(length 3.81)
					(name "A11")
					(number "L1")
				)
				(pin bidirectional line
					(at 31.75 -33.02 180)
					(length 3.81)
					(name "A7")
					(number "L3")
				)
				(pin bidirectional line
					(at 31.75 -17.78 180)
					(length 3.81)
					(name "A1")
					(number "L4")
				)
				(pin bidirectional line
					(at 31.75 -25.4 180)
					(length 3.81)
					(name "A4")
					(number "L6")
				)
				(pin bidirectional line
					(at 31.75 -55.88 180)
					(length 3.81)
					(name "A16")
					(number "L9")
					(alternate "RAS_N" passive line)
				)
				(pin input line
					(at 31.75 -5.08 180)
					(length 3.81)
					(name "ODT0")
					(number "L10")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 3.81)
					(name "CK_C")
					(number "L11")
				)
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(name "CK_T")
					(number "L12")
				)
				(pin input line
					(at 31.75 -7.62 180)
					(length 3.81)
					(name "PARITY")
					(number "M1")
				)
				(pin bidirectional line
					(at 31.75 -20.32 180)
					(length 3.81)
					(name "A2")
					(number "M2")
				)
				(pin bidirectional line
					(at 31.75 -35.56 180)
					(length 3.81)
					(name "A8")
					(number "M3")
				)
				(pin bidirectional line
					(at 31.75 -15.24 180)
					(length 3.81)
					(name "A0")
					(number "M4")
				)
				(pin bidirectional line
					(at 31.75 -27.94 180)
					(length 3.81)
					(name "A5")
					(number "M5")
				)
				(pin bidirectional line
					(at 31.75 -22.86 180)
					(length 3.81)
					(name "A3")
					(number "M6")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 3.81)
					(name "BA0")
					(number "M7")
				)
				(pin bidirectional line
					(at 31.75 -40.64 180)
					(length 3.81)
					(name "A10")
					(number "M8")
					(alternate "AP" passive line)
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "BG1")
					(number "M9")
				)
				(pin bidirectional line
					(at 31.75 -53.34 180)
					(length 3.81)
					(name "A15")
					(number "M10")
					(alternate "CAS_N" passive line)
				)
				(pin input line
					(at 0 -7.62 0)
					(length 3.81)
					(name "CKE0")
					(number "N11")
				)
				(pin no_connect line
					(at 3.81 -53.34 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "R2")
				)
				(pin no_connect line
					(at 3.81 -53.34 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "T2")
				)
				(pin no_connect line
					(at 3.81 -53.34 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "T4")
				)
				(pin no_connect line
					(at 3.81 -53.34 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "U2")
				)
				(pin no_connect line
					(at 3.81 -53.34 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "U4")
				)
			)
			(symbol "UT8SD4MQ2G72RMLH_2_1"
				(pin power_in line
					(at 19.05 0 180)
					(length 3.81)
					(name "VPP")
					(number "A1")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A2")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VDD")
					(number "A3")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "A4")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A5")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A7")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A9")
				)
				(pin power_in line
					(at 19.05 -8.89 180)
					(length 3.81)
					(name "GND")
					(number "A11")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A14")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B1")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "B2")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B3")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B5")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B7")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B11")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "B13")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "C3")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "C5")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "D3")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "D5")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "D9")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "D11")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "D12")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "D13")
				)
				(pin passive line
					(at 19.05 0 180)
					(length 3.81)
					(hide yes)
					(name "VPP")
					(number "D14")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E3")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E5")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E8")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "E11")
				)
				(pin power_in line
					(at 0 -8.89 0)
					(length 3.81)
					(name "VTT")
					(number "F1")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "F2")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F3")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "F5")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F11")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "F13")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "G1")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G3")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G5")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G9")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G14")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "H1")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "H3")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "H5")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "H6")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "H7")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "H9")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "J1")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "J2")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "J3")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "J4")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "J5")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "J7")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "J9")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "J12")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "K11")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "K12")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "K13")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 3.81)
					(hide yes)
					(name "VTT")
					(number "K14")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "L2")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "L5")
				)
				(pin power_in line
					(at 0 -3.81 0)
					(length 3.81)
					(name "VREFCA")
					(number "L7")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "L8")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "L13")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 3.81)
					(hide yes)
					(name "VTT")
					(number "L14")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "M11")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "M12")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "M13")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 3.81)
					(hide yes)
					(name "VTT")
					(number "M14")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "N1")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "N2")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "N4")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "N5")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "N7")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "N9")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "N14")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 3.81)
					(hide yes)
					(name "VTT")
					(number "P1")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "P3")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "P5")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "P9")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "P11")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "P13")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "R3")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "R5")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "R11")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "R13")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "T3")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "T5")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "T8")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "T11")
				)
				(pin passive line
					(at 19.05 0 180)
					(length 3.81)
					(hide yes)
					(name "VPP")
					(number "T14")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "U3")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "U5")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "U13")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "V1")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "V2")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "V3")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "V5")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "V11")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "V13")
				)
				(pin passive line
					(at 19.05 0 180)
					(length 3.81)
					(hide yes)
					(name "VPP")
					(number "W1")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "W2")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "W3")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "W5")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "W6")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "W7")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "W9")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "W11")
				)
				(pin passive line
					(at 19.05 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "W14")
				)
			)
			(symbol "UT8SD4MQ2G72RMLH_3_1"
				(pin bidirectional line
					(at 31.75 -83.82 180)
					(length 3.81)
					(name "DQ30")
					(number "A6")
				)
				(pin bidirectional line
					(at 31.75 -71.12 180)
					(length 3.81)
					(name "DQ25")
					(number "A8")
				)
				(pin bidirectional line
					(at 31.75 -60.96 180)
					(length 3.81)
					(name "DQ22")
					(number "A10")
				)
				(pin bidirectional line
					(at 31.75 -53.34 180)
					(length 3.81)
					(name "DQ19")
					(number "A12")
				)
				(pin bidirectional line
					(at 31.75 -48.26 180)
					(length 3.81)
					(name "DQ17")
					(number "A13")
				)
				(pin bidirectional line
					(at 31.75 -78.74 180)
					(length 3.81)
					(name "DQ28")
					(number "B4")
				)
				(pin bidirectional line
					(at 31.75 -81.28 180)
					(length 3.81)
					(name "DQ29")
					(number "B6")
				)
				(pin bidirectional line
					(at 31.75 -76.2 180)
					(length 3.81)
					(name "DQ27")
					(number "B8")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 3.81)
					(name "DQS3_T")
					(number "B9")
				)
				(pin bidirectional line
					(at 31.75 -55.88 180)
					(length 3.81)
					(name "DQ20")
					(number "B10")
				)
				(pin bidirectional line
					(at 31.75 -45.72 180)
					(length 3.81)
					(name "DQ16")
					(number "B12")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 3.81)
					(name "DQS2_C")
					(number "B14")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "RESET0_N")
					(number "C1")
				)
				(pin bidirectional line
					(at 31.75 -86.36 180)
					(length 3.81)
					(name "DQ31")
					(number "C6")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 3.81)
					(name "ZQ2")
					(number "C7")
				)
				(pin bidirectional line
					(at 31.75 -73.66 180)
					(length 3.81)
					(name "DQ26")
					(number "C8")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 3.81)
					(name "DQS3_C")
					(number "C9")
				)
				(pin bidirectional line
					(at 31.75 -63.5 180)
					(length 3.81)
					(name "DQ23")
					(number "C10")
				)
				(pin bidirectional line
					(at 31.75 -58.42 180)
					(length 3.81)
					(name "DQ21")
					(number "C11")
				)
				(pin bidirectional line
					(at 31.75 -50.8 180)
					(length 3.81)
					(name "DQ18")
					(number "C12")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 3.81)
					(name "DM2_N")
					(number "C13")
					(alternate "DBI2" passive line)
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 3.81)
					(name "DQS2_T")
					(number "C14")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "RESET1_N")
					(number "D1")
				)
				(pin bidirectional line
					(at 31.75 -68.58 180)
					(length 3.81)
					(name "DQ24")
					(number "D6")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 3.81)
					(name "ZQ3")
					(number "D7")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 3.81)
					(name "DM3_N")
					(number "D8")
					(alternate "DBI3" passive line)
				)
				(pin bidirectional line
					(at 31.75 -40.64 180)
					(length 3.81)
					(name "DQ15")
					(number "D10")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 3.81)
					(name "RESET2_N")
					(number "E1")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 3.81)
					(name "RESET3_N")
					(number "E2")
				)
				(pin bidirectional line
					(at 31.75 -7.62 180)
					(length 3.81)
					(name "DQ3")
					(number "E6")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 3.81)
					(name "ZQ1")
					(number "E7")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "DQS0_C")
					(number "E9")
				)
				(pin bidirectional line
					(at 31.75 -33.02 180)
					(length 3.81)
					(name "DQ12")
					(number "E10")
				)
				(pin bidirectional line
					(at 31.75 -27.94 180)
					(length 3.81)
					(name "DQ10")
					(number "E12")
				)
				(pin bidirectional line
					(at 31.75 -25.4 180)
					(length 3.81)
					(name "DQ9")
					(number "E13")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "DQS1_T")
					(number "E14")
				)
				(pin bidirectional line
					(at 31.75 -17.78 180)
					(length 3.81)
					(name "DQ7")
					(number "F4")
				)
				(pin bidirectional line
					(at 31.75 -5.08 180)
					(length 3.81)
					(name "DQ2")
					(number "F6")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "ZQ0")
					(number "F7")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 3.81)
					(name "DM0_N")
					(number "F8")
					(alternate "DBI0" passive line)
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "DQS0_T")
					(number "F9")
				)
				(pin bidirectional line
					(at 31.75 -35.56 180)
					(length 3.81)
					(name "DQ13")
					(number "F10")
				)
				(pin bidirectional line
					(at 31.75 -22.86 180)
					(length 3.81)
					(name "DQ8")
					(number "F12")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 3.81)
					(name "DQS1_C")
					(number "F14")
				)
				(pin bidirectional line
					(at 0 -186.69 0)
					(length 3.81)
					(name "RESET8_N")
					(number "G2")
				)
				(pin bidirectional line
					(at 31.75 -10.16 180)
					(length 3.81)
					(name "DQ4")
					(number "G4")
				)
				(pin bidirectional line
					(at 31.75 -12.7 180)
					(length 3.81)
					(name "DQ5")
					(number "G6")
				)
				(pin bidirectional line
					(at 0 -199.39 0)
					(length 3.81)
					(name "ZQ8")
					(number "G7")
				)
				(pin bidirectional line
					(at 31.75 -2.54 180)
					(length 3.81)
					(name "DQ1")
					(number "G8")
				)
				(pin bidirectional line
					(at 31.75 -38.1 180)
					(length 3.81)
					(name "DQ14")
					(number "G10")
				)
				(pin bidirectional line
					(at 31.75 -196.85 180)
					(length 3.81)
					(name "CB5")
					(number "G11")
				)
				(pin bidirectional line
					(at 31.75 -30.48 180)
					(length 3.81)
					(name "DQ11")
					(number "G12")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "DM1_N")
					(number "G13")
					(alternate "DBI1" passive line)
				)
				(pin bidirectional line
					(at 31.75 -15.24 180)
					(length 3.81)
					(name "DQ6")
					(number "H4")
				)
				(pin bidirectional line
					(at 31.75 0 180)
					(length 3.81)
					(name "DQ0")
					(number "H8")
				)
				(pin bidirectional line
					(at 31.75 -201.93 180)
					(length 3.81)
					(name "CB7")
					(number "H10")
				)
				(pin bidirectional line
					(at 31.75 -189.23 180)
					(length 3.81)
					(name "CB2")
					(number "H11")
				)
				(pin bidirectional line
					(at 0 -184.15 0)
					(length 3.81)
					(name "DM8_N")
					(number "H12")
					(alternate "DBI8" passive line)
				)
				(pin bidirectional line
					(at 31.75 -186.69 180)
					(length 3.81)
					(name "CB1")
					(number "H13")
				)
				(pin bidirectional line
					(at 0 -191.77 0)
					(length 3.81)
					(name "DQS8_T")
					(number "H14")
				)
				(pin bidirectional line
					(at 31.75 -199.39 180)
					(length 3.81)
					(name "CB6")
					(number "J6")
				)
				(pin bidirectional line
					(at 31.75 -191.77 180)
					(length 3.81)
					(name "CB3")
					(number "J8")
				)
				(pin bidirectional line
					(at 31.75 -194.31 180)
					(length 3.81)
					(name "CB4")
					(number "J10")
				)
				(pin bidirectional line
					(at 31.75 -184.15 180)
					(length 3.81)
					(name "CB0")
					(number "J13")
				)
				(pin bidirectional line
					(at 0 -194.31 0)
					(length 3.81)
					(name "DQS8_C")
					(number "J14")
				)
				(pin bidirectional line
					(at 31.75 -176.53 180)
					(length 3.81)
					(name "DQ62")
					(number "N3")
				)
				(pin bidirectional line
					(at 31.75 -173.99 180)
					(length 3.81)
					(name "DQ61")
					(number "N6")
				)
				(pin bidirectional line
					(at 31.75 -163.83 180)
					(length 3.81)
					(name "DQ57")
					(number "N8")
				)
				(pin bidirectional line
					(at 31.75 -153.67 180)
					(length 3.81)
					(name "DQ54")
					(number "N10")
				)
				(pin bidirectional line
					(at 31.75 -146.05 180)
					(length 3.81)
					(name "DQ51")
					(number "N12")
				)
				(pin bidirectional line
					(at 0 -138.43 0)
					(length 3.81)
					(name "DM6_N")
					(number "N13")
					(alternate "DBI6" passive line)
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 3.81)
					(name "RESET4_N")
					(number "P2")
				)
				(pin bidirectional line
					(at 31.75 -171.45 180)
					(length 3.81)
					(name "DQ60")
					(number "P4")
				)
				(pin bidirectional line
					(at 31.75 -166.37 180)
					(length 3.81)
					(name "DQ58")
					(number "P6")
				)
				(pin bidirectional line
					(at 31.75 -168.91 180)
					(length 3.81)
					(name "DQ59")
					(number "P7")
				)
				(pin bidirectional line
					(at 31.75 -148.59 180)
					(length 3.81)
					(name "DQ52")
					(number "P8")
				)
				(pin bidirectional line
					(at 31.75 -156.21 180)
					(length 3.81)
					(name "DQ55")
					(number "P10")
				)
				(pin bidirectional line
					(at 31.75 -138.43 180)
					(length 3.81)
					(name "DQ48")
					(number "P12")
				)
				(pin bidirectional line
					(at 0 -148.59 0)
					(length 3.81)
					(name "DQS6_C")
					(number "P14")
				)
				(pin bidirectional line
					(at 0 -118.11 0)
					(length 3.81)
					(name "RESET5_N")
					(number "R1")
				)
				(pin bidirectional line
					(at 31.75 -179.07 180)
					(length 3.81)
					(name "DQ63")
					(number "R4")
				)
				(pin bidirectional line
					(at 31.75 -161.29 180)
					(length 3.81)
					(name "DQ56")
					(number "R6")
				)
				(pin bidirectional line
					(at 0 -153.67 0)
					(length 3.81)
					(name "ZQ6")
					(number "R7")
				)
				(pin bidirectional line
					(at 31.75 -96.52 180)
					(length 3.81)
					(name "DQ34")
					(number "R8")
				)
				(pin bidirectional line
					(at 31.75 -151.13 180)
					(length 3.81)
					(name "DQ53")
					(number "R9")
				)
				(pin bidirectional line
					(at 0 -168.91 0)
					(length 3.81)
					(name "DQS7_T")
					(number "R10")
				)
				(pin bidirectional line
					(at 31.75 -143.51 180)
					(length 3.81)
					(name "DQ50")
					(number "R12")
				)
				(pin bidirectional line
					(at 0 -146.05 0)
					(length 3.81)
					(name "DQS6_T")
					(number "R14")
				)
				(pin bidirectional line
					(at 0 -140.97 0)
					(length 3.81)
					(name "RESET6_N")
					(number "T1")
				)
				(pin bidirectional line
					(at 31.75 -109.22 180)
					(length 3.81)
					(name "DQ39")
					(number "T6")
				)
				(pin bidirectional line
					(at 0 -176.53 0)
					(length 3.81)
					(name "ZQ7")
					(number "T7")
				)
				(pin bidirectional line
					(at 0 -161.29 0)
					(length 3.81)
					(name "DM7_N")
					(number "T9")
					(alternate "DBI7" passive line)
				)
				(pin bidirectional line
					(at 0 -171.45 0)
					(length 3.81)
					(name "DQS7_C")
					(number "T10")
				)
				(pin bidirectional line
					(at 31.75 -140.97 180)
					(length 3.81)
					(name "DQ49")
					(number "T12")
				)
				(pin bidirectional line
					(at 0 -115.57 0)
					(length 3.81)
					(name "DM5_N")
					(number "T13")
					(alternate "DBI5" passive line)
				)
				(pin bidirectional line
					(at 0 -163.83 0)
					(length 3.81)
					(name "RESET7_N")
					(number "U1")
				)
				(pin bidirectional line
					(at 31.75 -91.44 180)
					(length 3.81)
					(name "DQ32")
					(number "U6")
				)
				(pin bidirectional line
					(at 0 -130.81 0)
					(length 3.81)
					(name "ZQ5")
					(number "U7")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 3.81)
					(name "DM4_N")
					(number "U8")
					(alternate "DBI4" passive line)
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 3.81)
					(name "DQS4_C")
					(number "U9")
				)
				(pin bidirectional line
					(at 31.75 -133.35 180)
					(length 3.81)
					(name "DQ47")
					(number "U10")
				)
				(pin bidirectional line
					(at 31.75 -128.27 180)
					(length 3.81)
					(name "DQ45")
					(number "U11")
				)
				(pin bidirectional line
					(at 31.75 -120.65 180)
					(length 3.81)
					(name "DQ42")
					(number "U12")
				)
				(pin bidirectional line
					(at 0 -123.19 0)
					(length 3.81)
					(name "DQS5_T")
					(number "U14")
				)
				(pin bidirectional line
					(at 31.75 -106.68 180)
					(length 3.81)
					(name "DQ38")
					(number "V4")
				)
				(pin bidirectional line
					(at 31.75 -104.14 180)
					(length 3.81)
					(name "DQ37")
					(number "V6")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 3.81)
					(name "ZQ4")
					(number "V7")
				)
				(pin bidirectional line
					(at 31.75 -93.98 180)
					(length 3.81)
					(name "DQ33")
					(number "V8")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 3.81)
					(name "DQS4_T")
					(number "V9")
				)
				(pin bidirectional line
					(at 31.75 -130.81 180)
					(length 3.81)
					(name "DQ46")
					(number "V10")
				)
				(pin bidirectional line
					(at 31.75 -115.57 180)
					(length 3.81)
					(name "DQ40")
					(number "V12")
				)
				(pin bidirectional line
					(at 0 -125.73 0)
					(length 3.81)
					(name "DQS5_C")
					(number "V14")
				)
				(pin bidirectional line
					(at 31.75 -101.6 180)
					(length 3.81)
					(name "DQ36")
					(number "W4")
				)
				(pin bidirectional line
					(at 31.75 -99.06 180)
					(length 3.81)
					(name "DQ35")
					(number "W8")
				)
				(pin bidirectional line
					(at 31.75 -125.73 180)
					(length 3.81)
					(name "DQ44")
					(number "W10")
				)
				(pin bidirectional line
					(at 31.75 -123.19 180)
					(length 3.81)
					(name "DQ43")
					(number "W12")
				)
				(pin bidirectional line
					(at 31.75 -118.11 180)
					(length 3.81)
					(name "DQ41")
					(number "W13")
				)
			)
			(embedded_fonts no)
		)
)
