(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Socket_Amphenol_HPCE_2x17_10107844-002LF"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 50.8 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Socket_Amphenol_HPCE_2x17_10107844-002LF"
				(at 50.8 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Socket_Amphenol_HPCE_2x17_10107844-002LF"
				(at 50.8 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.farnell.com/cad/2569863.pdf"
				(at 50.8 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "60 (24 + 36 Power) Position Edge Card Connector"
				(at 50.8 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "10107844-002LF"
				(at 50.8 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Amphenol"
				(at 50.8 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 50.8 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 50.8 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "HORIZONTAL, EDGE, CONNECTOR, SOCKET, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Socket_Amphenol_HPCE_2x17_10107844-002LF_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 7.62)
					(name "P1")
					(number "P1/2")
					(alternate "2" passive line)
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 7.62)
					(name "P3")
					(number "P3/4")
					(alternate "4" passive line)
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 7.62)
					(name "P5")
					(number "P5/6")
					(alternate "6" passive line)
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 7.62)
					(name "P7")
					(number "P7/8")
					(alternate "8" passive line)
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 7.62)
					(name "P9")
					(number "P9/10")
					(alternate "10" passive line)
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 7.62)
					(name "P11")
					(number "P11/12")
					(alternate "12" passive line)
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 7.62)
					(name "P13")
					(number "P13/14")
					(alternate "14" passive line)
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 7.62)
					(name "P15")
					(number "P15/16")
					(alternate "16" passive line)
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 7.62)
					(name "P17")
					(number "P17/18")
					(alternate "18" passive line)
				)
				(pin power_in line
					(at 35.56 -20.32 180)
					(length 7.62)
					(name "P19")
					(number "P19/20")
					(alternate "20" passive line)
				)
				(pin power_in line
					(at 35.56 -17.78 180)
					(length 7.62)
					(name "P21")
					(number "P21/22")
					(alternate "22" passive line)
				)
				(pin power_in line
					(at 35.56 -15.24 180)
					(length 7.62)
					(name "P23")
					(number "P23/24")
					(alternate "24" passive line)
				)
				(pin power_in line
					(at 35.56 -12.7 180)
					(length 7.62)
					(name "P25")
					(number "P25/26")
					(alternate "26" passive line)
				)
				(pin power_in line
					(at 35.56 -10.16 180)
					(length 7.62)
					(name "P27")
					(number "P27/28")
					(alternate "28" passive line)
				)
				(pin power_in line
					(at 35.56 -7.62 180)
					(length 7.62)
					(name "P29")
					(number "P29/30")
					(alternate "30" passive line)
				)
				(pin power_in line
					(at 35.56 -5.08 180)
					(length 7.62)
					(name "P31")
					(number "P31/32")
					(alternate "32" passive line)
				)
				(pin power_in line
					(at 35.56 -2.54 180)
					(length 7.62)
					(name "P33")
					(number "P33/34")
					(alternate "34" passive line)
				)
				(pin power_in line
					(at 35.56 0 180)
					(length 7.62)
					(name "P35")
					(number "P35/36")
					(alternate "36" passive line)
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 7.62)
					(name "S1")
					(number "S1")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 7.62)
					(name "S2")
					(number "S2")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 7.62)
					(name "S3")
					(number "S3")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 7.62)
					(name "S4")
					(number "S4")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 7.62)
					(name "S5")
					(number "S5")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 7.62)
					(name "S6")
					(number "S6")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 7.62)
					(name "S7")
					(number "S7")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 7.62)
					(name "S8")
					(number "S8")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 7.62)
					(name "S9")
					(number "S9")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 7.62)
					(name "S10")
					(number "S10")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 7.62)
					(name "S11")
					(number "S11")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 7.62)
					(name "S12")
					(number "S12")
				)
				(pin passive line
					(at 35.56 -53.34 180)
					(length 7.62)
					(name "S13")
					(number "S13")
				)
				(pin passive line
					(at 35.56 -50.8 180)
					(length 7.62)
					(name "S14")
					(number "S14")
				)
				(pin passive line
					(at 35.56 -48.26 180)
					(length 7.62)
					(name "S15")
					(number "S15")
				)
				(pin passive line
					(at 35.56 -45.72 180)
					(length 7.62)
					(name "S16")
					(number "S16")
				)
				(pin passive line
					(at 35.56 -43.18 180)
					(length 7.62)
					(name "S17")
					(number "S17")
				)
				(pin passive line
					(at 35.56 -40.64 180)
					(length 7.62)
					(name "S18")
					(number "S18")
				)
				(pin passive line
					(at 35.56 -38.1 180)
					(length 7.62)
					(name "S19")
					(number "S19")
				)
				(pin passive line
					(at 35.56 -35.56 180)
					(length 7.62)
					(name "S20")
					(number "S20")
				)
				(pin passive line
					(at 35.56 -33.02 180)
					(length 7.62)
					(name "S21")
					(number "S21")
				)
				(pin passive line
					(at 35.56 -30.48 180)
					(length 7.62)
					(name "S22")
					(number "S22")
				)
				(pin passive line
					(at 35.56 -27.94 180)
					(length 7.62)
					(name "S23")
					(number "S23")
				)
				(pin passive line
					(at 35.56 -25.4 180)
					(length 7.62)
					(name "S24")
					(number "S24")
				)
			)
			(embedded_fonts no)
		)
)
