(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Socket_Amphenol_HPCE_2x17_10114587-001LF"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 55.88 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Socket_Amphenol_HPCE_2x17_10114587-001LF"
				(at 55.88 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Socket_Amphenol_HPCE_2x17_10114587-001LF"
				(at 55.88 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://cdn.amphenol-cs.com/media/wysiwyg/files/drawing/10114587.pdf"
				(at 55.88 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Vertical, 60 (24 + 36 Power) Position Edge Card Connector"
				(at 55.88 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Amphenol"
				(at 55.88 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "10114587-001LF"
				(at 55.88 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 55.88 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 55.88 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "VERTICAL, EDGE, CONNECTOR, SOCKET, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Socket_Amphenol_HPCE_2x17_10114587-001LF_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 8.89)
					(name "P1")
					(number "P1/P2")
					(alternate "P2" passive line)
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 8.89)
					(name "P3")
					(number "P3/P4")
					(alternate "P4" passive line)
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 8.89)
					(name "P5")
					(number "P5/P6")
					(alternate "P6" passive line)
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 8.89)
					(name "P7")
					(number "P7/P8")
					(alternate "P8" passive line)
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 8.89)
					(name "P9")
					(number "P9/P10")
					(alternate "P10" passive line)
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 8.89)
					(name "P11")
					(number "P11/P12")
					(alternate "P12" passive line)
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 8.89)
					(name "P13")
					(number "P13/P14")
					(alternate "P14" passive line)
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 8.89)
					(name "P15")
					(number "P15/P16")
					(alternate "P16" passive line)
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 8.89)
					(name "P17")
					(number "P17/P18")
					(alternate "P18" passive line)
				)
				(pin power_in line
					(at 43.18 -20.32 180)
					(length 8.89)
					(name "P20")
					(number "P20/P19")
					(alternate "P19" passive line)
				)
				(pin power_in line
					(at 43.18 -17.78 180)
					(length 8.89)
					(name "P22")
					(number "P22/P21")
					(alternate "P21" passive line)
				)
				(pin power_in line
					(at 43.18 -15.24 180)
					(length 8.89)
					(name "P24")
					(number "P24/P23")
					(alternate "P23" passive line)
				)
				(pin power_in line
					(at 43.18 -12.7 180)
					(length 8.89)
					(name "P26")
					(number "P26/P25")
					(alternate "P25" passive line)
				)
				(pin power_in line
					(at 43.18 -10.16 180)
					(length 8.89)
					(name "P28")
					(number "P28/P27")
					(alternate "P27" passive line)
				)
				(pin power_in line
					(at 43.18 -7.62 180)
					(length 8.89)
					(name "P30")
					(number "P30/P29")
					(alternate "P29" passive line)
				)
				(pin power_in line
					(at 43.18 -5.08 180)
					(length 8.89)
					(name "P32")
					(number "P32/P31")
					(alternate "P31" passive line)
				)
				(pin power_in line
					(at 43.18 -2.54 180)
					(length 8.89)
					(name "P34")
					(number "P34/P33")
					(alternate "P33" passive line)
				)
				(pin power_in line
					(at 43.18 0 180)
					(length 8.89)
					(name "P36")
					(number "P36/P35")
					(alternate "P35" passive line)
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 8.89)
					(name "S1")
					(number "S1")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 8.89)
					(name "S2")
					(number "S2")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 8.89)
					(name "S3")
					(number "S3")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 8.89)
					(name "S4")
					(number "S4")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 8.89)
					(name "S5")
					(number "S5")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 8.89)
					(name "S6")
					(number "S6")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 8.89)
					(name "S7")
					(number "S7")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 8.89)
					(name "S8")
					(number "S8")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 8.89)
					(name "S9")
					(number "S9")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 8.89)
					(name "S10")
					(number "S10")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 8.89)
					(name "S11")
					(number "S11")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 8.89)
					(name "S12")
					(number "S12")
				)
				(pin passive line
					(at 43.18 -53.34 180)
					(length 8.89)
					(name "S13")
					(number "S13")
				)
				(pin passive line
					(at 43.18 -50.8 180)
					(length 8.89)
					(name "S14")
					(number "S14")
				)
				(pin passive line
					(at 43.18 -48.26 180)
					(length 8.89)
					(name "S15")
					(number "S15")
				)
				(pin passive line
					(at 43.18 -45.72 180)
					(length 8.89)
					(name "S16")
					(number "S16")
				)
				(pin passive line
					(at 43.18 -43.18 180)
					(length 8.89)
					(name "S17")
					(number "S17")
				)
				(pin passive line
					(at 43.18 -40.64 180)
					(length 8.89)
					(name "S18")
					(number "S18")
				)
				(pin passive line
					(at 43.18 -38.1 180)
					(length 8.89)
					(name "S19")
					(number "S19")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 8.89)
					(name "S20")
					(number "S20")
				)
				(pin passive line
					(at 43.18 -33.02 180)
					(length 8.89)
					(name "S21")
					(number "S21")
				)
				(pin passive line
					(at 43.18 -30.48 180)
					(length 8.89)
					(name "S22")
					(number "S22")
				)
				(pin passive line
					(at 43.18 -27.94 180)
					(length 8.89)
					(name "S23")
					(number "S23")
				)
				(pin passive line
					(at 43.18 -25.4 180)
					(length 8.89)
					(name "S24")
					(number "S24")
				)
			)
			(embedded_fonts no)
		)
)
