(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Bus_DDR5_SODIMM_Amphenol_10161033-002RHLF"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 50.8 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Bus_DDR5_SODIMM_Amphenol_10161033-002RHLF"
				(at 50.8 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Bus_DDR5_SODIMM_Amphenol_10161033-002RHLF"
				(at 50.8 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://cdn.amphenol-cs.com/media/wysiwyg/files/documentation/datasheet/ssio/ssio_ddr5_sodimm.pdf"
				(at 50.8 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "DDR5 SODIMM connector, Right Angle, Surface Mount, 262 Position, 0.5mm Pitch, 5,2mm Height"
				(at 50.8 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "10161033-002RHLF"
				(at 50.8 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Amphenol"
				(at 50.8 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 50.8 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 50.8 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "SMT, CONNECTOR, DDR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Bus_DDR5_SODIMM_Amphenol_10161033-002RHLF_1_1"
				(text "ECC"
					(at 17.78 -69.85 900)
				)
				(pin passive line
					(at 35.56 -6.35 180)
					(length 3.81)
					(name "DQ0_A")
					(number "11")
				)
				(pin passive line
					(at 35.56 -8.89 180)
					(length 3.81)
					(name "DQ1_A")
					(number "12")
				)
				(pin passive line
					(at 35.56 -11.43 180)
					(length 3.81)
					(name "DQ2_A")
					(number "15")
				)
				(pin passive line
					(at 35.56 -13.97 180)
					(length 3.81)
					(name "DQ3_A")
					(number "16")
				)
				(pin passive line
					(at 35.56 -27.94 180)
					(length 3.81)
					(name "DM0_A_n")
					(number "19")
				)
				(pin passive line
					(at 35.56 -2.54 180)
					(length 3.81)
					(name "DQS0_A_C")
					(number "20")
				)
				(pin passive line
					(at 35.56 0 180)
					(length 3.81)
					(name "DQS0_A_t")
					(number "22")
				)
				(pin passive line
					(at 35.56 -16.51 180)
					(length 3.81)
					(name "DQ4_A")
					(number "23")
				)
				(pin passive line
					(at 35.56 -19.05 180)
					(length 3.81)
					(name "DQ5_A")
					(number "26")
				)
				(pin passive line
					(at 35.56 -21.59 180)
					(length 3.81)
					(name "DQ6_A")
					(number "27")
				)
				(pin passive line
					(at 35.56 -24.13 180)
					(length 3.81)
					(name "DQ7_A")
					(number "30")
				)
				(pin passive line
					(at 35.56 -39.37 180)
					(length 3.81)
					(name "DQ8_A")
					(number "31")
				)
				(pin passive line
					(at 35.56 -41.91 180)
					(length 3.81)
					(name "DQ09_A")
					(number "34")
				)
				(pin passive line
					(at 35.56 -44.45 180)
					(length 3.81)
					(name "DQ10_A")
					(number "35")
				)
				(pin passive line
					(at 35.56 -46.99 180)
					(length 3.81)
					(name "DQ11_A")
					(number "38")
				)
				(pin passive line
					(at 35.56 -35.56 180)
					(length 3.81)
					(name "DQS1_A_C")
					(number "39")
				)
				(pin passive line
					(at 35.56 -33.02 180)
					(length 3.81)
					(name "DQS1_A_t")
					(number "41")
				)
				(pin passive line
					(at 35.56 -60.96 180)
					(length 3.81)
					(name "DM1_A_n")
					(number "42")
				)
				(pin passive line
					(at 35.56 -49.53 180)
					(length 3.81)
					(name "DQ12_A")
					(number "45")
				)
				(pin passive line
					(at 35.56 -52.07 180)
					(length 3.81)
					(name "DQ13_A")
					(number "46")
				)
				(pin passive line
					(at 35.56 -54.61 180)
					(length 3.81)
					(name "DQ14_A")
					(number "49")
				)
				(pin passive line
					(at 35.56 -57.15 180)
					(length 3.81)
					(name "DQ15_A")
					(number "50")
				)
				(pin passive line
					(at 35.56 -72.39 180)
					(length 3.81)
					(name "DQ16_A")
					(number "53")
				)
				(pin passive line
					(at 35.56 -74.93 180)
					(length 3.81)
					(name "DQ17_A")
					(number "54")
				)
				(pin passive line
					(at 35.56 -77.47 180)
					(length 3.81)
					(name "DQ18_A")
					(number "57")
				)
				(pin passive line
					(at 35.56 -80.01 180)
					(length 3.81)
					(name "DQ19_A")
					(number "58")
				)
				(pin passive line
					(at 35.56 -93.98 180)
					(length 3.81)
					(name "DM2_A_n")
					(number "61")
				)
				(pin passive line
					(at 35.56 -68.58 180)
					(length 3.81)
					(name "DQS2_A_C")
					(number "62")
				)
				(pin passive line
					(at 35.56 -66.04 180)
					(length 3.81)
					(name "DQS2_A_t")
					(number "64")
				)
				(pin passive line
					(at 35.56 -82.55 180)
					(length 3.81)
					(name "DQ20_A")
					(number "65")
				)
				(pin passive line
					(at 35.56 -85.09 180)
					(length 3.81)
					(name "DQ21_A")
					(number "68")
				)
				(pin passive line
					(at 35.56 -87.63 180)
					(length 3.81)
					(name "DQ22_A")
					(number "69")
				)
				(pin passive line
					(at 35.56 -90.17 180)
					(length 3.81)
					(name "DQ23_A")
					(number "72")
				)
				(pin passive line
					(at 35.56 -105.41 180)
					(length 3.81)
					(name "DQ24_A")
					(number "73")
				)
				(pin passive line
					(at 35.56 -107.95 180)
					(length 3.81)
					(name "DQ25_A")
					(number "76")
				)
				(pin passive line
					(at 35.56 -110.49 180)
					(length 3.81)
					(name "DQ26_A")
					(number "77")
				)
				(pin passive line
					(at 35.56 -113.03 180)
					(length 3.81)
					(name "DQ27_A")
					(number "80")
				)
				(pin passive line
					(at 35.56 -101.6 180)
					(length 3.81)
					(name "DQS3_A_C")
					(number "81")
				)
				(pin passive line
					(at 35.56 -99.06 180)
					(length 3.81)
					(name "DQS3_A_t")
					(number "83")
				)
				(pin passive line
					(at 35.56 -127 180)
					(length 3.81)
					(name "DM3_A_n")
					(number "84")
				)
				(pin passive line
					(at 35.56 -115.57 180)
					(length 3.81)
					(name "DQ28_A")
					(number "87")
				)
				(pin passive line
					(at 35.56 -118.11 180)
					(length 3.81)
					(name "DQ29_A")
					(number "88")
				)
				(pin passive line
					(at 35.56 -120.65 180)
					(length 3.81)
					(name "DQ30_A")
					(number "91")
				)
				(pin passive line
					(at 35.56 -123.19 180)
					(length 3.81)
					(name "DQ31_A")
					(number "92")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(name "CB0_A")
					(number "95")
				)
				(pin passive line
					(at 0 -69.85 0)
					(length 3.81)
					(name "CB1_A")
					(number "96")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 3.81)
					(name "CB2_A")
					(number "99")
				)
				(pin passive line
					(at 0 -62.23 0)
					(length 3.81)
					(name "DQS4_A_c")
					(number "100")
				)
				(pin passive line
					(at 0 -59.69 0)
					(length 3.81)
					(name "DQS4_A_t")
					(number "102")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(name "CB3_A")
					(number "103")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "CS0_A_n")
					(number "106")
				)
				(pin passive line
					(at 0 -21.59 0)
					(length 3.81)
					(name "CA0_A")
					(number "107")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 3.81)
					(name "CA1_A")
					(number "109")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "CS1_A_n")
					(number "110")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 3.81)
					(name "CA2_A")
					(number "113")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 3.81)
					(name "CA3_A")
					(number "114")
				)
				(pin passive line
					(at 0 -31.75 0)
					(length 3.81)
					(name "CA4_A")
					(number "115")
				)
				(pin passive line
					(at 0 -34.29 0)
					(length 3.81)
					(name "CA5_A")
					(number "116")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 3.81)
					(name "CA6_A")
					(number "119")
				)
				(pin passive line
					(at 0 -39.37 0)
					(length 3.81)
					(name "CA7_A")
					(number "120")
				)
				(pin passive line
					(at 0 -41.91 0)
					(length 3.81)
					(name "CA8_A")
					(number "121")
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 3.81)
					(name "CA9_A")
					(number "122")
				)
				(pin passive line
					(at 0 -46.99 0)
					(length 3.81)
					(name "CA10_A")
					(number "125")
				)
				(pin passive line
					(at 0 -49.53 0)
					(length 3.81)
					(name "CA11_A")
					(number "126")
				)
				(pin passive line
					(at 0 -52.07 0)
					(length 3.81)
					(name "CA12_A")
					(number "127")
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 3.81)
					(name "CK0_A_t")
					(number "131")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 3.81)
					(name "CK1_A_t")
					(number "132")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 3.81)
					(name "CK0_A_c")
					(number "133")
				)
				(pin passive line
					(at 0 -16.51 0)
					(length 3.81)
					(name "CK1_A_c")
					(number "134")
				)
			)
			(symbol "Bus_DDR5_SODIMM_Amphenol_10161033-002RHLF_2_1"
				(text "ECC"
					(at 17.78 -69.85 900)
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 3.81)
					(name "CK0_B_t")
					(number "137")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 3.81)
					(name "CK1_B_t")
					(number "138")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 3.81)
					(name "CK0_B_c")
					(number "139")
				)
				(pin passive line
					(at 0 -16.51 0)
					(length 3.81)
					(name "CK1_B_C")
					(number "140")
				)
				(pin passive line
					(at 0 -52.07 0)
					(length 3.81)
					(name "CA12_B")
					(number "144")
				)
				(pin passive line
					(at 0 -49.53 0)
					(length 3.81)
					(name "CA11_B")
					(number "145")
				)
				(pin passive line
					(at 0 -46.99 0)
					(length 3.81)
					(name "CA10_B")
					(number "146")
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 3.81)
					(name "CA9_B")
					(number "149")
				)
				(pin passive line
					(at 0 -41.91 0)
					(length 3.81)
					(name "CA8_B")
					(number "150")
				)
				(pin passive line
					(at 0 -39.37 0)
					(length 3.81)
					(name "CA7_B")
					(number "151")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 3.81)
					(name "CA6_B")
					(number "152")
				)
				(pin passive line
					(at 0 -34.29 0)
					(length 3.81)
					(name "CA5_B")
					(number "155")
				)
				(pin passive line
					(at 0 -31.75 0)
					(length 3.81)
					(name "CA4_B")
					(number "156")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 3.81)
					(name "CA3_B")
					(number "157")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 3.81)
					(name "CA2_B")
					(number "158")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "CS0_B_n")
					(number "161")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 3.81)
					(name "CA1_B")
					(number "162")
				)
				(pin passive line
					(at 0 -21.59 0)
					(length 3.81)
					(name "CA0_B")
					(number "164")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "CS1_B_N")
					(number "165")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 3.81)
					(name "CB0_B")
					(number "168")
				)
				(pin passive line
					(at 0 -62.23 0)
					(length 3.81)
					(name "DQS4_B_c")
					(number "169")
				)
				(pin passive line
					(at 0 -59.69 0)
					(length 3.81)
					(name "DQS4_B_T")
					(number "171")
				)
				(pin passive line
					(at 0 -69.85 0)
					(length 3.81)
					(name "CB1_B")
					(number "172")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(name "CB3_B")
					(number "175")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 3.81)
					(name "CB2_B")
					(number "176")
				)
				(pin passive line
					(at 35.56 -6.35 180)
					(length 3.81)
					(name "DQ0_B")
					(number "179")
				)
				(pin passive line
					(at 35.56 -8.89 180)
					(length 3.81)
					(name "DQ1_B")
					(number "180")
				)
				(pin passive line
					(at 35.56 -11.43 180)
					(length 3.81)
					(name "DQ2_B")
					(number "183")
				)
				(pin passive line
					(at 35.56 -13.97 180)
					(length 3.81)
					(name "DQ3_B")
					(number "184")
				)
				(pin passive line
					(at 35.56 -27.94 180)
					(length 3.81)
					(name "DM0_B_n")
					(number "187")
				)
				(pin passive line
					(at 35.56 -2.54 180)
					(length 3.81)
					(name "DQS0_B_C")
					(number "188")
				)
				(pin passive line
					(at 35.56 0 180)
					(length 3.81)
					(name "DQS0_B_t")
					(number "190")
				)
				(pin passive line
					(at 35.56 -16.51 180)
					(length 3.81)
					(name "DQ4_B")
					(number "191")
				)
				(pin passive line
					(at 35.56 -19.05 180)
					(length 3.81)
					(name "DQ5_B")
					(number "194")
				)
				(pin passive line
					(at 35.56 -21.59 180)
					(length 3.81)
					(name "DQ6_B")
					(number "195")
				)
				(pin passive line
					(at 35.56 -24.13 180)
					(length 3.81)
					(name "DQ7_B")
					(number "198")
				)
				(pin passive line
					(at 35.56 -39.37 180)
					(length 3.81)
					(name "DQ8_B")
					(number "199")
				)
				(pin passive line
					(at 35.56 -41.91 180)
					(length 3.81)
					(name "DQ9_B")
					(number "202")
				)
				(pin passive line
					(at 35.56 -44.45 180)
					(length 3.81)
					(name "DQ10_B")
					(number "203")
				)
				(pin passive line
					(at 35.56 -46.99 180)
					(length 3.81)
					(name "DQ11_B")
					(number "206")
				)
				(pin passive line
					(at 35.56 -35.56 180)
					(length 3.81)
					(name "DQS1_B_C")
					(number "207")
				)
				(pin passive line
					(at 35.56 -33.02 180)
					(length 3.81)
					(name "DQS1_B_t")
					(number "209")
				)
				(pin passive line
					(at 35.56 -60.96 180)
					(length 3.81)
					(name "DM1_B_n")
					(number "210")
				)
				(pin passive line
					(at 35.56 -49.53 180)
					(length 3.81)
					(name "DQ12_B")
					(number "213")
				)
				(pin passive line
					(at 35.56 -52.07 180)
					(length 3.81)
					(name "DQ13_B")
					(number "214")
				)
				(pin passive line
					(at 35.56 -54.61 180)
					(length 3.81)
					(name "DQ14_B")
					(number "217")
				)
				(pin passive line
					(at 35.56 -57.15 180)
					(length 3.81)
					(name "DQ15_B")
					(number "218")
				)
				(pin passive line
					(at 35.56 -72.39 180)
					(length 3.81)
					(name "DQ16_B")
					(number "221")
				)
				(pin passive line
					(at 35.56 -74.93 180)
					(length 3.81)
					(name "DQ17_B")
					(number "222")
				)
				(pin passive line
					(at 35.56 -77.47 180)
					(length 3.81)
					(name "DQ18_B")
					(number "225")
				)
				(pin passive line
					(at 35.56 -80.01 180)
					(length 3.81)
					(name "DQ19_B")
					(number "226")
				)
				(pin passive line
					(at 35.56 -93.98 180)
					(length 3.81)
					(name "DM2_B_n")
					(number "229")
				)
				(pin passive line
					(at 35.56 -68.58 180)
					(length 3.81)
					(name "DQS2_B_C")
					(number "230")
				)
				(pin passive line
					(at 35.56 -66.04 180)
					(length 3.81)
					(name "DQS2_B_t")
					(number "232")
				)
				(pin passive line
					(at 35.56 -82.55 180)
					(length 3.81)
					(name "DQ20_B")
					(number "233")
				)
				(pin passive line
					(at 35.56 -85.09 180)
					(length 3.81)
					(name "DQ21_B")
					(number "236")
				)
				(pin passive line
					(at 35.56 -87.63 180)
					(length 3.81)
					(name "DQ22_B")
					(number "237")
				)
				(pin passive line
					(at 35.56 -90.17 180)
					(length 3.81)
					(name "DQ23_B")
					(number "240")
				)
				(pin passive line
					(at 35.56 -105.41 180)
					(length 3.81)
					(name "DQ24_B")
					(number "241")
				)
				(pin passive line
					(at 35.56 -107.95 180)
					(length 3.81)
					(name "DQ25_B")
					(number "244")
				)
				(pin passive line
					(at 35.56 -110.49 180)
					(length 3.81)
					(name "DQ26_B")
					(number "245")
				)
				(pin passive line
					(at 35.56 -113.03 180)
					(length 3.81)
					(name "DQ27_B")
					(number "248")
				)
				(pin passive line
					(at 35.56 -101.6 180)
					(length 3.81)
					(name "DQS3_B_c")
					(number "249")
				)
				(pin passive line
					(at 35.56 -99.06 180)
					(length 3.81)
					(name "DQS3_B_t")
					(number "251")
				)
				(pin passive line
					(at 35.56 -127 180)
					(length 3.81)
					(name "DM3_B_n")
					(number "252")
				)
				(pin passive line
					(at 35.56 -115.57 180)
					(length 3.81)
					(name "DQ28_B")
					(number "255")
				)
				(pin passive line
					(at 35.56 -118.11 180)
					(length 3.81)
					(name "DQ29_B")
					(number "256")
				)
				(pin passive line
					(at 35.56 -120.65 180)
					(length 3.81)
					(name "DQ30_B")
					(number "259")
				)
				(pin passive line
					(at 35.56 -123.19 180)
					(length 3.81)
					(name "DQ31_B")
					(number "260")
				)
			)
			(symbol "Bus_DDR5_SODIMM_Amphenol_10161033-002RHLF_3_1"
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "VIN_BULK")
					(number "1")
				)
				(pin passive line
					(at 27.94 -11.43 180)
					(length 3.81)
					(name "HSA")
					(number "2")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VIN_BULK")
					(number "3")
				)
				(pin passive line
					(at 27.94 -13.97 180)
					(length 3.81)
					(name "HSCL")
					(number "4")
				)
				(pin no_connect line
					(at 3.81 -3.81 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "5")
				)
				(pin passive line
					(at 27.94 -16.51 180)
					(length 3.81)
					(name "HSDA")
					(number "6")
				)
				(pin passive line
					(at 27.94 -5.08 180)
					(length 3.81)
					(name "PWR_GOOD")
					(number "7")
				)
				(pin passive line
					(at 27.94 0 180)
					(length 3.81)
					(name "PWR_EN")
					(number "8")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "9")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(name "VSS")
					(number "10")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "13")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "14")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "17")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "18")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "21")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "24")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "25")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "28")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "29")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "32")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "33")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "36")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "37")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "40")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "43")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "44")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "47")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "48")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "51")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "52")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "55")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "56")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "59")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "60")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "63")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "66")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "67")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "70")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "71")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "74")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "75")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "78")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "79")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "82")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "85")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "86")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "89")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "90")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "93")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "94")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "97")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "98")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "101")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "104")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "105")
				)
				(pin passive line
					(at 27.94 -7.62 180)
					(length 3.81)
					(name "ALERT_n")
					(number "108")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "111")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "112")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "117")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "118")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "123")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "124")
				)
				(pin no_connect line
					(at 3.81 -6.35 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "128")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "129")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "130")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "135")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "136")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "141")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "142")
				)
				(pin no_connect line
					(at 3.81 -8.89 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "143")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "147")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "148")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "153")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "154")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "159")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "160")
				)
				(pin passive line
					(at 27.94 -2.54 180)
					(length 3.81)
					(name "RESET_n")
					(number "163")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "166")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "167")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "170")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "173")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "174")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "177")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "178")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "181")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "182")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "185")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "186")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "189")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "192")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "193")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "196")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "197")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "200")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "201")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "204")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "205")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "208")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "211")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "212")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "215")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "216")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "219")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "220")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "223")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "224")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "227")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "228")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "231")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "234")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "235")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "238")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "239")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "242")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "243")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "246")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "247")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "250")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "253")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "254")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "257")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "258")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "261")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "262")
				)
				(pin passive line
					(at 0 -21.59 0)
					(length 3.81)
					(name "")
					(number "SH")
				)
			)
			(embedded_fonts no)
		)
)
