(footprint "MicroSD_Amphenol_101-00660-68-6"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "SMT, MICRO, SD, CARD, CONNECTOR")
	(property "Reference" "REF**"
		(at -7.7 -9.1 0)
		(layer "F.SilkS")
	)
	(property "Value" "MicroSD_Amphenol_101-00660-68-6"
		(at -8.4 13 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Author: Antmicro"
		(at -8.4 14.2 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -8.4 15.4 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -8.4 16.6 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at 1.94 2.5)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "2" smd roundrect
		(at 0.84 2.1)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "3" smd roundrect
		(at -0.26 2.5)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "4" smd roundrect
		(at -1.36 2.7)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "5" smd roundrect
		(at -2.46 2.5)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "6" smd roundrect
		(at -3.56 2.7)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "7" smd roundrect
		(at -4.66 2.5)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "8" smd roundrect
		(at -5.76 2.5)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "9" smd roundrect
		(at -4.95 -7.8)
		(size 1.8 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "SH" smd roundrect
		(at -6.55 5.35)
		(size 1.4 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "SH" smd roundrect
		(at 0.75 -7.8)
		(size 1.8 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "SH" smd roundrect
		(at 6.6 6.35)
		(size 1.4 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(embedded_fonts no)
	(model "antmicro_101_00660_68_6.glb"
		(offset
			(xyz 0 -5.35 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
