(footprint "MicroSD_Amphenol_1140084168"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -6.6 -6.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "MicroSD_Amphenol_1140084168"
		(at -6.9 11.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -6.925 12.774 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -6.925 14.1 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -6.925 15.4 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at 3.124 5.254 180)
		(size 0.7 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 2.024 5.254 180)
		(size 0.7 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 0.925 5.254 180)
		(size 0.7 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -0.176 5.254 180)
		(size 0.7 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -1.276 5.254 180)
		(size 0.7 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -2.375 5.254 180)
		(size 0.7 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -3.476 5.254 180)
		(size 0.7 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -4.576 5.254 180)
		(size 0.7 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -5.675 -4.05)
		(size 1.4 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 5.424 -5.531 90)
		(size 1.4 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at -5.976 -2.48 90)
		(size 1.5 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at -5.776 5.129)
		(size 1.3 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at 5.575 5.129)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at 5.874 -3.13 90)
		(size 1.5 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_1140084168.glb"
		(offset
			(xyz 0 0.05 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
