(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Bus_M.2_2199119-5"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 45.72 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Bus_M.2_2199119-5"
				(at 45.72 -2.286 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Bus_M.2_2199119-5"
				(at 45.72 -4.572 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=2199119&DocType=Customer%20Drawing&DocLang=English&DocFormat=pdf&PartCntxt=2199119-5"
				(at 45.72 -6.858 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Key B, PCI connector, M.2, P: 0.5mm; H: 3.2mm; 30U'' AU"
				(at 45.72 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "2199119-5"
				(at 45.72 -9.398 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "TE Connectivity"
				(at 45.72 -11.938 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 45.72 -14.224 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "MODULE"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Bus_M.2_2199119-5_1_1"
				(pin input line
					(at 0 -93.98 0)
					(length 3.81)
					(name "CONFIG_3")
					(number "1")
				)
				(pin power_in line
					(at 33.02 -96.52 180)
					(length 3.81)
					(name "GND")
					(number "3")
				)
				(pin passive line
					(at 33.02 -96.52 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "5")
				)
				(pin output line
					(at 0 -78.74 0)
					(length 3.81)
					(name "~{PWR_OFF}")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 3.81)
					(name "USB_D+")
					(number "7")
				)
				(pin output line
					(at 33.02 -17.78 180)
					(length 3.81)
					(name "~{W_DISABLE1}")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 3.81)
					(name "USB_D-")
					(number "9")
				)
				(pin bidirectional line
					(at 33.02 -71.12 180)
					(length 3.81)
					(name "GPIO_9")
					(number "10")
				)
				(pin passive line
					(at 33.02 -96.52 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "11")
				)
				(pin bidirectional line
					(at 33.02 -60.96 180)
					(length 3.81)
					(name "GPIO_5")
					(number "20")
				)
				(pin input line
					(at 0 -86.36 0)
					(length 3.81)
					(name "CONFIG_0")
					(number "21")
				)
				(pin bidirectional line
					(at 33.02 -63.5 180)
					(length 3.81)
					(name "GPIO_6")
					(number "22")
				)
				(pin bidirectional line
					(at 33.02 -76.2 180)
					(length 3.81)
					(name "GPIO_11")
					(number "23")
				)
				(pin bidirectional line
					(at 33.02 -66.04 180)
					(length 3.81)
					(name "GPIO_7")
					(number "24")
				)
				(pin output line
					(at 33.02 -81.28 180)
					(length 3.81)
					(name "DPR")
					(number "25")
				)
				(pin bidirectional line
					(at 33.02 -73.66 180)
					(length 3.81)
					(name "GPIO_10")
					(number "26")
				)
				(pin passive line
					(at 33.02 -96.52 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "27")
				)
				(pin bidirectional line
					(at 33.02 -68.58 180)
					(length 3.81)
					(name "GPIO_8")
					(number "28")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 3.81)
					(name "PER1_N/USBSS_RX_N")
					(number "29")
					(alternate "PER1_N" input line)
					(alternate "USBSS_RX_N" input line)
				)
				(pin input line
					(at 0 -68.58 0)
					(length 3.81)
					(name "UIM-RESET")
					(number "30")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 3.81)
					(name "PER1_P/USBSS_RX_P")
					(number "31")
					(alternate "PER1_P" input line)
					(alternate "USBSS_RX_P" input line)
				)
				(pin input line
					(at 0 -66.04 0)
					(length 3.81)
					(name "UIM-CLK")
					(number "32")
				)
				(pin passive line
					(at 33.02 -96.52 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "33")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 3.81)
					(name "UIM-DATA")
					(number "34")
				)
				(pin output line
					(at 0 -35.56 0)
					(length 3.81)
					(name "PET1_N/USBSS_TX_N")
					(number "35")
					(alternate "PET1_N" output line)
					(alternate "USBSS_TX_N" output line)
				)
				(pin input line
					(at 0 -57.15 0)
					(length 3.81)
					(name "UIM-PWR")
					(number "36")
				)
				(pin output line
					(at 0 -33.02 0)
					(length 3.81)
					(name "PET1_P/USBSS_TX_P")
					(number "37")
					(alternate "PET1_P" output line)
					(alternate "USBSS_TX_P" output line)
				)
				(pin output line
					(at 0 -76.2 0)
					(length 3.81)
					(name "DEVSLP")
					(number "38")
				)
				(pin passive line
					(at 33.02 -96.52 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "39")
				)
				(pin bidirectional line
					(at 33.02 -48.26 180)
					(length 3.81)
					(name "GPIO_0")
					(number "40")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 3.81)
					(name "PER0_N")
					(number "41")
				)
				(pin bidirectional line
					(at 33.02 -50.8 180)
					(length 3.81)
					(name "GPIO_1")
					(number "42")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 3.81)
					(name "PER0_P")
					(number "43")
				)
				(pin bidirectional line
					(at 33.02 -53.34 180)
					(length 3.81)
					(name "GPIO_2")
					(number "44")
				)
				(pin passive line
					(at 33.02 -96.52 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "45")
				)
				(pin bidirectional line
					(at 33.02 -55.88 180)
					(length 3.81)
					(name "GPIO_3")
					(number "46")
				)
				(pin output line
					(at 0 -20.32 0)
					(length 3.81)
					(name "PET0_N")
					(number "47")
				)
				(pin bidirectional line
					(at 33.02 -58.42 180)
					(length 3.81)
					(name "GPIO_4")
					(number "48")
				)
				(pin output line
					(at 0 -17.78 0)
					(length 3.81)
					(name "PET0_P")
					(number "49")
				)
				(pin output line
					(at 0 0 0)
					(length 3.81)
					(name "~{PERST}")
					(number "50")
				)
				(pin passive line
					(at 33.02 -96.52 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "51")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "~{CLKREQ}")
					(number "52")
				)
				(pin output line
					(at 0 -12.7 0)
					(length 3.81)
					(name "REFCLK_N")
					(number "53")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "~{PEWAKE}")
					(number "54")
				)
				(pin output line
					(at 0 -10.16 0)
					(length 3.81)
					(name "REFCLK_P")
					(number "55")
				)
				(pin no_connect line
					(at 29.21 -6.35 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "56")
				)
				(pin passive line
					(at 33.02 -96.52 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "57")
				)
				(pin no_connect line
					(at 29.21 -5.08 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "58")
				)
				(pin input line
					(at 33.02 -20.32 180)
					(length 3.81)
					(name "ANTCTL0")
					(number "59")
				)
				(pin bidirectional line
					(at 33.02 -91.44 180)
					(length 3.81)
					(name "COEX3")
					(number "60")
				)
				(pin input line
					(at 33.02 -22.86 180)
					(length 3.81)
					(name "ANTCTL1")
					(number "61")
				)
				(pin bidirectional line
					(at 33.02 -88.9 180)
					(length 3.81)
					(name "COEX2")
					(number "62")
				)
				(pin input line
					(at 33.02 -25.4 180)
					(length 3.81)
					(name "ANTCTL2")
					(number "63")
				)
				(pin bidirectional line
					(at 33.02 -86.36 180)
					(length 3.81)
					(name "COEX1")
					(number "64")
				)
				(pin input line
					(at 33.02 -27.94 180)
					(length 3.81)
					(name "ANTCTL3")
					(number "65")
				)
				(pin output line
					(at 0 -73.66 0)
					(length 3.81)
					(name "SIM_DETECT")
					(number "66")
				)
				(pin output line
					(at 0 -81.28 0)
					(length 3.81)
					(name "~{RESET}")
					(number "67")
				)
				(pin output line
					(at 33.02 -12.7 180)
					(length 3.81)
					(name "SUSCLK")
					(number "68")
				)
				(pin input line
					(at 0 -88.9 0)
					(length 3.81)
					(name "CONFIG_1")
					(number "69")
				)
				(pin passive line
					(at 33.02 -96.52 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "71")
				)
				(pin passive line
					(at 33.02 -96.52 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "73")
				)
				(pin input line
					(at 0 -91.44 0)
					(length 3.81)
					(name "CONFIG_2")
					(number "75")
				)
				(pin passive line
					(at 33.02 -93.98 180)
					(length 3.81)
					(name "MP")
					(number "MP")
				)
				(pin power_in line
					(at 33.02 0 180)
					(length 3.81)
					(name "3.3V")
					(number "[2,4,70,72,74]")
				)
			)
			(embedded_fonts no)
		)
)
