(footprint "Bus_DDR4_SODIMM_TE_2309409"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "260 pin DDR4 SODIMM Right Angle Socket, 5.2 mm (0.205 in) Stack Height, https://www.te.com/usa-en/product-2309409-1.html")
	(property "Reference" "REF**"
		(at -36.726 -13.477 0)
		(layer "F.SilkS")
	)
	(property "Value" "Bus_DDR4_SODIMM_TE_2309409"
		(at -8.1 -7.7 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Author: Antmicro"
		(at -39.26 15 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -39.26 16.2 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -39.26 17.4 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -34.402 -8.077)
		(size 1.15 1.15)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 34.399 -8.077)
		(size 1.65 1.65)
		(drill 1.65)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd rect
		(at 33.374 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 33.124 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 32.874 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 32.624 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 32.374 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 32.124 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 31.874 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 31.624 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 31.374 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 31.124 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 30.874 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 30.624 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 30.374 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 30.124 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 29.874 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 29.624 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 29.374 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 29.124 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at 28.874 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 28.624 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 28.374 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 28.124 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 27.874 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 27.624 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at 27.374 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 27.124 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at 26.874 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 26.624 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 26.374 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at 26.124 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at 25.874 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at 25.624 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at 25.374 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at 25.124 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at 24.874 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at 24.624 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at 24.374 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at 24.124 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at 23.874 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at 23.624 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd rect
		(at 23.374 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd rect
		(at 23.124 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd rect
		(at 22.874 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd rect
		(at 22.624 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "45" smd rect
		(at 22.374 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "46" smd rect
		(at 22.124 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "47" smd rect
		(at 21.874 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "48" smd rect
		(at 21.624 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "49" smd rect
		(at 21.374 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "50" smd rect
		(at 21.124 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "51" smd rect
		(at 20.874 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "52" smd rect
		(at 20.624 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "53" smd rect
		(at 20.374 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "54" smd rect
		(at 20.124 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "55" smd rect
		(at 19.874 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "56" smd rect
		(at 19.624 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "57" smd rect
		(at 19.374 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "58" smd rect
		(at 19.124 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "59" smd rect
		(at 18.874 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "60" smd rect
		(at 18.624 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "61" smd rect
		(at 18.374 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "62" smd rect
		(at 18.124 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "63" smd rect
		(at 17.874 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "64" smd rect
		(at 17.624 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "65" smd rect
		(at 17.374 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "66" smd rect
		(at 17.124 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "67" smd rect
		(at 16.874 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "68" smd rect
		(at 16.624 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "69" smd rect
		(at 16.374 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "70" smd rect
		(at 16.124 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "71" smd rect
		(at 15.874 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "72" smd rect
		(at 15.624 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "73" smd rect
		(at 15.374 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "74" smd rect
		(at 15.124 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "75" smd rect
		(at 14.874 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "76" smd rect
		(at 14.624 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "77" smd rect
		(at 14.374 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "78" smd rect
		(at 14.124 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "79" smd rect
		(at 13.874 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "80" smd rect
		(at 13.624 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "81" smd rect
		(at 13.374 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "82" smd rect
		(at 13.124 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "83" smd rect
		(at 12.874 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "84" smd rect
		(at 12.624 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "85" smd rect
		(at 12.374 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "86" smd rect
		(at 12.124 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "87" smd rect
		(at 11.874 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "88" smd rect
		(at 11.624 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "89" smd rect
		(at 11.374 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "90" smd rect
		(at 11.124 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "91" smd rect
		(at 10.874 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "92" smd rect
		(at 10.624 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "93" smd rect
		(at 10.374 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "94" smd rect
		(at 10.124 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "95" smd rect
		(at 9.874 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "96" smd rect
		(at 9.624 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "97" smd rect
		(at 9.374 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "98" smd rect
		(at 9.124 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "99" smd rect
		(at 8.874 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "100" smd rect
		(at 8.624 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "101" smd rect
		(at 8.374 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "102" smd rect
		(at 8.124 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "103" smd rect
		(at 7.874 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "104" smd rect
		(at 7.624 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "105" smd rect
		(at 7.374 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "106" smd rect
		(at 7.124 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "107" smd rect
		(at 6.874 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "108" smd rect
		(at 6.624 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "109" smd rect
		(at 6.374 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "110" smd rect
		(at 6.124 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "111" smd rect
		(at 5.874 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "112" smd rect
		(at 5.624 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "113" smd rect
		(at 5.374 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "114" smd rect
		(at 5.124 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "115" smd rect
		(at 4.874 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "116" smd rect
		(at 4.624 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "117" smd rect
		(at 4.374 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "118" smd rect
		(at 4.124 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "119" smd rect
		(at 3.874 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "120" smd rect
		(at 3.624 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "121" smd rect
		(at 3.374 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "122" smd rect
		(at 3.124 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "123" smd rect
		(at 2.874 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "124" smd rect
		(at 2.624 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "125" smd rect
		(at 2.374 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "126" smd rect
		(at 2.124 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "127" smd rect
		(at 1.874 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "128" smd rect
		(at 1.624 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "129" smd rect
		(at 1.374 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "130" smd rect
		(at 1.124 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "131" smd rect
		(at 0.874 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "132" smd rect
		(at 0.624 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "133" smd rect
		(at 0.374 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "134" smd rect
		(at 0.124 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "135" smd rect
		(at -0.125 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "136" smd rect
		(at -0.375 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "137" smd rect
		(at -0.625 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "138" smd rect
		(at -0.875 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "139" smd rect
		(at -1.125 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "140" smd rect
		(at -1.375 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "141" smd rect
		(at -1.625 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "142" smd rect
		(at -1.875 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "143" smd rect
		(at -2.125 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "144" smd rect
		(at -2.375 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "145" smd rect
		(at -4.625 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "146" smd rect
		(at -4.875 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "147" smd rect
		(at -5.125 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "148" smd rect
		(at -5.375 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "149" smd rect
		(at -5.625 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "150" smd rect
		(at -5.875 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "151" smd rect
		(at -6.125 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "152" smd rect
		(at -6.375 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "153" smd rect
		(at -6.625 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "154" smd rect
		(at -6.875 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "155" smd rect
		(at -7.125 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "156" smd rect
		(at -7.375 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "157" smd rect
		(at -7.625 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "158" smd rect
		(at -7.875 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "159" smd rect
		(at -8.125 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "160" smd rect
		(at -8.375 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "161" smd rect
		(at -8.625 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "162" smd rect
		(at -8.875 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "163" smd rect
		(at -9.125 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "164" smd rect
		(at -9.375 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "165" smd rect
		(at -9.625 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "166" smd rect
		(at -9.875 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "167" smd rect
		(at -10.125 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "168" smd rect
		(at -10.375 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "169" smd rect
		(at -10.625 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "170" smd rect
		(at -10.875 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "171" smd rect
		(at -11.125 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "172" smd rect
		(at -11.375 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "173" smd rect
		(at -11.625 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "174" smd rect
		(at -11.875 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "175" smd rect
		(at -12.125 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "176" smd rect
		(at -12.375 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "177" smd rect
		(at -12.625 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "178" smd rect
		(at -12.875 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "179" smd rect
		(at -13.125 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "180" smd rect
		(at -13.375 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "181" smd rect
		(at -13.625 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "182" smd rect
		(at -13.875 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "183" smd rect
		(at -14.125 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "184" smd rect
		(at -14.375 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "185" smd rect
		(at -14.625 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "186" smd rect
		(at -14.875 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "187" smd rect
		(at -15.125 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "188" smd rect
		(at -15.375 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "189" smd rect
		(at -15.625 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "190" smd rect
		(at -15.875 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "191" smd rect
		(at -16.125 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "192" smd rect
		(at -16.375 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "193" smd rect
		(at -16.625 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "194" smd rect
		(at -16.875 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "195" smd rect
		(at -17.125 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "196" smd rect
		(at -17.375 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "197" smd rect
		(at -17.625 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "198" smd rect
		(at -17.875 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "199" smd rect
		(at -18.125 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "200" smd rect
		(at -18.375 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "201" smd rect
		(at -18.625 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "202" smd rect
		(at -18.875 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "203" smd rect
		(at -19.125 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "204" smd rect
		(at -19.375 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "205" smd rect
		(at -19.625 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "206" smd rect
		(at -19.875 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "207" smd rect
		(at -20.125 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "208" smd rect
		(at -20.375 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "209" smd rect
		(at -20.625 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "210" smd rect
		(at -20.875 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "211" smd rect
		(at -21.125 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "212" smd rect
		(at -21.375 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "213" smd rect
		(at -21.625 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "214" smd rect
		(at -21.875 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "215" smd rect
		(at -22.125 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "216" smd rect
		(at -22.375 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "217" smd rect
		(at -22.625 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "218" smd rect
		(at -22.875 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "219" smd rect
		(at -23.125 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "220" smd rect
		(at -23.375 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "221" smd rect
		(at -23.625 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "222" smd rect
		(at -23.875 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "223" smd rect
		(at -24.125 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "224" smd rect
		(at -24.375 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "225" smd rect
		(at -24.625 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "226" smd rect
		(at -24.875 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "227" smd rect
		(at -25.125 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "228" smd rect
		(at -25.375 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "229" smd rect
		(at -25.625 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "230" smd rect
		(at -25.875 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "231" smd rect
		(at -26.125 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "232" smd rect
		(at -26.375 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "233" smd rect
		(at -26.625 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "234" smd rect
		(at -26.875 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "235" smd rect
		(at -27.125 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "236" smd rect
		(at -27.375 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "237" smd rect
		(at -27.625 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "238" smd rect
		(at -27.875 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "239" smd rect
		(at -28.125 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "240" smd rect
		(at -28.375 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "241" smd rect
		(at -28.625 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "242" smd rect
		(at -28.875 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "243" smd rect
		(at -29.125 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "244" smd rect
		(at -29.375 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "245" smd rect
		(at -29.625 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "246" smd rect
		(at -29.875 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "247" smd rect
		(at -30.125 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "248" smd rect
		(at -30.375 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "249" smd rect
		(at -30.625 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "250" smd rect
		(at -30.875 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "251" smd rect
		(at -31.125 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "252" smd rect
		(at -31.375 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "253" smd rect
		(at -31.625 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "254" smd rect
		(at -31.875 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "255" smd rect
		(at -32.125 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "256" smd rect
		(at -32.375 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "257" smd rect
		(at -32.625 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "258" smd rect
		(at -32.875 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "259" smd rect
		(at -33.125 -12.176)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "260" smd rect
		(at -33.375 -3.979)
		(size 0.3 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "S1" smd rect
		(at 33.798 3.925)
		(size 3.5 4.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "S2" smd rect
		(at -33.8 3.925)
		(size 3.5 4.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_2309409_1.glb"
		(offset
			(xyz 0.0005 -12.925 2.8)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
