(footprint "TE_2309413"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "260 pin DDR4 SODIMM Right Angle Socket, 9.2 mm (0.362 in) Stack Height, https://www.te.com/global-en/product-2309413-1.html")
	(tags "ddr4 sodimm right angle 9.2mm height jetson som")
	(property "Reference" "REF**"
		(at -36.75 -13.25 0)
		(layer "F.SilkS")
	)
	(property "Value" "TE_2309413"
		(at -38 14.25 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -38 15.5 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -38 16.75 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -38 18 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -34.406 -7.926)
		(size 1.15 1.15)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 34.395 -7.926)
		(size 1.65 1.65)
		(drill 1.65)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd rect
		(at 33.369 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 33.119 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 32.869 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 32.619 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 32.369 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 32.119 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 31.87 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 31.62 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 31.37 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 31.12 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 30.87 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 30.62 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 30.37 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 30.12 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 29.87 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 29.62 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 29.37 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 29.12 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at 28.87 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 28.62 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 28.37 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 28.12 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 27.87 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 27.62 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at 27.37 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 27.12 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at 26.87 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 26.62 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 26.37 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at 26.12 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at 25.87 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at 25.62 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at 25.37 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at 25.12 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at 24.87 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at 24.62 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at 24.37 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at 24.12 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at 23.87 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at 23.62 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd rect
		(at 23.37 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd rect
		(at 23.12 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd rect
		(at 22.87 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd rect
		(at 22.62 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "45" smd rect
		(at 22.37 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "46" smd rect
		(at 22.12 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "47" smd rect
		(at 21.87 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "48" smd rect
		(at 21.62 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "49" smd rect
		(at 21.37 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "50" smd rect
		(at 21.12 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "51" smd rect
		(at 20.87 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "52" smd rect
		(at 20.62 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "53" smd rect
		(at 20.37 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "54" smd rect
		(at 20.12 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "55" smd rect
		(at 19.87 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "56" smd rect
		(at 19.62 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "57" smd rect
		(at 19.37 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "58" smd rect
		(at 19.12 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "59" smd rect
		(at 18.87 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "60" smd rect
		(at 18.62 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "61" smd rect
		(at 18.37 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "62" smd rect
		(at 18.12 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "63" smd rect
		(at 17.87 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "64" smd rect
		(at 17.62 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "65" smd rect
		(at 17.37 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "66" smd rect
		(at 17.12 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "67" smd rect
		(at 16.87 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "68" smd rect
		(at 16.62 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "69" smd rect
		(at 16.37 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "70" smd rect
		(at 16.12 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "71" smd rect
		(at 15.87 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "72" smd rect
		(at 15.62 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "73" smd rect
		(at 15.37 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "74" smd rect
		(at 15.12 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "75" smd rect
		(at 14.87 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "76" smd rect
		(at 14.62 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "77" smd rect
		(at 14.37 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "78" smd rect
		(at 14.12 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "79" smd rect
		(at 13.87 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "80" smd rect
		(at 13.62 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "81" smd rect
		(at 13.37 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "82" smd rect
		(at 13.12 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "83" smd rect
		(at 12.87 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "84" smd rect
		(at 12.62 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "85" smd rect
		(at 12.37 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "86" smd rect
		(at 12.12 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "87" smd rect
		(at 11.87 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "88" smd rect
		(at 11.62 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "89" smd rect
		(at 11.37 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "90" smd rect
		(at 11.12 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "91" smd rect
		(at 10.87 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "92" smd rect
		(at 10.62 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "93" smd rect
		(at 10.37 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "94" smd rect
		(at 10.12 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "95" smd rect
		(at 9.87 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "96" smd rect
		(at 9.62 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "97" smd rect
		(at 9.37 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "98" smd rect
		(at 9.12 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "99" smd rect
		(at 8.87 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "100" smd rect
		(at 8.62 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "101" smd rect
		(at 8.37 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "102" smd rect
		(at 8.12 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "103" smd rect
		(at 7.869 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "104" smd rect
		(at 7.619 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "105" smd rect
		(at 7.369 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "106" smd rect
		(at 7.119 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "107" smd rect
		(at 6.869 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "108" smd rect
		(at 6.619 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "109" smd rect
		(at 6.369 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "110" smd rect
		(at 6.119 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "111" smd rect
		(at 5.869 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "112" smd rect
		(at 5.619 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "113" smd rect
		(at 5.369 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "114" smd rect
		(at 5.12 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "115" smd rect
		(at 4.87 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "116" smd rect
		(at 4.62 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "117" smd rect
		(at 4.37 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "118" smd rect
		(at 4.12 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "119" smd rect
		(at 3.87 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "120" smd rect
		(at 3.62 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "121" smd rect
		(at 3.37 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "122" smd rect
		(at 3.12 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "123" smd rect
		(at 2.87 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "124" smd rect
		(at 2.62 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "125" smd rect
		(at 2.37 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "126" smd rect
		(at 2.12 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "127" smd rect
		(at 1.87 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "128" smd rect
		(at 1.62 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "129" smd rect
		(at 1.37 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "130" smd rect
		(at 1.12 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "131" smd rect
		(at 0.869 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "132" smd rect
		(at 0.619 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "133" smd rect
		(at 0.369 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "134" smd rect
		(at 0.119 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "135" smd rect
		(at -0.131 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "136" smd rect
		(at -0.38 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "137" smd rect
		(at -0.63 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "138" smd rect
		(at -0.88 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "139" smd rect
		(at -1.131 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "140" smd rect
		(at -1.381 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "141" smd rect
		(at -1.631 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "142" smd rect
		(at -1.881 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "143" smd rect
		(at -2.13 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "144" smd rect
		(at -2.38 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "145" smd rect
		(at -4.63 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "146" smd rect
		(at -4.88 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "147" smd rect
		(at -5.13 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "148" smd rect
		(at -5.38 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "149" smd rect
		(at -5.63 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "150" smd rect
		(at -5.88 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "151" smd rect
		(at -6.13 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "152" smd rect
		(at -6.38 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "153" smd rect
		(at -6.63 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "154" smd rect
		(at -6.88 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "155" smd rect
		(at -7.13 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "156" smd rect
		(at -7.38 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "157" smd rect
		(at -7.63 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "158" smd rect
		(at -7.88 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "159" smd rect
		(at -8.131 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "160" smd rect
		(at -8.381 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "161" smd rect
		(at -8.631 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "162" smd rect
		(at -8.881 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "163" smd rect
		(at -9.131 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "164" smd rect
		(at -9.381 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "165" smd rect
		(at -9.631 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "166" smd rect
		(at -9.881 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "167" smd rect
		(at -10.131 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "168" smd rect
		(at -10.381 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "169" smd rect
		(at -10.631 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "170" smd rect
		(at -10.881 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "171" smd rect
		(at -11.131 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "172" smd rect
		(at -11.381 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "173" smd rect
		(at -11.631 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "174" smd rect
		(at -11.881 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "175" smd rect
		(at -12.131 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "176" smd rect
		(at -12.381 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "177" smd rect
		(at -12.631 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "178" smd rect
		(at -12.881 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "179" smd rect
		(at -13.131 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "180" smd rect
		(at -13.381 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "181" smd rect
		(at -13.631 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "182" smd rect
		(at -13.881 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "183" smd rect
		(at -14.131 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "184" smd rect
		(at -14.381 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "185" smd rect
		(at -14.631 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "186" smd rect
		(at -14.881 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "187" smd rect
		(at -15.131 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "188" smd rect
		(at -15.381 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "189" smd rect
		(at -15.631 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "190" smd rect
		(at -15.881 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "191" smd rect
		(at -16.13 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "192" smd rect
		(at -16.38 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "193" smd rect
		(at -16.63 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "194" smd rect
		(at -16.88 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "195" smd rect
		(at -17.13 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "196" smd rect
		(at -17.38 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "197" smd rect
		(at -17.63 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "198" smd rect
		(at -17.88 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "199" smd rect
		(at -18.13 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "200" smd rect
		(at -18.38 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "201" smd rect
		(at -18.63 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "202" smd rect
		(at -18.88 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "203" smd rect
		(at -19.13 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "204" smd rect
		(at -19.38 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "205" smd rect
		(at -19.63 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "206" smd rect
		(at -19.88 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "207" smd rect
		(at -20.13 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "208" smd rect
		(at -20.38 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "209" smd rect
		(at -20.63 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "210" smd rect
		(at -20.88 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "211" smd rect
		(at -21.13 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "212" smd rect
		(at -21.38 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "213" smd rect
		(at -21.63 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "214" smd rect
		(at -21.88 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "215" smd rect
		(at -22.13 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "216" smd rect
		(at -22.38 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "217" smd rect
		(at -22.63 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "218" smd rect
		(at -22.88 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "219" smd rect
		(at -23.13 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "220" smd rect
		(at -23.38 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "221" smd rect
		(at -23.63 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "222" smd rect
		(at -23.88 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "223" smd rect
		(at -24.13 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "224" smd rect
		(at -24.38 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "225" smd rect
		(at -24.63 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "226" smd rect
		(at -24.88 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "227" smd rect
		(at -25.13 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "228" smd rect
		(at -25.38 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "229" smd rect
		(at -25.63 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "230" smd rect
		(at -25.88 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "231" smd rect
		(at -26.13 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "232" smd rect
		(at -26.38 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "233" smd rect
		(at -26.63 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "234" smd rect
		(at -26.88 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "235" smd rect
		(at -27.13 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "236" smd rect
		(at -27.38 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "237" smd rect
		(at -27.63 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "238" smd rect
		(at -27.88 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "239" smd rect
		(at -28.13 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "240" smd rect
		(at -28.38 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "241" smd rect
		(at -28.63 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "242" smd rect
		(at -28.88 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "243" smd rect
		(at -29.13 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "244" smd rect
		(at -29.38 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "245" smd rect
		(at -29.63 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "246" smd rect
		(at -29.88 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "247" smd rect
		(at -30.13 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "248" smd rect
		(at -30.38 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "249" smd rect
		(at -30.63 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "250" smd rect
		(at -30.88 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "251" smd rect
		(at -31.13 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "252" smd rect
		(at -31.38 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "253" smd rect
		(at -31.63 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "254" smd rect
		(at -31.88 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "255" smd rect
		(at -32.131 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "256" smd rect
		(at -32.381 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "257" smd rect
		(at -32.631 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "258" smd rect
		(at -32.881 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "259" smd rect
		(at -33.131 -12.026 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "260" smd rect
		(at -33.381 -3.826 90)
		(size 1.75 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "261" smd rect
		(at -37.756 0.073 180)
		(size 2 3.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "262" smd rect
		(at 37.744 4.073 180)
		(size 2 3.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_2309413_1.glb"
		(offset
			(xyz -0.0044 -12.925 4.6353)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
