(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "2822541-1"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 40.64 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "2822541-1"
				(at 40.64 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "2822541-1"
				(at 40.64 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://sigma.octopart.com/111080620/technical_drawing/TE-Connectivity-2822541-1.pdf"
				(at 40.64 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "SIM card connector"
				(at 40.64 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "2822541-1"
				(at 40.64 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "TE Connectivity"
				(at 40.64 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 40.64 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 40.64 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "CONNECTOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "2822541-1_0_1")
			(symbol "2822541-1_1_1"
				(pin passive line
					(at 0 -16.51 0)
					(length 2.54)
					(name "SW")
					(number "7")
				)
				(pin passive line
					(at 25.4 -16.51 180)
					(length 2.54)
					(hide yes)
					(name "Shell")
					(number "8")
				)
				(pin passive line
					(at 25.4 -16.51 180)
					(length 2.54)
					(hide yes)
					(name "Shell")
					(number "9")
				)
				(pin passive line
					(at 25.4 -16.51 180)
					(length 2.54)
					(name "Shell")
					(number "10")
				)
				(pin passive line
					(at 25.4 -16.51 180)
					(length 2.54)
					(hide yes)
					(name "Shell")
					(number "11")
				)
				(pin passive line
					(at 25.4 -16.51 180)
					(length 2.54)
					(hide yes)
					(name "Shell")
					(number "12")
				)
				(pin passive line
					(at 25.4 -16.51 180)
					(length 2.54)
					(hide yes)
					(name "Shell")
					(number "13")
				)
				(pin passive line
					(at 25.4 -16.51 180)
					(length 2.54)
					(hide yes)
					(name "Shell")
					(number "14")
				)
				(pin passive line
					(at 25.4 -16.51 180)
					(length 2.54)
					(hide yes)
					(name "Shell")
					(number "15")
				)
				(pin passive line
					(at 25.4 -16.51 180)
					(length 2.54)
					(hide yes)
					(name "Shell")
					(number "16")
				)
				(pin passive line
					(at 25.4 -16.51 180)
					(length 2.54)
					(hide yes)
					(name "Shell")
					(number "17")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "C1")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 2.54)
					(name "RST")
					(number "C2")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 2.54)
					(name "CLK")
					(number "C3")
				)
				(pin power_in line
					(at 25.4 -13.97 180)
					(length 2.54)
					(name "GND")
					(number "C5")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VPP")
					(number "C6")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 2.54)
					(name "I/O")
					(number "C7")
				)
			)
			(embedded_fonts no)
		)
)
