(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Bus_DDR3_SODIMM_TE_2-2013289-1"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 36.83 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Bus_DDR3_SODIMM_TE_2-2013289-1"
				(at 36.83 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Bus_DDR3_SODIMM_TE_2-2013289-1"
				(at 36.83 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.farnell.com/datasheets/1648402.pdf"
				(at 36.83 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Memory Card Connector, DDR3, SODIMM, Cam-In Locking, 204 Contacts, Copper Alloy"
				(at 36.83 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "2-2013289-1"
				(at 36.83 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "TE Connectivity"
				(at 36.83 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 36.83 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 36.83 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "DDR, SDRAM, CONNECTOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Bus_DDR3_SODIMM_TE_2-2013289-1_1_1"
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 22.86 0 180)
					(length 3.81)
					(name "2")
					(number "2")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "3")
					(number "3")
				)
				(pin passive line
					(at 22.86 -2.54 180)
					(length 3.81)
					(name "4")
					(number "4")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "5")
					(number "5")
				)
				(pin passive line
					(at 22.86 -5.08 180)
					(length 3.81)
					(name "6")
					(number "6")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "7")
					(number "7")
				)
				(pin passive line
					(at 22.86 -7.62 180)
					(length 3.81)
					(name "8")
					(number "8")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "9")
					(number "9")
				)
				(pin passive line
					(at 22.86 -10.16 180)
					(length 3.81)
					(name "10")
					(number "10")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "11")
					(number "11")
				)
				(pin passive line
					(at 22.86 -12.7 180)
					(length 3.81)
					(name "12")
					(number "12")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "13")
					(number "13")
				)
				(pin passive line
					(at 22.86 -15.24 180)
					(length 3.81)
					(name "14")
					(number "14")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 3.81)
					(name "15")
					(number "15")
				)
				(pin passive line
					(at 22.86 -17.78 180)
					(length 3.81)
					(name "16")
					(number "16")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(name "17")
					(number "17")
				)
				(pin passive line
					(at 22.86 -20.32 180)
					(length 3.81)
					(name "18")
					(number "18")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 3.81)
					(name "19")
					(number "19")
				)
				(pin passive line
					(at 22.86 -22.86 180)
					(length 3.81)
					(name "20")
					(number "20")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(name "21")
					(number "21")
				)
				(pin passive line
					(at 22.86 -25.4 180)
					(length 3.81)
					(name "22")
					(number "22")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(name "23")
					(number "23")
				)
				(pin passive line
					(at 22.86 -27.94 180)
					(length 3.81)
					(name "24")
					(number "24")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(name "25")
					(number "25")
				)
				(pin passive line
					(at 22.86 -30.48 180)
					(length 3.81)
					(name "26")
					(number "26")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(name "27")
					(number "27")
				)
				(pin passive line
					(at 22.86 -33.02 180)
					(length 3.81)
					(name "28")
					(number "28")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 3.81)
					(name "29")
					(number "29")
				)
				(pin passive line
					(at 22.86 -35.56 180)
					(length 3.81)
					(name "30")
					(number "30")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 3.81)
					(name "31")
					(number "31")
				)
				(pin passive line
					(at 22.86 -38.1 180)
					(length 3.81)
					(name "32")
					(number "32")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(name "33")
					(number "33")
				)
				(pin passive line
					(at 22.86 -40.64 180)
					(length 3.81)
					(name "34")
					(number "34")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 3.81)
					(name "35")
					(number "35")
				)
				(pin passive line
					(at 22.86 -43.18 180)
					(length 3.81)
					(name "36")
					(number "36")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 3.81)
					(name "37")
					(number "37")
				)
				(pin passive line
					(at 22.86 -45.72 180)
					(length 3.81)
					(name "38")
					(number "38")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 3.81)
					(name "39")
					(number "39")
				)
				(pin passive line
					(at 22.86 -48.26 180)
					(length 3.81)
					(name "40")
					(number "40")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "41")
					(number "41")
				)
				(pin passive line
					(at 22.86 -50.8 180)
					(length 3.81)
					(name "42")
					(number "42")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 3.81)
					(name "43")
					(number "43")
				)
				(pin passive line
					(at 22.86 -53.34 180)
					(length 3.81)
					(name "44")
					(number "44")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(name "45")
					(number "45")
				)
				(pin passive line
					(at 22.86 -55.88 180)
					(length 3.81)
					(name "46")
					(number "46")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "47")
					(number "47")
				)
				(pin passive line
					(at 22.86 -58.42 180)
					(length 3.81)
					(name "48")
					(number "48")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 3.81)
					(name "49")
					(number "49")
				)
				(pin passive line
					(at 22.86 -60.96 180)
					(length 3.81)
					(name "50")
					(number "50")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 3.81)
					(name "51")
					(number "51")
				)
				(pin passive line
					(at 22.86 -63.5 180)
					(length 3.81)
					(name "52")
					(number "52")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "53")
					(number "53")
				)
				(pin passive line
					(at 22.86 -66.04 180)
					(length 3.81)
					(name "54")
					(number "54")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 3.81)
					(name "55")
					(number "55")
				)
				(pin passive line
					(at 22.86 -68.58 180)
					(length 3.81)
					(name "56")
					(number "56")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 3.81)
					(name "57")
					(number "57")
				)
				(pin passive line
					(at 22.86 -71.12 180)
					(length 3.81)
					(name "58")
					(number "58")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 3.81)
					(name "59")
					(number "59")
				)
				(pin passive line
					(at 22.86 -73.66 180)
					(length 3.81)
					(name "60")
					(number "60")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 3.81)
					(name "61")
					(number "61")
				)
				(pin passive line
					(at 22.86 -76.2 180)
					(length 3.81)
					(name "62")
					(number "62")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 3.81)
					(name "63")
					(number "63")
				)
				(pin passive line
					(at 22.86 -78.74 180)
					(length 3.81)
					(name "64")
					(number "64")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 3.81)
					(name "65")
					(number "65")
				)
				(pin passive line
					(at 22.86 -81.28 180)
					(length 3.81)
					(name "66")
					(number "66")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 3.81)
					(name "67")
					(number "67")
				)
				(pin passive line
					(at 22.86 -83.82 180)
					(length 3.81)
					(name "68")
					(number "68")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 3.81)
					(name "69")
					(number "69")
				)
				(pin passive line
					(at 22.86 -86.36 180)
					(length 3.81)
					(name "70")
					(number "70")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 3.81)
					(name "71")
					(number "71")
				)
				(pin passive line
					(at 22.86 -88.9 180)
					(length 3.81)
					(name "72")
					(number "72")
				)
				(pin passive line
					(at 22.86 -92.71 180)
					(length 3.81)
					(name "SHIELD")
					(number "SH")
				)
			)
			(symbol "Bus_DDR3_SODIMM_TE_2-2013289-1_2_1"
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "73")
					(number "73")
				)
				(pin passive line
					(at 22.86 0 180)
					(length 3.81)
					(name "74")
					(number "74")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "75")
					(number "75")
				)
				(pin passive line
					(at 22.86 -2.54 180)
					(length 3.81)
					(name "76")
					(number "76")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "77")
					(number "77")
				)
				(pin passive line
					(at 22.86 -5.08 180)
					(length 3.81)
					(name "78")
					(number "78")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "79")
					(number "79")
				)
				(pin passive line
					(at 22.86 -7.62 180)
					(length 3.81)
					(name "80")
					(number "80")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "81")
					(number "81")
				)
				(pin passive line
					(at 22.86 -10.16 180)
					(length 3.81)
					(name "82")
					(number "82")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "83")
					(number "83")
				)
				(pin passive line
					(at 22.86 -12.7 180)
					(length 3.81)
					(name "84")
					(number "84")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "85")
					(number "85")
				)
				(pin passive line
					(at 22.86 -15.24 180)
					(length 3.81)
					(name "86")
					(number "86")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 3.81)
					(name "87")
					(number "87")
				)
				(pin passive line
					(at 22.86 -17.78 180)
					(length 3.81)
					(name "88")
					(number "88")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(name "89")
					(number "89")
				)
				(pin passive line
					(at 22.86 -20.32 180)
					(length 3.81)
					(name "90")
					(number "90")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 3.81)
					(name "91")
					(number "91")
				)
				(pin passive line
					(at 22.86 -22.86 180)
					(length 3.81)
					(name "92")
					(number "92")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(name "93")
					(number "93")
				)
				(pin passive line
					(at 22.86 -25.4 180)
					(length 3.81)
					(name "94")
					(number "94")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(name "95")
					(number "95")
				)
				(pin passive line
					(at 22.86 -27.94 180)
					(length 3.81)
					(name "96")
					(number "96")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(name "97")
					(number "97")
				)
				(pin passive line
					(at 22.86 -30.48 180)
					(length 3.81)
					(name "98")
					(number "98")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(name "99")
					(number "99")
				)
				(pin passive line
					(at 22.86 -33.02 180)
					(length 3.81)
					(name "100")
					(number "100")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 3.81)
					(name "101")
					(number "101")
				)
				(pin passive line
					(at 22.86 -35.56 180)
					(length 3.81)
					(name "102")
					(number "102")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 3.81)
					(name "103")
					(number "103")
				)
				(pin passive line
					(at 22.86 -38.1 180)
					(length 3.81)
					(name "104")
					(number "104")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(name "105")
					(number "105")
				)
				(pin passive line
					(at 22.86 -40.64 180)
					(length 3.81)
					(name "106")
					(number "106")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 3.81)
					(name "107")
					(number "107")
				)
				(pin passive line
					(at 22.86 -43.18 180)
					(length 3.81)
					(name "108")
					(number "108")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 3.81)
					(name "109")
					(number "109")
				)
				(pin passive line
					(at 22.86 -45.72 180)
					(length 3.81)
					(name "110")
					(number "110")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 3.81)
					(name "111")
					(number "111")
				)
				(pin passive line
					(at 22.86 -48.26 180)
					(length 3.81)
					(name "112")
					(number "112")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "113")
					(number "113")
				)
				(pin passive line
					(at 22.86 -50.8 180)
					(length 3.81)
					(name "114")
					(number "114")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 3.81)
					(name "115")
					(number "115")
				)
				(pin passive line
					(at 22.86 -53.34 180)
					(length 3.81)
					(name "116")
					(number "116")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(name "117")
					(number "117")
				)
				(pin passive line
					(at 22.86 -55.88 180)
					(length 3.81)
					(name "118")
					(number "118")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "119")
					(number "119")
				)
				(pin passive line
					(at 22.86 -58.42 180)
					(length 3.81)
					(name "120")
					(number "120")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 3.81)
					(name "121")
					(number "121")
				)
				(pin passive line
					(at 22.86 -60.96 180)
					(length 3.81)
					(name "122")
					(number "122")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 3.81)
					(name "123")
					(number "123")
				)
				(pin passive line
					(at 22.86 -63.5 180)
					(length 3.81)
					(name "124")
					(number "124")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "125")
					(number "125")
				)
				(pin passive line
					(at 22.86 -66.04 180)
					(length 3.81)
					(name "126")
					(number "126")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 3.81)
					(name "127")
					(number "127")
				)
				(pin passive line
					(at 22.86 -68.58 180)
					(length 3.81)
					(name "128")
					(number "128")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 3.81)
					(name "129")
					(number "129")
				)
				(pin passive line
					(at 22.86 -71.12 180)
					(length 3.81)
					(name "130")
					(number "130")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 3.81)
					(name "131")
					(number "131")
				)
				(pin passive line
					(at 22.86 -73.66 180)
					(length 3.81)
					(name "132")
					(number "132")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 3.81)
					(name "133")
					(number "133")
				)
				(pin passive line
					(at 22.86 -76.2 180)
					(length 3.81)
					(name "134")
					(number "134")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 3.81)
					(name "135")
					(number "135")
				)
				(pin passive line
					(at 22.86 -78.74 180)
					(length 3.81)
					(name "136")
					(number "136")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 3.81)
					(name "137")
					(number "137")
				)
				(pin passive line
					(at 22.86 -81.28 180)
					(length 3.81)
					(name "138")
					(number "138")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 3.81)
					(name "139")
					(number "139")
				)
				(pin passive line
					(at 22.86 -83.82 180)
					(length 3.81)
					(name "140")
					(number "140")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 3.81)
					(name "141")
					(number "141")
				)
				(pin passive line
					(at 22.86 -86.36 180)
					(length 3.81)
					(name "142")
					(number "142")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 3.81)
					(name "143")
					(number "143")
				)
				(pin passive line
					(at 22.86 -88.9 180)
					(length 3.81)
					(name "144")
					(number "144")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 3.81)
					(name "145")
					(number "145")
				)
				(pin passive line
					(at 22.86 -91.44 180)
					(length 3.81)
					(name "146")
					(number "146")
				)
				(pin passive line
					(at 0 -93.98 0)
					(length 3.81)
					(name "147")
					(number "147")
				)
				(pin passive line
					(at 22.86 -93.98 180)
					(length 3.81)
					(name "148")
					(number "148")
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 3.81)
					(name "149")
					(number "149")
				)
				(pin passive line
					(at 22.86 -96.52 180)
					(length 3.81)
					(name "150")
					(number "150")
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 3.81)
					(name "151")
					(number "151")
				)
				(pin passive line
					(at 22.86 -99.06 180)
					(length 3.81)
					(name "152")
					(number "152")
				)
				(pin passive line
					(at 0 -101.6 0)
					(length 3.81)
					(name "153")
					(number "153")
				)
				(pin passive line
					(at 22.86 -101.6 180)
					(length 3.81)
					(name "154")
					(number "154")
				)
				(pin passive line
					(at 0 -104.14 0)
					(length 3.81)
					(name "155")
					(number "155")
				)
				(pin passive line
					(at 22.86 -104.14 180)
					(length 3.81)
					(name "156")
					(number "156")
				)
				(pin passive line
					(at 0 -106.68 0)
					(length 3.81)
					(name "157")
					(number "157")
				)
				(pin passive line
					(at 22.86 -106.68 180)
					(length 3.81)
					(name "158")
					(number "158")
				)
				(pin passive line
					(at 0 -109.22 0)
					(length 3.81)
					(name "159")
					(number "159")
				)
				(pin passive line
					(at 22.86 -109.22 180)
					(length 3.81)
					(name "160")
					(number "160")
				)
				(pin passive line
					(at 0 -111.76 0)
					(length 3.81)
					(name "161")
					(number "161")
				)
				(pin passive line
					(at 22.86 -111.76 180)
					(length 3.81)
					(name "162")
					(number "162")
				)
				(pin passive line
					(at 0 -114.3 0)
					(length 3.81)
					(name "163")
					(number "163")
				)
				(pin passive line
					(at 22.86 -114.3 180)
					(length 3.81)
					(name "164")
					(number "164")
				)
				(pin passive line
					(at 0 -116.84 0)
					(length 3.81)
					(name "165")
					(number "165")
				)
				(pin passive line
					(at 22.86 -116.84 180)
					(length 3.81)
					(name "166")
					(number "166")
				)
				(pin passive line
					(at 0 -119.38 0)
					(length 3.81)
					(name "167")
					(number "167")
				)
				(pin passive line
					(at 22.86 -119.38 180)
					(length 3.81)
					(name "168")
					(number "168")
				)
				(pin passive line
					(at 0 -121.92 0)
					(length 3.81)
					(name "169")
					(number "169")
				)
				(pin passive line
					(at 22.86 -121.92 180)
					(length 3.81)
					(name "170")
					(number "170")
				)
				(pin passive line
					(at 0 -124.46 0)
					(length 3.81)
					(name "171")
					(number "171")
				)
				(pin passive line
					(at 22.86 -124.46 180)
					(length 3.81)
					(name "172")
					(number "172")
				)
				(pin passive line
					(at 0 -127 0)
					(length 3.81)
					(name "173")
					(number "173")
				)
				(pin passive line
					(at 22.86 -127 180)
					(length 3.81)
					(name "174")
					(number "174")
				)
				(pin passive line
					(at 0 -129.54 0)
					(length 3.81)
					(name "175")
					(number "175")
				)
				(pin passive line
					(at 22.86 -129.54 180)
					(length 3.81)
					(name "176")
					(number "176")
				)
				(pin passive line
					(at 0 -132.08 0)
					(length 3.81)
					(name "177")
					(number "177")
				)
				(pin passive line
					(at 22.86 -132.08 180)
					(length 3.81)
					(name "178")
					(number "178")
				)
				(pin passive line
					(at 0 -134.62 0)
					(length 3.81)
					(name "179")
					(number "179")
				)
				(pin passive line
					(at 22.86 -134.62 180)
					(length 3.81)
					(name "180")
					(number "180")
				)
				(pin passive line
					(at 0 -137.16 0)
					(length 3.81)
					(name "181")
					(number "181")
				)
				(pin passive line
					(at 22.86 -137.16 180)
					(length 3.81)
					(name "182")
					(number "182")
				)
				(pin passive line
					(at 0 -139.7 0)
					(length 3.81)
					(name "183")
					(number "183")
				)
				(pin passive line
					(at 22.86 -139.7 180)
					(length 3.81)
					(name "184")
					(number "184")
				)
				(pin passive line
					(at 0 -142.24 0)
					(length 3.81)
					(name "185")
					(number "185")
				)
				(pin passive line
					(at 22.86 -142.24 180)
					(length 3.81)
					(name "186")
					(number "186")
				)
				(pin passive line
					(at 0 -144.78 0)
					(length 3.81)
					(name "187")
					(number "187")
				)
				(pin passive line
					(at 22.86 -144.78 180)
					(length 3.81)
					(name "188")
					(number "188")
				)
				(pin passive line
					(at 0 -147.32 0)
					(length 3.81)
					(name "189")
					(number "189")
				)
				(pin passive line
					(at 22.86 -147.32 180)
					(length 3.81)
					(name "190")
					(number "190")
				)
				(pin passive line
					(at 0 -149.86 0)
					(length 3.81)
					(name "191")
					(number "191")
				)
				(pin passive line
					(at 22.86 -149.86 180)
					(length 3.81)
					(name "192")
					(number "192")
				)
				(pin passive line
					(at 0 -152.4 0)
					(length 3.81)
					(name "193")
					(number "193")
				)
				(pin passive line
					(at 22.86 -152.4 180)
					(length 3.81)
					(name "194")
					(number "194")
				)
				(pin passive line
					(at 0 -154.94 0)
					(length 3.81)
					(name "195")
					(number "195")
				)
				(pin passive line
					(at 22.86 -154.94 180)
					(length 3.81)
					(name "196")
					(number "196")
				)
				(pin passive line
					(at 0 -157.48 0)
					(length 3.81)
					(name "197")
					(number "197")
				)
				(pin passive line
					(at 22.86 -157.48 180)
					(length 3.81)
					(name "198")
					(number "198")
				)
				(pin passive line
					(at 0 -160.02 0)
					(length 3.81)
					(name "199")
					(number "199")
				)
				(pin passive line
					(at 22.86 -160.02 180)
					(length 3.81)
					(name "200")
					(number "200")
				)
				(pin passive line
					(at 0 -162.56 0)
					(length 3.81)
					(name "201")
					(number "201")
				)
				(pin passive line
					(at 22.86 -162.56 180)
					(length 3.81)
					(name "202")
					(number "202")
				)
				(pin passive line
					(at 0 -165.1 0)
					(length 3.81)
					(name "203")
					(number "203")
				)
				(pin passive line
					(at 22.86 -165.1 180)
					(length 3.81)
					(name "204")
					(number "204")
				)
			)
			(embedded_fonts no)
		)
)
