(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Bus_SDRAM_SODIMM_TE_390112-1"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Bus_SDRAM_SODIMM_TE_390112-1"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Bus_SDRAM_SODIMM_TE_390112-1"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.te.com/en/product-390112-1.html"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Small Outline (SO), 5.6 mm [.22 in] Stack Height, Right Angle Module Orientation, 144 Position, AMP-METRIMATE, SO DIMM Sockets"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "390112-1"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "TE Connectivity"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "SDRAM, CONNECTOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Bus_SDRAM_SODIMM_TE_390112-1_1_1"
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(name "VSS")
					(number "1")
				)
				(pin passive line
					(at 22.86 -25.4 180)
					(length 3.81)
					(name "VSS")
					(number "2")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "VDD")
					(number "11")
				)
				(pin passive line
					(at 22.86 0 180)
					(length 3.81)
					(name "VDD")
					(number "12")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(name "VSS")
					(number "21")
				)
				(pin passive line
					(at 22.86 -27.94 180)
					(length 3.81)
					(name "VSS")
					(number "22")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "VDD")
					(number "27")
				)
				(pin passive line
					(at 22.86 -2.54 180)
					(length 3.81)
					(name "VDD")
					(number "28")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(name "VSS")
					(number "35")
				)
				(pin passive line
					(at 22.86 -30.48 180)
					(length 3.81)
					(name "VSS")
					(number "36")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "VDD")
					(number "45")
				)
				(pin passive line
					(at 22.86 -5.08 180)
					(length 3.81)
					(name "VDD")
					(number "46")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(name "VSS")
					(number "55")
				)
				(pin passive line
					(at 22.86 -33.02 180)
					(length 3.81)
					(name "VSS")
					(number "56")
				)
				(pin no_connect line
					(at 19.05 -50.8 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "57")
				)
				(pin no_connect line
					(at 19.05 -50.8 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "58")
				)
				(pin no_connect line
					(at 19.05 -50.8 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "59")
				)
				(pin no_connect line
					(at 19.05 -50.8 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "60")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "VDD")
					(number "63")
				)
				(pin passive line
					(at 22.86 -7.62 180)
					(length 3.81)
					(name "VDD")
					(number "64")
				)
				(pin no_connect line
					(at 19.05 -50.8 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "73")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 3.81)
					(name "VSS")
					(number "75")
				)
				(pin passive line
					(at 22.86 -35.56 180)
					(length 3.81)
					(name "VSS")
					(number "76")
				)
				(pin no_connect line
					(at 19.05 -50.8 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "77")
				)
				(pin no_connect line
					(at 19.05 -50.8 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "78")
				)
				(pin no_connect line
					(at 19.05 -50.8 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "79")
				)
				(pin no_connect line
					(at 19.05 -50.8 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "80")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "VDD")
					(number "81")
				)
				(pin passive line
					(at 22.86 -10.16 180)
					(length 3.81)
					(name "VDD")
					(number "82")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 3.81)
					(name "VSS")
					(number "91")
				)
				(pin passive line
					(at 22.86 -38.1 180)
					(length 3.81)
					(name "VSS")
					(number "92")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "VDD")
					(number "101")
				)
				(pin passive line
					(at 22.86 -12.7 180)
					(length 3.81)
					(name "VDD")
					(number "102")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(name "VSS")
					(number "107")
				)
				(pin passive line
					(at 22.86 -40.64 180)
					(length 3.81)
					(name "VSS")
					(number "108")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "VDD")
					(number "113")
				)
				(pin passive line
					(at 22.86 -15.24 180)
					(length 3.81)
					(name "VDD")
					(number "114")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 3.81)
					(name "VSS")
					(number "119")
				)
				(pin passive line
					(at 22.86 -43.18 180)
					(length 3.81)
					(name "VSS")
					(number "120")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 3.81)
					(name "VDD")
					(number "129")
				)
				(pin passive line
					(at 22.86 -17.78 180)
					(length 3.81)
					(name "VDD")
					(number "130")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 3.81)
					(name "VSS")
					(number "139")
				)
				(pin passive line
					(at 22.86 -45.72 180)
					(length 3.81)
					(name "VSS")
					(number "140")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(name "VDD")
					(number "143")
				)
				(pin passive line
					(at 22.86 -20.32 180)
					(length 3.81)
					(name "VDD")
					(number "144")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "SHIELD")
					(number "SH")
				)
			)
			(symbol "Bus_SDRAM_SODIMM_TE_390112-1_2_1"
				(pin passive line
					(at 0 -22.86 0)
					(length 3.81)
					(name "A0")
					(number "29")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(name "A3")
					(number "30")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(name "A1")
					(number "31")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(name "A4")
					(number "32")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(name "A2")
					(number "33")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 3.81)
					(name "A5")
					(number "34")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 3.81)
					(name "CK0")
					(number "61")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 3.81)
					(name "CKE0")
					(number "62")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "RAS#")
					(number "65")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "CAS#")
					(number "66")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 3.81)
					(name "WE#")
					(number "67")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 3.81)
					(name "CKE1")
					(number "68")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "S0#")
					(number "69")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 3.81)
					(name "A12")
					(number "70")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "S1#")
					(number "71")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(name "A13")
					(number "72")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 3.81)
					(name "CK1")
					(number "74")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 3.81)
					(name "A6")
					(number "103")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(name "A7")
					(number "104")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 3.81)
					(name "A8")
					(number "105")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 3.81)
					(name "BA0")
					(number "106")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 3.81)
					(name "A9")
					(number "109")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 3.81)
					(name "BA1")
					(number "110")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 3.81)
					(name "A10")
					(number "111")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "A11")
					(number "112")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "SDA")
					(number "141")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "SCL")
					(number "142")
				)
			)
			(symbol "Bus_SDRAM_SODIMM_TE_390112-1_3_1"
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "DQ0")
					(number "3")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "DQ1")
					(number "5")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "DQ2")
					(number "7")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "DQ3")
					(number "9")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "DQ4")
					(number "13")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "DQ5")
					(number "15")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "DQ6")
					(number "17")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 3.81)
					(name "DQ7")
					(number "19")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 3.81)
					(name "DQMB0")
					(number "23")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 3.81)
					(name "DQMB1")
					(number "25")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(name "DQ8")
					(number "37")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 3.81)
					(name "DQ9")
					(number "39")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(name "DQ10")
					(number "41")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(name "DQ11")
					(number "43")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(name "DQ12")
					(number "47")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(name "DQ13")
					(number "49")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 3.81)
					(name "DQ14")
					(number "51")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 3.81)
					(name "DQ15")
					(number "53")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(name "DQ16")
					(number "83")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 3.81)
					(name "DQ17")
					(number "85")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 3.81)
					(name "DQ18")
					(number "87")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 3.81)
					(name "DQ19")
					(number "89")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "DQ20")
					(number "93")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 3.81)
					(name "DQ21")
					(number "95")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(name "DQ22")
					(number "97")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "DQ23")
					(number "99")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 3.81)
					(name "DQMB2")
					(number "115")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 3.81)
					(name "DQMB3")
					(number "117")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 3.81)
					(name "DQ24")
					(number "121")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 3.81)
					(name "DQ25")
					(number "123")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "DQ26")
					(number "125")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 3.81)
					(name "DQ27")
					(number "127")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 3.81)
					(name "DQ28")
					(number "131")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 3.81)
					(name "DQ29")
					(number "133")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 3.81)
					(name "DQ30")
					(number "135")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 3.81)
					(name "DQ31")
					(number "137")
				)
			)
			(symbol "Bus_SDRAM_SODIMM_TE_390112-1_4_1"
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "DQ32")
					(number "4")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "DQ33")
					(number "6")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "DQ34")
					(number "8")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "DQ35")
					(number "10")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "DQ36")
					(number "14")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "DQ37")
					(number "16")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "DQ38")
					(number "18")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 3.81)
					(name "DQ39")
					(number "20")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 3.81)
					(name "DQMB4")
					(number "24")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 3.81)
					(name "DQMB5")
					(number "26")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(name "DQ40")
					(number "38")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 3.81)
					(name "DQ41")
					(number "40")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(name "DQ42")
					(number "42")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(name "DQ43")
					(number "44")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(name "DQ44")
					(number "48")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(name "DQ45")
					(number "50")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 3.81)
					(name "DQ46")
					(number "52")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 3.81)
					(name "DQ47")
					(number "54")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(name "DQ48")
					(number "84")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 3.81)
					(name "DQ49")
					(number "86")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 3.81)
					(name "DQ50")
					(number "88")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 3.81)
					(name "DQ51")
					(number "90")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "DQ52")
					(number "94")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 3.81)
					(name "DQ53")
					(number "96")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(name "DQ54")
					(number "98")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "DQ55")
					(number "100")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 3.81)
					(name "DQMB6")
					(number "116")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 3.81)
					(name "DQMB7")
					(number "118")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 3.81)
					(name "DQ56")
					(number "122")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 3.81)
					(name "DQ57")
					(number "124")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "DQ58")
					(number "126")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 3.81)
					(name "DQ59")
					(number "128")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 3.81)
					(name "DQ60")
					(number "132")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 3.81)
					(name "DQ61")
					(number "134")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 3.81)
					(name "DQ62")
					(number "136")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 3.81)
					(name "DQ63")
					(number "138")
				)
			)
			(embedded_fonts no)
		)
)
