(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MicroSD_5025700893"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 38.1 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MicroSD_5025700893"
				(at 38.1 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MicroSD_5025700893"
				(at 38.1 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.molex.com/content/dam/molex/molex-dot-com/products/automated/en-us/salesdrawingpdf/502/502570/5025700893_sd.pdf?inline"
				(at 38.1 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Memory Card Connector, MicroSD, Push-Pull, 8 Contacts"
				(at 38.1 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "5025700893"
				(at 38.1 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Molex"
				(at 38.1 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 38.1 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "HORIZONTAL, SMT, MEMORY, CONNECTOR, MICRO, No-RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MicroSD_5025700893_1_1"
				(text "microSD CARD"
					(at 19.05 -12.7 900)
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 2.54)
					(name "DAT2")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 2.54)
					(name "CD/DAT3")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "CMD")
					(number "3")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VDD")
					(number "4")
				)
				(pin output line
					(at 0 -10.16 0)
					(length 2.54)
					(name "CLK")
					(number "5")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 2.54)
					(name "VSS")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "DAT0")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "DAT1")
					(number "8")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "CD1")
					(number "9")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 2.54)
					(name "CD2")
					(number "10")
				)
				(pin passive line
					(at 21.59 -22.86 180)
					(length 2.54)
					(name "Shell")
					(number "SH")
				)
			)
			(embedded_fonts no)
		)
)
