(footprint "MicroSD_Wurth_693071020811"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "SMT MICRO SD CARD CONNECTOR")
	(property "Reference" "REF**"
		(at 0 -9 0)
		(layer "F.SilkS")
	)
	(property "Value" "MicroSD_Wurth_693071020811"
		(at 0 8.9 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Author: Antmicro"
		(at -9.1 13.501 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -9.1 14.701 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -9.1 15.901 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -4.95 3.485)
		(size 1 1)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole oval
		(at 3.05 3.485)
		(size 1.7 1)
		(drill oval 1.7 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd rect
		(at 2.25 -7.57)
		(size 0.7 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 1.15 -7.57)
		(size 0.7 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 0.05 -7.57)
		(size 0.7 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.05 -7.57)
		(size 0.7 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -2.15 -7.57)
		(size 0.7 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -3.25 -7.57)
		(size 0.7 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -4.35 -7.57)
		(size 0.7 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -5.45 -7.57)
		(size 0.7 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -6.55 -7.57)
		(size 0.7 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at -8.1 -6.515)
		(size 1.7 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at -7.85 3.08)
		(size 1.4 2.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at 7.4 -6.515)
		(size 1.7 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at 7.85 3.08)
		(size 1.4 2.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_693071020811.glb"
		(offset
			(xyz 0.001 -0.964 0.9)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 0 0)
		)
	)
)
