(footprint "Bus_DDR4_DIMM_TE_9-2199155-6"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -4.3 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Bus_DDR4_DIMM_TE_9-2199155-6"
		(at 0 5 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "In1.Cu")
		(layer "In2.Cu")
		(layer "In3.Cu")
		(layer "In4.Cu")
		(layer "In5.Cu")
		(layer "In6.Cu")
		(layer "In7.Cu")
		(layer "In8.Cu")
		(layer "In9.Cu")
		(layer "In10.Cu")
		(layer "In11.Cu")
		(layer "In12.Cu")
		(layer "In13.Cu")
		(layer "In14.Cu")
		(layer "In15.Cu")
		(layer "In16.Cu")
		(layer "In17.Cu")
		(layer "In18.Cu")
		(layer "User.1")
		(layer "In19.Cu")
		(layer "User.2")
		(layer "In20.Cu")
		(layer "User.3")
		(layer "In21.Cu")
		(layer "User.4")
		(layer "In22.Cu")
		(layer "User.5")
		(layer "In23.Cu")
		(layer "User.6")
		(layer "In24.Cu")
		(layer "User.7")
		(layer "In25.Cu")
		(layer "User.8")
		(layer "In26.Cu")
		(layer "User.9")
		(layer "In27.Cu")
		(layer "In28.Cu")
		(layer "In29.Cu")
		(layer "In30.Cu")
		(layer "In31.Cu")
		(layer "In32.Cu")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -74.65 6.9 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -74.65 8.1 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -74.65 9.3 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -63.315 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "2" smd rect
		(at -62.465 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "3" smd rect
		(at -61.615 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "4" smd rect
		(at -60.765 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "5" smd rect
		(at -59.915 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "6" smd rect
		(at -59.065 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "7" smd rect
		(at -58.215 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "8" smd rect
		(at -57.365 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "9" smd rect
		(at -56.515 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "10" smd rect
		(at -55.665 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "11" smd rect
		(at -54.815 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "12" smd rect
		(at -53.965 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "13" smd rect
		(at -53.115 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "14" smd rect
		(at -52.265 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "15" smd rect
		(at -51.415 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "16" smd rect
		(at -50.565 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "17" smd rect
		(at -49.715 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "18" smd rect
		(at -48.865 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "19" smd rect
		(at -48.015 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "20" smd rect
		(at -47.165 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "21" smd rect
		(at -46.315 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "22" smd rect
		(at -45.465 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "23" smd rect
		(at -44.615 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "24" smd rect
		(at -43.765 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "25" smd rect
		(at -42.915 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "26" smd rect
		(at -42.065 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "27" smd rect
		(at -41.215 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "28" smd rect
		(at -40.365 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "29" smd rect
		(at -39.515 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "30" smd rect
		(at -38.665 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "31" smd rect
		(at -37.815 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "32" smd rect
		(at -36.965 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "33" smd rect
		(at -36.115 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "34" smd rect
		(at -35.265 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "35" smd rect
		(at -34.415 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "36" smd rect
		(at -33.565 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "37" smd rect
		(at -32.715 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "38" smd rect
		(at -31.865 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "39" smd rect
		(at -31.015 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "40" smd rect
		(at -30.165 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "41" smd rect
		(at -29.315 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "42" smd rect
		(at -28.465 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "43" smd rect
		(at -27.615 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "44" smd rect
		(at -26.765 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "45" smd rect
		(at -25.915 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "46" smd rect
		(at -25.065 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "47" smd rect
		(at -24.215 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "48" smd rect
		(at -23.365 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "49" smd rect
		(at -22.515 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "50" smd rect
		(at -21.665 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "51" smd rect
		(at -20.815 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "52" smd rect
		(at -19.965 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "53" smd rect
		(at -19.115 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "54" smd rect
		(at -18.265 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "55" smd rect
		(at -17.415 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "56" smd rect
		(at -16.565 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "57" smd rect
		(at -15.715 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "58" smd rect
		(at -14.865 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "59" smd rect
		(at -14.015 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "60" smd rect
		(at -13.165 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "61" smd rect
		(at -12.315 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "62" smd rect
		(at -11.465 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "63" smd rect
		(at -10.615 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "64" smd rect
		(at -9.765 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "65" smd rect
		(at -8.915 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "66" smd rect
		(at -8.065 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "67" smd rect
		(at -7.215 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "68" smd rect
		(at -6.365 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "69" smd rect
		(at -5.515 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "70" smd rect
		(at -4.665 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "71" smd rect
		(at -3.815 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "72" smd rect
		(at -2.965 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "73" smd rect
		(at -2.115 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "74" smd rect
		(at -1.265 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "75" smd rect
		(at -0.415 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "76" smd rect
		(at 0.435 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "77" smd rect
		(at 1.285 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "78" smd rect
		(at 7.235 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "79" smd rect
		(at 8.085 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "80" smd rect
		(at 8.935 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "81" smd rect
		(at 9.785 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "82" smd rect
		(at 10.635 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "83" smd rect
		(at 11.485 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "84" smd rect
		(at 12.335 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "85" smd rect
		(at 13.185 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "86" smd rect
		(at 14.035 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "87" smd rect
		(at 14.885 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "88" smd rect
		(at 15.735 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "89" smd rect
		(at 16.585 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "90" smd rect
		(at 17.435 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "91" smd rect
		(at 18.285 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "92" smd rect
		(at 19.135 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "93" smd rect
		(at 19.985 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "94" smd rect
		(at 20.835 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "95" smd rect
		(at 21.685 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "96" smd rect
		(at 22.535 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "97" smd rect
		(at 23.385 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "98" smd rect
		(at 24.235 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "99" smd rect
		(at 25.085 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "100" smd rect
		(at 25.935 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "101" smd rect
		(at 26.785 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "102" smd rect
		(at 27.635 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "103" smd rect
		(at 28.485 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "104" smd rect
		(at 29.335 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "105" smd rect
		(at 30.185 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "106" smd rect
		(at 31.035 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "107" smd rect
		(at 31.885 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "108" smd rect
		(at 32.735 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "109" smd rect
		(at 33.585 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "110" smd rect
		(at 34.435 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "111" smd rect
		(at 35.285 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "112" smd rect
		(at 36.135 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "113" smd rect
		(at 36.985 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "114" smd rect
		(at 37.835 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "115" smd rect
		(at 38.685 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "116" smd rect
		(at 39.535 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "117" smd rect
		(at 40.385 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "118" smd rect
		(at 41.235 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "119" smd rect
		(at 42.085 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "120" smd rect
		(at 42.935 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "121" smd rect
		(at 43.785 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "122" smd rect
		(at 44.635 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "123" smd rect
		(at 45.485 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "124" smd rect
		(at 46.335 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "125" smd rect
		(at 47.185 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "126" smd rect
		(at 48.035 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "127" smd rect
		(at 48.885 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "128" smd rect
		(at 49.735 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "129" smd rect
		(at 50.585 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "130" smd rect
		(at 51.435 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "131" smd rect
		(at 52.285 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "132" smd rect
		(at 53.135 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "133" smd rect
		(at 53.985 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "134" smd rect
		(at 54.835 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "135" smd rect
		(at 55.685 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "136" smd rect
		(at 56.535 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "137" smd rect
		(at 57.385 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "138" smd rect
		(at 58.235 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "139" smd rect
		(at 59.085 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "140" smd rect
		(at 59.935 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "141" smd rect
		(at 60.785 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "142" smd rect
		(at 61.635 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "143" smd rect
		(at 62.485 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "144" smd rect
		(at 63.335 2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "145" smd rect
		(at -63.315 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "146" smd rect
		(at -62.465 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "147" smd rect
		(at -61.615 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "148" smd rect
		(at -60.765 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "149" smd rect
		(at -59.915 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "150" smd rect
		(at -59.065 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "151" smd rect
		(at -58.215 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "152" smd rect
		(at -57.365 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "153" smd rect
		(at -56.515 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "154" smd rect
		(at -55.665 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "155" smd rect
		(at -54.815 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "156" smd rect
		(at -53.965 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "157" smd rect
		(at -53.115 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "158" smd rect
		(at -52.265 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "159" smd rect
		(at -51.415 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "160" smd rect
		(at -50.565 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "161" smd rect
		(at -49.715 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "162" smd rect
		(at -48.865 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "163" smd rect
		(at -48.015 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "164" smd rect
		(at -47.165 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "165" smd rect
		(at -46.315 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "166" smd rect
		(at -45.465 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "167" smd rect
		(at -44.615 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "168" smd rect
		(at -43.765 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "169" smd rect
		(at -42.915 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "170" smd rect
		(at -42.065 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "171" smd rect
		(at -41.215 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "172" smd rect
		(at -40.365 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "173" smd rect
		(at -39.515 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "174" smd rect
		(at -38.665 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "175" smd rect
		(at -37.815 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "176" smd rect
		(at -36.965 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "177" smd rect
		(at -36.115 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "178" smd rect
		(at -35.265 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "179" smd rect
		(at -34.415 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "180" smd rect
		(at -33.565 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "181" smd rect
		(at -32.715 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "182" smd rect
		(at -31.865 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "183" smd rect
		(at -31.015 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "184" smd rect
		(at -30.165 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "185" smd rect
		(at -29.315 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "186" smd rect
		(at -28.465 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "187" smd rect
		(at -27.615 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "188" smd rect
		(at -26.765 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "189" smd rect
		(at -25.915 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "190" smd rect
		(at -25.065 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "191" smd rect
		(at -24.215 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "192" smd rect
		(at -23.365 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "193" smd rect
		(at -22.515 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "194" smd rect
		(at -21.665 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "195" smd rect
		(at -20.815 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "196" smd rect
		(at -19.965 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "197" smd rect
		(at -19.115 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "198" smd rect
		(at -18.265 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "199" smd rect
		(at -17.415 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "200" smd rect
		(at -16.565 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "201" smd rect
		(at -15.715 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "202" smd rect
		(at -14.865 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "203" smd rect
		(at -14.015 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "204" smd rect
		(at -13.165 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "205" smd rect
		(at -12.315 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "206" smd rect
		(at -11.465 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "207" smd rect
		(at -10.615 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "208" smd rect
		(at -9.765 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "209" smd rect
		(at -8.915 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "210" smd rect
		(at -8.065 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "211" smd rect
		(at -7.215 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "212" smd rect
		(at -6.365 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "213" smd rect
		(at -5.515 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "214" smd rect
		(at -4.665 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "215" smd rect
		(at -3.815 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "216" smd rect
		(at -2.965 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "217" smd rect
		(at -2.115 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "218" smd rect
		(at -1.265 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "219" smd rect
		(at -0.415 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "220" smd rect
		(at 0.435 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "221" smd rect
		(at 1.285 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "222" smd rect
		(at 7.235 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "223" smd rect
		(at 8.085 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "224" smd rect
		(at 8.935 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "225" smd rect
		(at 9.785 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "226" smd rect
		(at 10.635 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "227" smd rect
		(at 11.485 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "228" smd rect
		(at 12.335 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "229" smd rect
		(at 13.185 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "230" smd rect
		(at 14.035 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "231" smd rect
		(at 14.885 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "232" smd rect
		(at 15.735 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "233" smd rect
		(at 16.585 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "234" smd rect
		(at 17.435 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "235" smd rect
		(at 18.285 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "236" smd rect
		(at 19.135 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "237" smd rect
		(at 19.985 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "238" smd rect
		(at 20.835 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "239" smd rect
		(at 21.685 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "240" smd rect
		(at 22.535 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "241" smd rect
		(at 23.385 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "242" smd rect
		(at 24.235 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "243" smd rect
		(at 25.085 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "244" smd rect
		(at 25.935 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "245" smd rect
		(at 26.785 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "246" smd rect
		(at 27.635 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "247" smd rect
		(at 28.485 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "248" smd rect
		(at 29.335 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "249" smd rect
		(at 30.185 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "250" smd rect
		(at 31.035 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "251" smd rect
		(at 31.885 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "252" smd rect
		(at 32.735 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "253" smd rect
		(at 33.585 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "254" smd rect
		(at 34.435 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "255" smd rect
		(at 35.285 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "256" smd rect
		(at 36.135 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "257" smd rect
		(at 36.985 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "258" smd rect
		(at 37.835 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "259" smd rect
		(at 38.685 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "260" smd rect
		(at 39.535 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "261" smd rect
		(at 40.385 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "262" smd rect
		(at 41.235 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "263" smd rect
		(at 42.085 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "264" smd rect
		(at 42.935 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "265" smd rect
		(at 43.785 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "266" smd rect
		(at 44.635 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "267" smd rect
		(at 45.485 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "268" smd rect
		(at 46.335 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "269" smd rect
		(at 47.185 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "270" smd rect
		(at 48.035 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "271" smd rect
		(at 48.885 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "272" smd rect
		(at 49.735 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "273" smd rect
		(at 50.585 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "274" smd rect
		(at 51.435 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "275" smd rect
		(at 52.285 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "276" smd rect
		(at 53.135 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "277" smd rect
		(at 53.985 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "278" smd rect
		(at 54.835 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "279" smd rect
		(at 55.685 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "280" smd rect
		(at 56.535 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "281" smd rect
		(at 57.385 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "282" smd rect
		(at 58.235 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "283" smd rect
		(at 59.085 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "284" smd rect
		(at 59.935 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "285" smd rect
		(at 60.785 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "286" smd rect
		(at 61.635 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "287" smd rect
		(at 62.485 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "288" smd rect
		(at 63.335 -2.3)
		(size 0.57 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "MP" thru_hole oval
		(at -68.965 0)
		(size 1.8 3.05)
		(drill oval 1.2 2.45)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.076)
	)
	(pad "MP" thru_hole oval
		(at 5.585 0)
		(size 1.8 3.05)
		(drill oval 1.2 2.45)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.076)
	)
	(pad "MP" thru_hole oval
		(at 68.985 0)
		(size 1.8 3.05)
		(drill oval 1.2 2.45)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.076)
	)
	(embedded_fonts no)
	(model "antmicro_9_2199155_6.glb"
		(offset
			(xyz 0 0 6.15)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
