(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Bus_DDR4_9-2199155-6"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 49.53 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Bus_DDR4_9-2199155-6"
				(at 49.53 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Bus_DDR4_9-2199155-6"
				(at 49.53 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.te.com/usa-en/product-9-2199155-6.datasheet.pdf"
				(at 49.53 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "288 Position DIMM DDR4 SDRAM Socket Surface Mount"
				(at 49.53 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "9-2199155-6"
				(at 49.53 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "TE Connectivity"
				(at 49.53 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 49.53 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 49.53 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "SMT, MEMORY, IC, DDR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Bus_DDR4_9-2199155-6_1_1"
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "DQ4")
					(number "3")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "DQ0")
					(number "5")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(name "DQS9_t")
					(number "7")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(name "DQS9_c")
					(number "8")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "DQ6")
					(number "10")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "DQ2")
					(number "12")
				)
				(pin passive line
					(at 0 -41.91 0)
					(length 3.81)
					(name "DQ12")
					(number "14")
				)
				(pin passive line
					(at 0 -31.75 0)
					(length 3.81)
					(name "DQ8")
					(number "16")
				)
				(pin passive line
					(at 0 -57.15 0)
					(length 3.81)
					(name "DQS10_t")
					(number "18")
				)
				(pin passive line
					(at 0 -59.69 0)
					(length 3.81)
					(name "DQS10_c")
					(number "19")
				)
				(pin passive line
					(at 0 -46.99 0)
					(length 3.81)
					(name "DQ14")
					(number "21")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 3.81)
					(name "DQ10")
					(number "23")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 3.81)
					(name "DQ20")
					(number "25")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 3.81)
					(name "DQ16")
					(number "27")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 3.81)
					(name "DQS11_t")
					(number "29")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 3.81)
					(name "DQS11_c")
					(number "30")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 3.81)
					(name "DQ22")
					(number "32")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 3.81)
					(name "DQ18")
					(number "34")
				)
				(pin passive line
					(at 0 -105.41 0)
					(length 3.81)
					(name "DQ28")
					(number "36")
				)
				(pin passive line
					(at 0 -95.25 0)
					(length 3.81)
					(name "DQ24")
					(number "38")
				)
				(pin passive line
					(at 0 -120.65 0)
					(length 3.81)
					(name "DQS12_t")
					(number "40")
				)
				(pin passive line
					(at 0 -123.19 0)
					(length 3.81)
					(name "DQS12_c")
					(number "41")
				)
				(pin passive line
					(at 0 -110.49 0)
					(length 3.81)
					(name "DQ30")
					(number "43")
				)
				(pin passive line
					(at 0 -100.33 0)
					(length 3.81)
					(name "DQ26")
					(number "45")
				)
				(pin passive line
					(at 0 -137.16 0)
					(length 3.81)
					(name "CB4")
					(number "47")
				)
				(pin passive line
					(at 0 -127 0)
					(length 3.81)
					(name "CB0")
					(number "49")
				)
				(pin passive line
					(at 0 -152.4 0)
					(length 3.81)
					(name "DQS17_t")
					(number "51")
				)
				(pin passive line
					(at 0 -154.94 0)
					(length 3.81)
					(name "DQS17_c")
					(number "52")
				)
				(pin passive line
					(at 0 -142.24 0)
					(length 3.81)
					(name "CB6")
					(number "54")
				)
				(pin passive line
					(at 0 -132.08 0)
					(length 3.81)
					(name "CB2")
					(number "56")
				)
				(pin passive line
					(at 30.48 -10.16 180)
					(length 3.81)
					(name "DQ36")
					(number "95")
				)
				(pin passive line
					(at 30.48 0 180)
					(length 3.81)
					(name "DQ32")
					(number "97")
				)
				(pin passive line
					(at 30.48 -25.4 180)
					(length 3.81)
					(name "DQS13_t")
					(number "99")
				)
				(pin passive line
					(at 30.48 -27.94 180)
					(length 3.81)
					(name "DQS13_c")
					(number "100")
				)
				(pin passive line
					(at 30.48 -15.24 180)
					(length 3.81)
					(name "DQ38")
					(number "102")
				)
				(pin passive line
					(at 30.48 -5.08 180)
					(length 3.81)
					(name "DQ34")
					(number "104")
				)
				(pin passive line
					(at 30.48 -41.91 180)
					(length 3.81)
					(name "DQ44")
					(number "106")
				)
				(pin passive line
					(at 30.48 -31.75 180)
					(length 3.81)
					(name "DQ40")
					(number "108")
				)
				(pin passive line
					(at 30.48 -57.15 180)
					(length 3.81)
					(name "DQS14_t")
					(number "110")
				)
				(pin passive line
					(at 30.48 -59.69 180)
					(length 3.81)
					(name "DQS14_c")
					(number "111")
				)
				(pin passive line
					(at 30.48 -46.99 180)
					(length 3.81)
					(name "DQ46")
					(number "113")
				)
				(pin passive line
					(at 30.48 -36.83 180)
					(length 3.81)
					(name "DQ42")
					(number "115")
				)
				(pin passive line
					(at 30.48 -73.66 180)
					(length 3.81)
					(name "DQ52")
					(number "117")
				)
				(pin passive line
					(at 30.48 -63.5 180)
					(length 3.81)
					(name "DQ48")
					(number "119")
				)
				(pin passive line
					(at 30.48 -88.9 180)
					(length 3.81)
					(name "DQS15_t")
					(number "121")
				)
				(pin passive line
					(at 30.48 -91.44 180)
					(length 3.81)
					(name "DQS15_c")
					(number "122")
				)
				(pin passive line
					(at 30.48 -78.74 180)
					(length 3.81)
					(name "DQ54")
					(number "124")
				)
				(pin passive line
					(at 30.48 -68.58 180)
					(length 3.81)
					(name "DQ50")
					(number "126")
				)
				(pin passive line
					(at 30.48 -105.41 180)
					(length 3.81)
					(name "DQ60")
					(number "128")
				)
				(pin passive line
					(at 30.48 -95.25 180)
					(length 3.81)
					(name "DQ56")
					(number "130")
				)
				(pin passive line
					(at 30.48 -120.65 180)
					(length 3.81)
					(name "DQS16_t")
					(number "132")
				)
				(pin passive line
					(at 30.48 -123.19 180)
					(length 3.81)
					(name "DQS16_c")
					(number "133")
				)
				(pin passive line
					(at 30.48 -110.49 180)
					(length 3.81)
					(name "DQ62")
					(number "135")
				)
				(pin passive line
					(at 30.48 -100.33 180)
					(length 3.81)
					(name "DQ58")
					(number "137")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "DQ5")
					(number "148")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "DQ1")
					(number "150")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 3.81)
					(name "DQS0_c")
					(number "152")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(name "DQS0_t")
					(number "153")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 3.81)
					(name "DQ7")
					(number "155")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "DQ3")
					(number "157")
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 3.81)
					(name "DQ13")
					(number "159")
				)
				(pin passive line
					(at 0 -34.29 0)
					(length 3.81)
					(name "DQ9")
					(number "161")
				)
				(pin passive line
					(at 0 -54.61 0)
					(length 3.81)
					(name "DQS1_c")
					(number "163")
				)
				(pin passive line
					(at 0 -52.07 0)
					(length 3.81)
					(name "DQS_1_t")
					(number "164")
				)
				(pin passive line
					(at 0 -49.53 0)
					(length 3.81)
					(name "DQ15")
					(number "166")
				)
				(pin passive line
					(at 0 -39.37 0)
					(length 3.81)
					(name "DQ11")
					(number "168")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 3.81)
					(name "DQ21")
					(number "170")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "DQ17")
					(number "172")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 3.81)
					(name "DQS2_c")
					(number "174")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 3.81)
					(name "DQS2_t")
					(number "175")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 3.81)
					(name "DQ23")
					(number "177")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 3.81)
					(name "DQ19")
					(number "179")
				)
				(pin passive line
					(at 0 -107.95 0)
					(length 3.81)
					(name "DQ29")
					(number "181")
				)
				(pin passive line
					(at 0 -97.79 0)
					(length 3.81)
					(name "DQ25")
					(number "183")
				)
				(pin passive line
					(at 0 -118.11 0)
					(length 3.81)
					(name "DQS3_c")
					(number "185")
				)
				(pin passive line
					(at 0 -115.57 0)
					(length 3.81)
					(name "DQS3_t")
					(number "186")
				)
				(pin passive line
					(at 0 -113.03 0)
					(length 3.81)
					(name "DQ31")
					(number "188")
				)
				(pin passive line
					(at 0 -102.87 0)
					(length 3.81)
					(name "DQ27")
					(number "190")
				)
				(pin passive line
					(at 0 -139.7 0)
					(length 3.81)
					(name "CB5")
					(number "192")
				)
				(pin passive line
					(at 0 -129.54 0)
					(length 3.81)
					(name "CB1")
					(number "194")
				)
				(pin passive line
					(at 0 -149.86 0)
					(length 3.81)
					(name "DQS8_c")
					(number "196")
				)
				(pin passive line
					(at 0 -147.32 0)
					(length 3.81)
					(name "DQS8_t")
					(number "197")
				)
				(pin passive line
					(at 0 -144.78 0)
					(length 3.81)
					(name "CB7")
					(number "199")
				)
				(pin passive line
					(at 0 -134.62 0)
					(length 3.81)
					(name "CB3")
					(number "201")
				)
				(pin passive line
					(at 30.48 -12.7 180)
					(length 3.81)
					(name "DQ37")
					(number "240")
				)
				(pin passive line
					(at 30.48 -2.54 180)
					(length 3.81)
					(name "DQ33")
					(number "242")
				)
				(pin passive line
					(at 30.48 -22.86 180)
					(length 3.81)
					(name "DQS4_c")
					(number "244")
				)
				(pin passive line
					(at 30.48 -20.32 180)
					(length 3.81)
					(name "DQS4_t")
					(number "245")
				)
				(pin passive line
					(at 30.48 -17.78 180)
					(length 3.81)
					(name "DQ39")
					(number "247")
				)
				(pin passive line
					(at 30.48 -7.62 180)
					(length 3.81)
					(name "DQ35")
					(number "249")
				)
				(pin passive line
					(at 30.48 -44.45 180)
					(length 3.81)
					(name "DQ45")
					(number "251")
				)
				(pin passive line
					(at 30.48 -34.29 180)
					(length 3.81)
					(name "DQ41")
					(number "253")
				)
				(pin passive line
					(at 30.48 -54.61 180)
					(length 3.81)
					(name "DQS5_c")
					(number "255")
				)
				(pin passive line
					(at 30.48 -52.07 180)
					(length 3.81)
					(name "DQS5_t")
					(number "256")
				)
				(pin passive line
					(at 30.48 -49.53 180)
					(length 3.81)
					(name "DQ47")
					(number "258")
				)
				(pin passive line
					(at 30.48 -39.37 180)
					(length 3.81)
					(name "DQ43")
					(number "260")
				)
				(pin passive line
					(at 30.48 -76.2 180)
					(length 3.81)
					(name "DQ53")
					(number "262")
				)
				(pin passive line
					(at 30.48 -66.04 180)
					(length 3.81)
					(name "DQ49")
					(number "264")
				)
				(pin passive line
					(at 30.48 -86.36 180)
					(length 3.81)
					(name "DQS6_c")
					(number "266")
				)
				(pin passive line
					(at 30.48 -83.82 180)
					(length 3.81)
					(name "DQS6_t")
					(number "267")
				)
				(pin passive line
					(at 30.48 -81.28 180)
					(length 3.81)
					(name "DQ55")
					(number "269")
				)
				(pin passive line
					(at 30.48 -71.12 180)
					(length 3.81)
					(name "DQ51")
					(number "271")
				)
				(pin passive line
					(at 30.48 -107.95 180)
					(length 3.81)
					(name "DQ61")
					(number "273")
				)
				(pin passive line
					(at 30.48 -97.79 180)
					(length 3.81)
					(name "DQ57")
					(number "275")
				)
				(pin passive line
					(at 30.48 -118.11 180)
					(length 3.81)
					(name "DQS7_c")
					(number "277")
				)
				(pin passive line
					(at 30.48 -115.57 180)
					(length 3.81)
					(name "DQS7_t")
					(number "278")
				)
				(pin passive line
					(at 30.48 -113.03 180)
					(length 3.81)
					(name "DQ63")
					(number "280")
				)
				(pin passive line
					(at 30.48 -102.87 180)
					(length 3.81)
					(name "DQ59")
					(number "282")
				)
			)
			(symbol "Bus_DDR4_9-2199155-6_2_1"
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "12V/NC")
					(number "1")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "2")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "4")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "6")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "9")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "11")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "13")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "15")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "17")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "20")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "22")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "24")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "26")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "28")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "31")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "33")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "35")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "37")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "39")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "42")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "44")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "46")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "48")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "50")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "53")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "55")
				)
				(pin passive line
					(at 0 -62.23 0)
					(length 3.81)
					(name "Presence")
					(number "57")
				)
				(pin passive line
					(at 30.48 -22.86 180)
					(length 3.81)
					(name "RESET_n")
					(number "58")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "59")
				)
				(pin passive line
					(at 30.48 -12.7 180)
					(length 3.81)
					(name "CKE0")
					(number "60")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "61")
				)
				(pin passive line
					(at 30.48 -10.16 180)
					(length 3.81)
					(name "ACT_n")
					(number "62")
				)
				(pin passive line
					(at 30.48 -5.08 180)
					(length 3.81)
					(name "BG0")
					(number "63")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "64")
				)
				(pin passive line
					(at 0 -46.99 0)
					(length 3.81)
					(name "A12/BC_n")
					(number "65")
				)
				(pin passive line
					(at 0 -39.37 0)
					(length 3.81)
					(name "A9")
					(number "66")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "67")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 3.81)
					(name "A8")
					(number "68")
				)
				(pin passive line
					(at 0 -31.75 0)
					(length 3.81)
					(name "A6")
					(number "69")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "70")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 3.81)
					(name "A3")
					(number "71")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(name "A1")
					(number "72")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "73")
				)
				(pin passive line
					(at 30.48 -31.75 180)
					(length 3.81)
					(name "CK0_t")
					(number "74")
				)
				(pin passive line
					(at 30.48 -34.29 180)
					(length 3.81)
					(name "CK0_c")
					(number "75")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "76")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VTT")
					(number "77")
				)
				(pin passive line
					(at 30.48 -45.72 180)
					(length 3.81)
					(name "EVENT_n")
					(number "78")
				)
				(pin passive line
					(at 0 -16.51 0)
					(length 3.81)
					(name "A0")
					(number "79")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "80")
				)
				(pin passive line
					(at 30.48 0 180)
					(length 3.81)
					(name "BA0")
					(number "81")
				)
				(pin passive line
					(at 0 -57.15 0)
					(length 3.81)
					(name "RAS_n/A16")
					(number "82")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "83")
				)
				(pin passive line
					(at 30.48 -49.53 180)
					(length 3.81)
					(name "CS0_n")
					(number "84")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "85")
				)
				(pin passive line
					(at 0 -54.61 0)
					(length 3.81)
					(name "CAS_n/A15")
					(number "86")
				)
				(pin passive line
					(at 30.48 -17.78 180)
					(length 3.81)
					(name "ODT0")
					(number "87")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "88")
				)
				(pin passive line
					(at 30.48 -52.07 180)
					(length 3.81)
					(name "CS1_n")
					(number "89")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "90")
				)
				(pin passive line
					(at 30.48 -20.32 180)
					(length 3.81)
					(name "ODT1")
					(number "91")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "92")
				)
				(pin passive line
					(at 30.48 -54.61 180)
					(length 3.81)
					(name "C0/CS2_n")
					(number "93")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "94")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "96")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "98")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(name "VSS")
					(number "101")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "103")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "105")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "107")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "109")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "112")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "114")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "116")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "118")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "120")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "123")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "125")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "127")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "129")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "131")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "134")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "136")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "138")
				)
				(pin passive line
					(at 30.48 -63.5 180)
					(length 3.81)
					(name "SA0")
					(number "139")
				)
				(pin passive line
					(at 30.48 -66.04 180)
					(length 3.81)
					(name "SA1")
					(number "140")
				)
				(pin passive line
					(at 30.48 -74.93 180)
					(length 3.81)
					(name "SCL")
					(number "141")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "VPP")
					(number "142")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "VPP")
					(number "143")
				)
				(pin no_connect line
					(at 3.81 -64.77 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "144")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "12V/NC")
					(number "145")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "VREFCA")
					(number "146")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "147")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "149")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "151")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "154")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "156")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "158")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "160")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "162")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "165")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "167")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "169")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "171")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "173")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "176")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "178")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "180")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "182")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "184")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "187")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "189")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "191")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "193")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "195")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "198")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "200")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "202")
				)
				(pin passive line
					(at 30.48 -15.24 180)
					(length 3.81)
					(name "CKE1")
					(number "203")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "VDD")
					(number "204")
				)
				(pin no_connect line
					(at 3.81 -67.31 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "205")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "206")
				)
				(pin passive line
					(at 30.48 -7.62 180)
					(length 3.81)
					(name "BG1")
					(number "207")
				)
				(pin passive line
					(at 30.48 -27.94 180)
					(length 3.81)
					(name "ALERT_n")
					(number "208")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "209")
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 3.81)
					(name "A11")
					(number "210")
				)
				(pin passive line
					(at 0 -34.29 0)
					(length 3.81)
					(name "A7")
					(number "211")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "212")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 3.81)
					(name "A5")
					(number "213")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 3.81)
					(name "A4")
					(number "214")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "215")
				)
				(pin passive line
					(at 0 -21.59 0)
					(length 3.81)
					(name "A2")
					(number "216")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "217")
				)
				(pin passive line
					(at 30.48 -36.83 180)
					(length 3.81)
					(name "CK1_t")
					(number "218")
				)
				(pin passive line
					(at 30.48 -39.37 180)
					(length 3.81)
					(name "CK1_c")
					(number "219")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "220")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "VTT")
					(number "221")
				)
				(pin passive line
					(at 30.48 -25.4 180)
					(length 3.81)
					(name "PARITY")
					(number "222")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "223")
				)
				(pin passive line
					(at 30.48 -2.54 180)
					(length 3.81)
					(name "BA1")
					(number "224")
				)
				(pin passive line
					(at 0 -41.91 0)
					(length 3.81)
					(name "A10/AP")
					(number "225")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "226")
				)
				(pin no_connect line
					(at 3.81 -69.85 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "227")
				)
				(pin passive line
					(at 0 -52.07 0)
					(length 3.81)
					(name "WE_n/A14")
					(number "228")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "229")
				)
				(pin passive line
					(at 30.48 -43.18 180)
					(length 3.81)
					(name "SAVE_n")
					(number "230")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "231")
				)
				(pin passive line
					(at 0 -49.53 0)
					(length 3.81)
					(name "A13")
					(number "232")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "233")
				)
				(pin passive line
					(at 0 -59.69 0)
					(length 3.81)
					(name "NC/A17")
					(number "234")
				)
				(pin passive line
					(at 30.48 -59.69 180)
					(length 3.81)
					(name "NC/C2")
					(number "235")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "236")
				)
				(pin passive line
					(at 30.48 -57.15 180)
					(length 3.81)
					(name "CS3_n/C1")
					(number "237")
				)
				(pin passive line
					(at 30.48 -68.58 180)
					(length 3.81)
					(name "SA2")
					(number "238")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "239")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "241")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "243")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "246")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "248")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "250")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "252")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "254")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "257")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "259")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "261")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "263")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "265")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "268")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "270")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "272")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "274")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "276")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "279")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "281")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "283")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "VDDSPD")
					(number "284")
				)
				(pin passive line
					(at 30.48 -72.39 180)
					(length 3.81)
					(name "SDA")
					(number "285")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "VPP")
					(number "286")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "VPP")
					(number "287")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "VPP")
					(number "288")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 3.81)
					(name "MP")
					(number "MP")
				)
			)
			(embedded_fonts no)
		)
)
