(footprint "Bus_DDR5_Socket_Amphenol_DDR504111002KQ"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "DIMM Connectors DDR5 SMD 288P")
	(property "Reference" "REF**"
		(at 0 -3.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Bus_DDR5_Socket_Amphenol_DDR504111002KQ"
		(at 0 4.2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "In1.Cu")
		(layer "In2.Cu")
		(layer "In3.Cu")
		(layer "In4.Cu")
		(layer "In5.Cu")
		(layer "In6.Cu")
		(layer "In7.Cu")
		(layer "In8.Cu")
		(layer "In9.Cu")
		(layer "In10.Cu")
		(layer "In11.Cu")
		(layer "In12.Cu")
		(layer "In13.Cu")
		(layer "In14.Cu")
		(layer "In15.Cu")
		(layer "In16.Cu")
		(layer "In17.Cu")
		(layer "In18.Cu")
		(layer "User.1")
		(layer "In19.Cu")
		(layer "User.2")
		(layer "In20.Cu")
		(layer "User.3")
		(layer "In21.Cu")
		(layer "User.4")
		(layer "In22.Cu")
		(layer "User.5")
		(layer "In23.Cu")
		(layer "User.6")
		(layer "In24.Cu")
		(layer "User.7")
		(layer "In25.Cu")
		(layer "User.8")
		(layer "In26.Cu")
		(layer "User.9")
		(layer "In27.Cu")
		(layer "In28.Cu")
		(layer "In29.Cu")
		(layer "In30.Cu")
		(layer "In31.Cu")
		(layer "In32.Cu")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -76.25 5.5 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -76.25 6.7 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -76.25 7.901 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -63.326 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -62.476 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -61.625 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -60.775 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -59.926 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -59.076 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -58.226 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -57.375 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -56.525 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -55.676 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -54.826 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -53.976 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -53.125 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -52.275 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -51.426 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -50.576 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -49.726 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -48.875 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -48.025 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at -47.176 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at -46.326 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at -45.476 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at -44.625 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at -43.775 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at -42.926 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at -42.076 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at -41.226 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at -40.375 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at -39.525 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at -38.676 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at -37.826 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at -36.976 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at -36.125 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at -35.275 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at -34.426 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at -33.576 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at -32.726 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at -31.875 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at -31.026 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at -30.177 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd rect
		(at -29.325 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd rect
		(at -28.476 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd rect
		(at -27.625 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd rect
		(at -26.776 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "45" smd rect
		(at -25.927 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "46" smd rect
		(at -25.075 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "47" smd rect
		(at -24.226 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "48" smd rect
		(at -23.375 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "49" smd rect
		(at -22.526 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "50" smd rect
		(at -21.677 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "51" smd rect
		(at -20.825 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "52" smd rect
		(at -19.976 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "53" smd rect
		(at -19.125 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "54" smd rect
		(at -18.276 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "55" smd rect
		(at -17.427 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "56" smd rect
		(at -16.575 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "57" smd rect
		(at -15.725 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "58" smd rect
		(at -14.875 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "59" smd rect
		(at -14.026 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "60" smd rect
		(at -13.176 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "61" smd rect
		(at -12.326 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "62" smd rect
		(at -11.475 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "63" smd rect
		(at -10.625 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "64" smd rect
		(at -9.776 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "65" smd rect
		(at -8.926 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "66" smd rect
		(at -8.075 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "67" smd rect
		(at -7.226 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "68" smd rect
		(at -6.375 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "69" smd rect
		(at -5.526 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "70" smd rect
		(at -4.675 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "71" smd rect
		(at -3.826 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "72" smd rect
		(at -2.976 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "73" smd rect
		(at -2.125 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "74" smd rect
		(at -1.276 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "75" smd rect
		(at -0.425 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "76" smd rect
		(at 5.525 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "77" smd rect
		(at 6.373 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "78" smd rect
		(at 7.224 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "79" smd rect
		(at 8.073 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "80" smd rect
		(at 8.925 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "81" smd rect
		(at 9.775 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "82" smd rect
		(at 10.624 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "83" smd rect
		(at 11.473 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "84" smd rect
		(at 12.323 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "85" smd rect
		(at 13.175 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "86" smd rect
		(at 14.025 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "87" smd rect
		(at 14.874 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "88" smd rect
		(at 15.723 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "89" smd rect
		(at 16.574 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "90" smd rect
		(at 17.425 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "91" smd rect
		(at 18.274 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "92" smd rect
		(at 19.123 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "93" smd rect
		(at 19.975 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "94" smd rect
		(at 20.824 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "95" smd rect
		(at 21.675 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "96" smd rect
		(at 22.524 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "97" smd rect
		(at 23.373 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "98" smd rect
		(at 24.225 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "99" smd rect
		(at 25.074 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "100" smd rect
		(at 25.925 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "101" smd rect
		(at 26.774 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "102" smd rect
		(at 27.623 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "103" smd rect
		(at 28.475 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "104" smd rect
		(at 29.324 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "105" smd rect
		(at 30.175 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "106" smd rect
		(at 31.024 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "107" smd rect
		(at 31.873 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "108" smd rect
		(at 32.725 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "109" smd rect
		(at 33.575 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "110" smd rect
		(at 34.423 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "111" smd rect
		(at 35.274 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "112" smd rect
		(at 36.124 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "113" smd rect
		(at 36.975 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "114" smd rect
		(at 37.825 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "115" smd rect
		(at 38.673 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "116" smd rect
		(at 39.524 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "117" smd rect
		(at 40.374 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "118" smd rect
		(at 41.225 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "119" smd rect
		(at 42.075 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "120" smd rect
		(at 42.923 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "121" smd rect
		(at 43.773 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "122" smd rect
		(at 44.624 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "123" smd rect
		(at 45.475 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "124" smd rect
		(at 46.325 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "125" smd rect
		(at 47.173 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "126" smd rect
		(at 48.023 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "127" smd rect
		(at 48.874 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "128" smd rect
		(at 49.725 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "129" smd rect
		(at 50.575 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "130" smd rect
		(at 51.423 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "131" smd rect
		(at 52.273 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "132" smd rect
		(at 53.124 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "133" smd rect
		(at 53.975 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "134" smd rect
		(at 54.825 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "135" smd rect
		(at 55.673 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "136" smd rect
		(at 56.523 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "137" smd rect
		(at 57.374 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "138" smd rect
		(at 58.225 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "139" smd rect
		(at 59.075 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "140" smd rect
		(at 59.923 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "141" smd rect
		(at 60.773 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "142" smd rect
		(at 61.624 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "143" smd rect
		(at 62.475 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "144" smd rect
		(at 63.325 2.297 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "145" smd rect
		(at -63.326 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "146" smd rect
		(at -62.476 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "147" smd rect
		(at -61.625 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "148" smd rect
		(at -60.775 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "149" smd rect
		(at -59.926 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "150" smd rect
		(at -59.076 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "151" smd rect
		(at -58.226 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "152" smd rect
		(at -57.375 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "153" smd rect
		(at -56.525 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "154" smd rect
		(at -55.676 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "155" smd rect
		(at -54.826 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "156" smd rect
		(at -53.976 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "157" smd rect
		(at -53.125 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "158" smd rect
		(at -52.275 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "159" smd rect
		(at -51.426 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "160" smd rect
		(at -50.576 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "161" smd rect
		(at -49.726 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "162" smd rect
		(at -48.875 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "163" smd rect
		(at -48.025 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "164" smd rect
		(at -47.176 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "165" smd rect
		(at -46.326 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "166" smd rect
		(at -45.476 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "167" smd rect
		(at -44.625 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "168" smd rect
		(at -43.775 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "169" smd rect
		(at -42.926 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "170" smd rect
		(at -42.076 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "171" smd rect
		(at -41.226 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "172" smd rect
		(at -40.375 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "173" smd rect
		(at -39.525 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "174" smd rect
		(at -38.676 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "175" smd rect
		(at -37.826 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "176" smd rect
		(at -36.976 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "177" smd rect
		(at -36.125 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "178" smd rect
		(at -35.275 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "179" smd rect
		(at -34.426 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "180" smd rect
		(at -33.576 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "181" smd rect
		(at -32.726 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "182" smd rect
		(at -31.875 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "183" smd rect
		(at -31.026 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "184" smd rect
		(at -30.177 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "185" smd rect
		(at -29.325 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "186" smd rect
		(at -28.476 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "187" smd rect
		(at -27.625 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "188" smd rect
		(at -26.776 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "189" smd rect
		(at -25.927 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "190" smd rect
		(at -25.075 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "191" smd rect
		(at -24.226 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "192" smd rect
		(at -23.375 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "193" smd rect
		(at -22.526 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "194" smd rect
		(at -21.677 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "195" smd rect
		(at -20.825 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "196" smd rect
		(at -19.976 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "197" smd rect
		(at -19.125 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "198" smd rect
		(at -18.276 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "199" smd rect
		(at -17.427 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "200" smd rect
		(at -16.575 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "201" smd rect
		(at -15.725 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "202" smd rect
		(at -14.875 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "203" smd rect
		(at -14.026 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "204" smd rect
		(at -13.176 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "205" smd rect
		(at -12.326 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "206" smd rect
		(at -11.475 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "207" smd rect
		(at -10.625 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "208" smd rect
		(at -9.776 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "209" smd rect
		(at -8.926 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "210" smd rect
		(at -8.075 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "211" smd rect
		(at -7.226 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "212" smd rect
		(at -6.375 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "213" smd rect
		(at -5.526 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "214" smd rect
		(at -4.675 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "215" smd rect
		(at -3.826 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "216" smd rect
		(at -2.976 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "217" smd rect
		(at -2.125 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "218" smd rect
		(at -1.276 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "219" smd rect
		(at -0.425 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "220" smd rect
		(at 5.525 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "221" smd rect
		(at 6.373 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "222" smd rect
		(at 7.224 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "223" smd rect
		(at 8.073 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "224" smd rect
		(at 8.925 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "225" smd rect
		(at 9.775 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "226" smd rect
		(at 10.624 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "227" smd rect
		(at 11.473 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "228" smd rect
		(at 12.323 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "229" smd rect
		(at 13.175 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "230" smd rect
		(at 14.025 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "231" smd rect
		(at 14.874 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "232" smd rect
		(at 15.723 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "233" smd rect
		(at 16.574 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "234" smd rect
		(at 17.425 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "235" smd rect
		(at 18.274 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "236" smd rect
		(at 19.123 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "237" smd rect
		(at 19.975 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "238" smd rect
		(at 20.824 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "239" smd rect
		(at 21.675 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "240" smd rect
		(at 22.524 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "241" smd rect
		(at 23.373 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "242" smd rect
		(at 24.225 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "243" smd rect
		(at 25.074 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "244" smd rect
		(at 25.925 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "245" smd rect
		(at 26.774 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "246" smd rect
		(at 27.623 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "247" smd rect
		(at 28.475 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "248" smd rect
		(at 29.324 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "249" smd rect
		(at 30.175 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "250" smd rect
		(at 31.024 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "251" smd rect
		(at 31.873 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "252" smd rect
		(at 32.725 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "253" smd rect
		(at 33.575 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "254" smd rect
		(at 34.423 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "255" smd rect
		(at 35.274 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "256" smd rect
		(at 36.124 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "257" smd rect
		(at 36.975 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "258" smd rect
		(at 37.825 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "259" smd rect
		(at 38.673 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "260" smd rect
		(at 39.524 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "261" smd rect
		(at 40.374 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "262" smd rect
		(at 41.225 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "263" smd rect
		(at 42.075 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "264" smd rect
		(at 42.923 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "265" smd rect
		(at 43.773 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "266" smd rect
		(at 44.624 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "267" smd rect
		(at 45.475 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "268" smd rect
		(at 46.325 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "269" smd rect
		(at 47.173 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "270" smd rect
		(at 48.023 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "271" smd rect
		(at 48.874 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "272" smd rect
		(at 49.725 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "273" smd rect
		(at 50.575 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "274" smd rect
		(at 51.423 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "275" smd rect
		(at 52.273 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "276" smd rect
		(at 53.124 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "277" smd rect
		(at 53.975 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "278" smd rect
		(at 54.825 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "279" smd rect
		(at 55.673 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "280" smd rect
		(at 56.523 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "281" smd rect
		(at 57.374 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "282" smd rect
		(at 58.225 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "283" smd rect
		(at 59.075 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "284" smd rect
		(at 59.923 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "285" smd rect
		(at 60.773 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "286" smd rect
		(at 61.624 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "287" smd rect
		(at 62.475 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "288" smd rect
		(at 63.325 -2.301 90)
		(size 1.8 0.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "S1" thru_hole oval
		(at -68.976 0)
		(size 1.875 3.75)
		(drill oval 1.25 2.53)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "S2" thru_hole oval
		(at 3.874 0)
		(size 1.875 3.75)
		(drill oval 1.25 2.53)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "S3" thru_hole oval
		(at 68.974 0)
		(size 1.875 3.75)
		(drill oval 1.25 2.53)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "antmicro_ddr504111002kq.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 90 -90)
		)
	)
)
