(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Bus_DDR5_DDR504111002KQ"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 45.72 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Bus_DDR5_DDR504111002KQ"
				(at 45.72 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Bus_DDR5_DDR504111002KQ"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.amphenol-icc.com/ddr5-smt-ddr504111002kq.html"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Memory Card Connector, DDR5 DIMM, Latched, 288 Contacts, Copper Alloy, Gold Plated Contacts"
				(at 45.72 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Amphenol"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "DDR504111002KQ"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "VERTICAL, SMT, CONNECTOR, DDR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Bus_DDR5_DDR504111002KQ_1_1"
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(name "DQ0_A")
					(number "7")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 3.81)
					(name "DQ1_A")
					(number "9")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 3.81)
					(name "DQS0_A_T")
					(number "11")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 3.81)
					(name "DQS0_A_C")
					(number "12")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 3.81)
					(name "DQ4_A")
					(number "14")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 3.81)
					(name "DQ5_A")
					(number "16")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 3.81)
					(name "DQ8_A")
					(number "18")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 3.81)
					(name "DQ9_A")
					(number "20")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 3.81)
					(name "DQS1_A_T")
					(number "22")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 3.81)
					(name "DQS1_A_C")
					(number "23")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 3.81)
					(name "DQ12_A")
					(number "25")
				)
				(pin input line
					(at 0 -50.8 0)
					(length 3.81)
					(name "DQ13_A")
					(number "27")
				)
				(pin input line
					(at 0 -66.04 0)
					(length 3.81)
					(name "DQ16_A")
					(number "29")
				)
				(pin input line
					(at 0 -68.58 0)
					(length 3.81)
					(name "DQ17_A")
					(number "31")
				)
				(pin input line
					(at 0 -76.2 0)
					(length 3.81)
					(name "DQS2_A_T")
					(number "33")
				)
				(pin input line
					(at 0 -78.74 0)
					(length 3.81)
					(name "DQS2_A_C")
					(number "34")
				)
				(pin input line
					(at 0 -81.28 0)
					(length 3.81)
					(name "DQ20_A")
					(number "36")
				)
				(pin input line
					(at 0 -83.82 0)
					(length 3.81)
					(name "DQ21_A")
					(number "38")
				)
				(pin input line
					(at 0 -99.06 0)
					(length 3.81)
					(name "DQ24_A")
					(number "40")
				)
				(pin input line
					(at 0 -101.6 0)
					(length 3.81)
					(name "DQ25_A")
					(number "42")
				)
				(pin input line
					(at 0 -109.22 0)
					(length 3.81)
					(name "DQS3_A_T")
					(number "44")
				)
				(pin input line
					(at 0 -111.76 0)
					(length 3.81)
					(name "DQS3_A_C")
					(number "45")
				)
				(pin input line
					(at 0 -114.3 0)
					(length 3.81)
					(name "DQ28_A")
					(number "47")
				)
				(pin input line
					(at 0 -116.84 0)
					(length 3.81)
					(name "DQ29_A")
					(number "49")
				)
				(pin input line
					(at 0 -132.08 0)
					(length 3.81)
					(name "CB0_A")
					(number "51")
				)
				(pin input line
					(at 0 -134.62 0)
					(length 3.81)
					(name "CB1_A")
					(number "53")
				)
				(pin input line
					(at 0 -142.24 0)
					(length 3.81)
					(name "DQS4_A_T")
					(number "55")
				)
				(pin input line
					(at 0 -144.78 0)
					(length 3.81)
					(name "DQS4_A_C")
					(number "56")
				)
				(pin input line
					(at 0 -147.32 0)
					(length 3.81)
					(name "CB4_A")
					(number "58")
				)
				(pin input line
					(at 0 -149.86 0)
					(length 3.81)
					(name "CB5_A")
					(number "60")
				)
				(pin input line
					(at 30.48 -147.32 180)
					(length 3.81)
					(name "CB4_B")
					(number "89")
				)
				(pin input line
					(at 30.48 -149.86 180)
					(length 3.81)
					(name "CB5_B")
					(number "91")
				)
				(pin input line
					(at 30.48 -157.48 180)
					(length 3.81)
					(name "DQS9_B_T")
					(number "93")
				)
				(pin input line
					(at 30.48 -160.02 180)
					(length 3.81)
					(name "DQS9_B_C")
					(number "94")
				)
				(pin input line
					(at 30.48 -132.08 180)
					(length 3.81)
					(name "CB0_B")
					(number "96")
				)
				(pin input line
					(at 30.48 -134.62 180)
					(length 3.81)
					(name "CB1_B")
					(number "98")
				)
				(pin input line
					(at 30.48 0 180)
					(length 3.81)
					(name "DQ0_B")
					(number "100")
				)
				(pin input line
					(at 30.48 -2.54 180)
					(length 3.81)
					(name "DQ1_B")
					(number "102")
				)
				(pin input line
					(at 30.48 -10.16 180)
					(length 3.81)
					(name "DQS0_B_T")
					(number "104")
				)
				(pin input line
					(at 30.48 -12.7 180)
					(length 3.81)
					(name "DQS0_B_C")
					(number "105")
				)
				(pin input line
					(at 30.48 -15.24 180)
					(length 3.81)
					(name "DQ4_B")
					(number "107")
				)
				(pin input line
					(at 30.48 -17.78 180)
					(length 3.81)
					(name "DQ5_B")
					(number "109")
				)
				(pin input line
					(at 30.48 -33.02 180)
					(length 3.81)
					(name "DQ8_B")
					(number "111")
				)
				(pin input line
					(at 30.48 -35.56 180)
					(length 3.81)
					(name "DQ9_B")
					(number "113")
				)
				(pin input line
					(at 30.48 -43.18 180)
					(length 3.81)
					(name "DQS1_B_T")
					(number "115")
				)
				(pin input line
					(at 30.48 -45.72 180)
					(length 3.81)
					(name "DQS1_B_C")
					(number "116")
				)
				(pin input line
					(at 30.48 -48.26 180)
					(length 3.81)
					(name "DQ12_B")
					(number "118")
				)
				(pin input line
					(at 30.48 -50.8 180)
					(length 3.81)
					(name "DQ13_B")
					(number "120")
				)
				(pin input line
					(at 30.48 -66.04 180)
					(length 3.81)
					(name "DQ16_B")
					(number "122")
				)
				(pin input line
					(at 30.48 -68.58 180)
					(length 3.81)
					(name "DQ17_B")
					(number "124")
				)
				(pin input line
					(at 30.48 -76.2 180)
					(length 3.81)
					(name "DQS2_B_T")
					(number "126")
				)
				(pin input line
					(at 30.48 -78.74 180)
					(length 3.81)
					(name "DQS2_B_C")
					(number "127")
				)
				(pin input line
					(at 30.48 -81.28 180)
					(length 3.81)
					(name "DQ20_B")
					(number "129")
				)
				(pin input line
					(at 30.48 -83.82 180)
					(length 3.81)
					(name "DQ21_B")
					(number "131")
				)
				(pin input line
					(at 30.48 -99.06 180)
					(length 3.81)
					(name "DQ24_B")
					(number "133")
				)
				(pin input line
					(at 30.48 -101.6 180)
					(length 3.81)
					(name "DQ25_B")
					(number "135")
				)
				(pin input line
					(at 30.48 -109.22 180)
					(length 3.81)
					(name "DQS3_B_T")
					(number "137")
				)
				(pin input line
					(at 30.48 -111.76 180)
					(length 3.81)
					(name "DQS3_B_C")
					(number "138")
				)
				(pin input line
					(at 30.48 -114.3 180)
					(length 3.81)
					(name "DQ28_B")
					(number "140")
				)
				(pin input line
					(at 30.48 -116.84 180)
					(length 3.81)
					(name "DQ29_B")
					(number "142")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 3.81)
					(name "DQ2_A")
					(number "152")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 3.81)
					(name "DQ3_A")
					(number "154")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 3.81)
					(name "DQS5_A_C")
					(number "156")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 3.81)
					(name "DQS5_A_T")
					(number "157")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 3.81)
					(name "DQ6_A")
					(number "159")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 3.81)
					(name "DQ7_A")
					(number "161")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 3.81)
					(name "DQ10_A")
					(number "163")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 3.81)
					(name "DQ11_A")
					(number "165")
				)
				(pin input line
					(at 0 -60.96 0)
					(length 3.81)
					(name "DQS6_A_C")
					(number "167")
				)
				(pin input line
					(at 0 -58.42 0)
					(length 3.81)
					(name "DQS6_A_T")
					(number "168")
				)
				(pin input line
					(at 0 -53.34 0)
					(length 3.81)
					(name "DQ14_A")
					(number "170")
				)
				(pin input line
					(at 0 -55.88 0)
					(length 3.81)
					(name "DQ15_A")
					(number "172")
				)
				(pin input line
					(at 0 -71.12 0)
					(length 3.81)
					(name "DQ18_A")
					(number "174")
				)
				(pin input line
					(at 0 -73.66 0)
					(length 3.81)
					(name "DQ19_A")
					(number "176")
				)
				(pin input line
					(at 0 -93.98 0)
					(length 3.81)
					(name "DQS7_A_C")
					(number "178")
				)
				(pin input line
					(at 0 -91.44 0)
					(length 3.81)
					(name "DQS7_A_T")
					(number "179")
				)
				(pin input line
					(at 0 -86.36 0)
					(length 3.81)
					(name "DQ22_A")
					(number "181")
				)
				(pin input line
					(at 0 -88.9 0)
					(length 3.81)
					(name "DQ23_A")
					(number "183")
				)
				(pin input line
					(at 0 -104.14 0)
					(length 3.81)
					(name "DQ26_A")
					(number "185")
				)
				(pin input line
					(at 0 -106.68 0)
					(length 3.81)
					(name "DQ27_A")
					(number "187")
				)
				(pin input line
					(at 0 -127 0)
					(length 3.81)
					(name "DQS8_A_C")
					(number "189")
				)
				(pin input line
					(at 0 -124.46 0)
					(length 3.81)
					(name "DQS8_A_T")
					(number "190")
				)
				(pin input line
					(at 0 -119.38 0)
					(length 3.81)
					(name "DQ30_A")
					(number "192")
				)
				(pin input line
					(at 0 -121.92 0)
					(length 3.81)
					(name "DQ31_A")
					(number "194")
				)
				(pin input line
					(at 0 -137.16 0)
					(length 3.81)
					(name "CB2_A")
					(number "196")
				)
				(pin input line
					(at 0 -139.7 0)
					(length 3.81)
					(name "CB3_A")
					(number "198")
				)
				(pin input line
					(at 0 -160.02 0)
					(length 3.81)
					(name "DQS9_A_C")
					(number "200")
				)
				(pin input line
					(at 0 -157.48 0)
					(length 3.81)
					(name "DQS9_A_T")
					(number "201")
				)
				(pin input line
					(at 0 -152.4 0)
					(length 3.81)
					(name "CB6_A")
					(number "203")
				)
				(pin input line
					(at 0 -154.94 0)
					(length 3.81)
					(name "CB7_A")
					(number "205")
				)
				(pin input line
					(at 30.48 -152.4 180)
					(length 3.81)
					(name "CB6_B")
					(number "234")
				)
				(pin input line
					(at 30.48 -154.94 180)
					(length 3.81)
					(name "CB7_B")
					(number "236")
				)
				(pin input line
					(at 30.48 -144.78 180)
					(length 3.81)
					(name "DQS4_B_C")
					(number "238")
				)
				(pin input line
					(at 30.48 -142.24 180)
					(length 3.81)
					(name "DQS4_B_T")
					(number "239")
				)
				(pin input line
					(at 30.48 -137.16 180)
					(length 3.81)
					(name "CB2_B")
					(number "241")
				)
				(pin input line
					(at 30.48 -139.7 180)
					(length 3.81)
					(name "CB3_B")
					(number "243")
				)
				(pin input line
					(at 30.48 -5.08 180)
					(length 3.81)
					(name "DQ2_B")
					(number "245")
				)
				(pin input line
					(at 30.48 -7.62 180)
					(length 3.81)
					(name "DQ3_B")
					(number "247")
				)
				(pin input line
					(at 30.48 -27.94 180)
					(length 3.81)
					(name "DQS5_B_C")
					(number "249")
				)
				(pin input line
					(at 30.48 -25.4 180)
					(length 3.81)
					(name "DQS5_B_T")
					(number "250")
				)
				(pin input line
					(at 30.48 -20.32 180)
					(length 3.81)
					(name "DQ6_B")
					(number "252")
				)
				(pin input line
					(at 30.48 -22.86 180)
					(length 3.81)
					(name "DQ7_B")
					(number "254")
				)
				(pin input line
					(at 30.48 -38.1 180)
					(length 3.81)
					(name "DQ10_B")
					(number "256")
				)
				(pin input line
					(at 30.48 -40.64 180)
					(length 3.81)
					(name "DQ11_B")
					(number "258")
				)
				(pin input line
					(at 30.48 -60.96 180)
					(length 3.81)
					(name "DQS6_B_C")
					(number "260")
				)
				(pin input line
					(at 30.48 -58.42 180)
					(length 3.81)
					(name "DQS6_B_T")
					(number "261")
				)
				(pin input line
					(at 30.48 -53.34 180)
					(length 3.81)
					(name "DQ14_B")
					(number "263")
				)
				(pin input line
					(at 30.48 -55.88 180)
					(length 3.81)
					(name "DQ15_B")
					(number "265")
				)
				(pin input line
					(at 30.48 -71.12 180)
					(length 3.81)
					(name "DQ18_B")
					(number "267")
				)
				(pin input line
					(at 30.48 -73.66 180)
					(length 3.81)
					(name "DQ19_B")
					(number "269")
				)
				(pin input line
					(at 30.48 -93.98 180)
					(length 3.81)
					(name "DQS7_B_C")
					(number "271")
				)
				(pin input line
					(at 30.48 -91.44 180)
					(length 3.81)
					(name "DQS7_B_T")
					(number "272")
				)
				(pin input line
					(at 30.48 -86.36 180)
					(length 3.81)
					(name "DQ22_B")
					(number "274")
				)
				(pin input line
					(at 30.48 -88.9 180)
					(length 3.81)
					(name "DQ23_B")
					(number "276")
				)
				(pin input line
					(at 30.48 -104.14 180)
					(length 3.81)
					(name "DQ26_B")
					(number "278")
				)
				(pin input line
					(at 30.48 -106.68 180)
					(length 3.81)
					(name "DQ27_B")
					(number "280")
				)
				(pin input line
					(at 30.48 -127 180)
					(length 3.81)
					(name "DQS8_B_C")
					(number "282")
				)
				(pin input line
					(at 30.48 -124.46 180)
					(length 3.81)
					(name "DQS8_B_T")
					(number "283")
				)
				(pin input line
					(at 30.48 -119.38 180)
					(length 3.81)
					(name "DQ30_B")
					(number "285")
				)
				(pin input line
					(at 30.48 -121.92 180)
					(length 3.81)
					(name "DQ31_B")
					(number "287")
				)
			)
			(symbol "Bus_DDR5_DDR504111002KQ_2_1"
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VIN_BULK")
					(number "1")
				)
				(pin no_connect line
					(at 3.81 -48.26 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "2")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(name "VIN_MGMT")
					(number "3")
				)
				(pin input line
					(at 30.48 -5.08 180)
					(length 3.81)
					(name "HSCL")
					(number "4")
				)
				(pin input line
					(at 30.48 -2.54 180)
					(length 3.81)
					(name "HSDA")
					(number "5")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "6")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "8")
				)
				(pin power_in line
					(at 0 -55.88 0)
					(length 3.81)
					(name "VSS")
					(number "10")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "13")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "15")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "17")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "19")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "21")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "24")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "26")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "28")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "30")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "32")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "35")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "37")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "39")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "41")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "43")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "46")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "48")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "50")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "52")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "54")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "57")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "59")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "61")
				)
				(pin input line
					(at 30.48 -10.16 180)
					(length 3.81)
					(name "ALERT_N")
					(number "62")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "63")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 3.81)
					(name "CS0_A_N")
					(number "64")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "65")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 3.81)
					(name "CA0_A")
					(number "66")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "67")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 3.81)
					(name "CA2_A")
					(number "68")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "69")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 3.81)
					(name "CA4_A")
					(number "70")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "71")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 3.81)
					(name "CA6_A")
					(number "72")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "73")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 3.81)
					(name "PAR_A")
					(number "74")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 3.81)
					(hide yes)
					(name "VSS_DET")
					(number "75")
				)
				(pin input line
					(at 30.48 -20.32 180)
					(length 3.81)
					(name "CA0_B")
					(number "76")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "77")
				)
				(pin input line
					(at 30.48 -25.4 180)
					(length 3.81)
					(name "CA2_B")
					(number "78")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "79")
				)
				(pin input line
					(at 30.48 -30.48 180)
					(length 3.81)
					(name "CA4_B")
					(number "80")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "81")
				)
				(pin input line
					(at 30.48 -35.56 180)
					(length 3.81)
					(name "CA6_B")
					(number "82")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "83")
				)
				(pin input line
					(at 30.48 -40.64 180)
					(length 3.81)
					(name "CS0_B_N")
					(number "84")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "85")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 3.81)
					(name "DLBDQ")
					(number "86")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 3.81)
					(name "DLBDQS")
					(number "87")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "88")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "90")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "92")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "95")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "97")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "99")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "101")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "103")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "106")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "108")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "110")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "112")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "114")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "117")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "119")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "121")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "123")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "125")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "128")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "130")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "132")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "134")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "136")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "139")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "141")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "143")
				)
				(pin no_connect line
					(at 3.81 -50.8 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "144")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VIN_BULK")
					(number "145")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VIN_BULK")
					(number "146")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 3.81)
					(name "PCAMP")
					(number "147")
				)
				(pin input line
					(at 30.48 0 180)
					(length 3.81)
					(name "HSA")
					(number "148")
				)
				(pin no_connect line
					(at 26.67 -45.72 180)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "149")
				)
				(pin no_connect line
					(at 3.81 -45.72 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "150")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "151")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "153")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "155")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "158")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "160")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "162")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "164")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "166")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "169")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "171")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "173")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "175")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "177")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "180")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "182")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "184")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "186")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "188")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "191")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "193")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "195")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "197")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "199")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "202")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "204")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "206")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 3.81)
					(name "RESET_N")
					(number "207")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "208")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 3.81)
					(name "CS1_A_N")
					(number "209")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "210")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 3.81)
					(name "CA1_A")
					(number "211")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "212")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 3.81)
					(name "CA3_A")
					(number "213")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "214")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 3.81)
					(name "CA5_A")
					(number "215")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "216")
				)
				(pin input line
					(at 30.48 -12.7 180)
					(length 3.81)
					(name "CK_T")
					(number "217")
				)
				(pin input line
					(at 30.48 -15.24 180)
					(length 3.81)
					(name "CK_C")
					(number "218")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "219")
				)
				(pin no_connect line
					(at 26.67 -50.8 180)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "220")
				)
				(pin input line
					(at 30.48 -22.86 180)
					(length 3.81)
					(name "CA1_B")
					(number "221")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "222")
				)
				(pin input line
					(at 30.48 -27.94 180)
					(length 3.81)
					(name "CA3_B")
					(number "223")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "224")
				)
				(pin input line
					(at 30.48 -33.02 180)
					(length 3.81)
					(name "CA5_B")
					(number "225")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "226")
				)
				(pin input line
					(at 30.48 -38.1 180)
					(length 3.81)
					(name "PAR_B")
					(number "227")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "228")
				)
				(pin input line
					(at 30.48 -43.18 180)
					(length 3.81)
					(name "CS1_B_N")
					(number "229")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "230")
				)
				(pin no_connect line
					(at 26.67 -53.34 180)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "231")
				)
				(pin no_connect line
					(at 26.67 -48.26 180)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "232")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "233")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "235")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "237")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "240")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "242")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "244")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "246")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "248")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "251")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "253")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "255")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "257")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "259")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "262")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "264")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "266")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "268")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "270")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "273")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "275")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "277")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "279")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "281")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "284")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "286")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "288")
				)
				(pin passive line
					(at 30.48 -55.88 180)
					(length 3.81)
					(name "SH")
					(number "S1")
				)
				(pin passive line
					(at 30.48 -58.42 180)
					(length 3.81)
					(name "SH")
					(number "S2")
				)
				(pin passive line
					(at 30.48 -60.96 180)
					(length 3.81)
					(name "SH")
					(number "S3")
				)
			)
			(embedded_fonts no)
		)
)
