(footprint "MicroSD_DM3AT-SF-PEJM5"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Micro SD, SMD, right-angle, push-pull")
	(tags "Micro SD")
	(property "Reference" "REF**"
		(at 0 -9.19 0)
		(layer "F.SilkS")
	)
	(property "Value" "MicroSD_DM3AT-SF-PEJM5"
		(at 0 9.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "KEEPOUT"
		(at -6.47 -1.2 90)
		(layer "Cmts.User")
	)
	(fp_text user "KEEPOUT"
		(at -5.42 4.64 90)
		(layer "Cmts.User")
	)
	(fp_text user "KEEPOUT"
		(at -3.54 -1.78 0)
		(layer "Cmts.User")
	)
	(fp_text user "KEEPOUT"
		(at 2.09 7.73 0)
		(layer "Cmts.User")
	)
	(fp_text user "Author: Antmicro"
		(at -7.927 15.498 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -7.927 16.698 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -7.927 17.898 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at 2.749 -7.952)
		(size 0.7 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 1.65 -7.952)
		(size 0.7 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 0.549 -7.952)
		(size 0.7 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -0.552 -7.952)
		(size 0.7 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -1.651 -7.952)
		(size 0.7 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -2.751 -7.952)
		(size 0.7 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -3.851 -7.952)
		(size 0.7 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -4.951 -7.952)
		(size 0.7 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -5.901 -7.952)
		(size 0.7 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -6.851 2.547)
		(size 1 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -6.851 -3.652)
		(size 1 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -6.851 6.698)
		(size 1 2.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 4.299 -7.952)
		(size 1 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 6.648 7.148)
		(size 1.3 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_dm3at_sf_pejm5.glb"
		(offset
			(xyz -0.225 8.075 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
