(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "DM3AT-SF-PEJM5"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 57.15 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "DM3AT-SF-PEJM5"
				(at 57.15 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "DM3AT-SF-PEJM5"
				(at 57.15 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.hirose.com/en/product/document?clcode=CL0609-0031-0-00&productname=DM3AT-SF-PEJM5&series=DM3&documenttype=2DDrawing&lang=en&documentid=0000947170"
				(at 57.15 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Memory Card Connector, MicroSD, Push-Push, 8 Contacts, Copper Alloy, Gold Plated Contacts, DM3"
				(at 57.15 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Hirose Electric"
				(at 57.15 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "DM3AT-SF-PEJM5"
				(at 57.15 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 57.15 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 57.15 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "DM3AT-SF-PEJM5_1_1"
				(pin bidirectional line
					(at 0 0 0)
					(length 2.54)
					(name "DAT2")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 2.54)
					(name "DAT3/CD")
					(number "2")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "CMD")
					(number "3")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VDD")
					(number "4")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "CLK")
					(number "5")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 2.54)
					(name "VSS")
					(number "6")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "DAT0")
					(number "7")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "DAT1")
					(number "8")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 2.54)
					(name "DET_B")
					(number "9")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "DET_A")
					(number "10")
				)
				(pin passive line
					(at 40.64 -22.86 180)
					(length 2.54)
					(name "SHIELD")
					(number "11")
				)
			)
			(embedded_fonts no)
		)
)
