(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "EMIF06-MSD02N16"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 40.64 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "EMIF06-MSD02N16"
				(at 40.64 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "EMIF06-MSD02N16"
				(at 40.64 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/389/emif06_msd02n16-1849116.pdf"
				(at 40.64 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "EMI Filter, 6-Channel, ESD Protection,  MHz, µQFN-16, SD Card"
				(at 40.64 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "EMIF06-MSD02N16"
				(at 40.64 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "STMicroelectronics"
				(at 40.64 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 40.64 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 40.64 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, SMT, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "EMIF06-MSD02N16_1_1"
				(pin input line
					(at 0 -24.13 0)
					(length 2.54)
					(name "WP/CD")
					(number "1")
				)
				(pin passive line
					(at 24.13 -21.59 180)
					(length 2.54)
					(name "RDAT3_GND")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 2.54)
					(name "DAT2_In")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 2.54)
					(name "DAT3_In")
					(number "4")
				)
				(pin input line
					(at 0 -11.43 0)
					(length 2.54)
					(name "CMD_In")
					(number "5")
				)
				(pin input line
					(at 0 -13.97 0)
					(length 2.54)
					(name "CLK_In")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 2.54)
					(name "DAT0_In")
					(number "7")
				)
				(pin input line
					(at 0 -19.05 0)
					(length 2.54)
					(name "DAT1_In")
					(number "8")
				)
				(pin bidirectional line
					(at 24.13 -19.05 180)
					(length 2.54)
					(name "DAT1_Ex")
					(number "9")
				)
				(pin bidirectional line
					(at 24.13 -16.51 180)
					(length 2.54)
					(name "DAT0_Ex")
					(number "10")
				)
				(pin output line
					(at 24.13 -13.97 180)
					(length 2.54)
					(name "CLK_Ex")
					(number "11")
				)
				(pin output line
					(at 24.13 -11.43 180)
					(length 2.54)
					(name "CMD_Ex")
					(number "12")
				)
				(pin bidirectional line
					(at 24.13 -8.89 180)
					(length 2.54)
					(name "DAT3_Ex")
					(number "13")
				)
				(pin bidirectional line
					(at 24.13 -6.35 180)
					(length 2.54)
					(name "DAT2_Ex")
					(number "14")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "15")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "RDATA_VCC")
					(number "16")
				)
				(pin power_in line
					(at 24.13 -24.13 180)
					(length 2.54)
					(name "GND")
					(number "17")
				)
			)
			(embedded_fonts no)
		)
)
