(footprint "Conn_Socket_Hirose_FX10_2x84_FX10A-168S-SV"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0.05 -5.25 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Conn_Socket_Hirose_FX10_2x84_FX10A-168S-SV"
		(at 0.1 5.75 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "License: Apache-2.0"
		(at -25.54 6.65 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -25.54 7.85 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -25.54 9.05 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -22.224 -0.023 90)
		(size 1.25 1.25)
		(drill 1.25)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 22.175 -0.023 90)
		(size 1.25 1.25)
		(drill 1.25)
		(layers "F.Cu" "*.Mask")
	)
	(pad "1" smd rect
		(at -20.75 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -20.75 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -20.25 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -20.25 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -19.75 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -19.75 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -19.25 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -19.25 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -18.75 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -18.75 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -18.25 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -18.25 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -17.75 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -17.75 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -17.25 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -17.25 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -16.75 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -16.75 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -16.25 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at -16.25 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at -15.75 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at -15.75 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at -15.25 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at -15.25 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at -14.75 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at -14.75 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at -14.25 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at -14.25 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at -13.75 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at -13.75 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at -13.25 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at -13.25 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at -12.75 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at -12.75 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at -12.25 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at -12.25 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at -11.75 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at -11.75 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at -11.25 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at -11.25 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd rect
		(at -10.75 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd rect
		(at -10.75 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd rect
		(at -10.25 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd rect
		(at -10.25 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "45" smd rect
		(at -9.75 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "46" smd rect
		(at -9.75 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "47" smd rect
		(at -9.25 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "48" smd rect
		(at -9.25 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "49" smd rect
		(at -8.75 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "50" smd rect
		(at -8.75 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "51" smd rect
		(at -8.25 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "52" smd rect
		(at -8.25 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "53" smd rect
		(at -7.751 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "54" smd rect
		(at -7.751 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "55" smd rect
		(at -7.251 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "56" smd rect
		(at -7.251 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "57" smd rect
		(at -6.75 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "58" smd rect
		(at -6.75 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "59" smd rect
		(at -6.25 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "60" smd rect
		(at -6.25 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "61" smd rect
		(at -5.75 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "62" smd rect
		(at -5.75 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "63" smd rect
		(at -5.25 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "64" smd rect
		(at -5.25 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "65" smd rect
		(at -4.751 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "66" smd rect
		(at -4.751 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "67" smd rect
		(at -4.251 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "68" smd rect
		(at -4.251 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "69" smd rect
		(at -3.751 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "70" smd rect
		(at -3.751 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "71" smd rect
		(at -3.251 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "72" smd rect
		(at -3.251 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "73" smd rect
		(at -2.751 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "74" smd rect
		(at -2.751 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "75" smd rect
		(at -2.251 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "76" smd rect
		(at -2.251 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "77" smd rect
		(at -1.751 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "78" smd rect
		(at -1.751 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "79" smd rect
		(at -1.251 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "80" smd rect
		(at -1.251 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "81" smd rect
		(at -0.751 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "82" smd rect
		(at -0.751 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "83" smd rect
		(at -0.251 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "84" smd rect
		(at -0.251 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "85" smd rect
		(at 0.25 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "86" smd rect
		(at 0.25 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "87" smd rect
		(at 0.749 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "88" smd rect
		(at 0.749 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "89" smd rect
		(at 1.249 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "90" smd rect
		(at 1.249 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "91" smd rect
		(at 1.749 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "92" smd rect
		(at 1.749 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "93" smd rect
		(at 2.25 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "94" smd rect
		(at 2.25 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "95" smd rect
		(at 2.75 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "96" smd rect
		(at 2.75 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "97" smd rect
		(at 3.249 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "98" smd rect
		(at 3.249 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "99" smd rect
		(at 3.75 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "100" smd rect
		(at 3.75 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "101" smd rect
		(at 4.251 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "102" smd rect
		(at 4.251 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "103" smd rect
		(at 4.751 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "104" smd rect
		(at 4.751 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "105" smd rect
		(at 5.251 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "106" smd rect
		(at 5.251 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "107" smd rect
		(at 5.751 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "108" smd rect
		(at 5.751 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "109" smd rect
		(at 6.251 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "110" smd rect
		(at 6.251 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "111" smd rect
		(at 6.751 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "112" smd rect
		(at 6.751 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "113" smd rect
		(at 7.251 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "114" smd rect
		(at 7.251 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "115" smd rect
		(at 7.751 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "116" smd rect
		(at 7.751 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "117" smd rect
		(at 8.251 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "118" smd rect
		(at 8.251 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "119" smd rect
		(at 8.751 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "120" smd rect
		(at 8.751 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "121" smd rect
		(at 9.251 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "122" smd rect
		(at 9.251 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "123" smd rect
		(at 9.751 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "124" smd rect
		(at 9.751 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "125" smd rect
		(at 10.251 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "126" smd rect
		(at 10.251 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "127" smd rect
		(at 10.751 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "128" smd rect
		(at 10.751 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "129" smd rect
		(at 11.25 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "130" smd rect
		(at 11.25 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "131" smd rect
		(at 11.75 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "132" smd rect
		(at 11.75 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "133" smd rect
		(at 12.25 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "134" smd rect
		(at 12.25 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "135" smd rect
		(at 12.75 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "136" smd rect
		(at 12.75 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "137" smd rect
		(at 13.25 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "138" smd rect
		(at 13.25 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "139" smd rect
		(at 13.75 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "140" smd rect
		(at 13.75 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "141" smd rect
		(at 14.25 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "142" smd rect
		(at 14.25 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "143" smd rect
		(at 14.75 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "144" smd rect
		(at 14.75 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "145" smd rect
		(at 15.25 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "146" smd rect
		(at 15.25 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "147" smd rect
		(at 15.75 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "148" smd rect
		(at 15.75 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "149" smd rect
		(at 16.25 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "150" smd rect
		(at 16.25 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "151" smd rect
		(at 16.75 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "152" smd rect
		(at 16.75 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "153" smd rect
		(at 17.25 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "154" smd rect
		(at 17.25 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "155" smd rect
		(at 17.75 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "156" smd rect
		(at 17.75 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "157" smd rect
		(at 18.25 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "158" smd rect
		(at 18.25 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "159" smd rect
		(at 18.75 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "160" smd rect
		(at 18.75 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "161" smd rect
		(at 19.25 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "162" smd rect
		(at 19.25 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "163" smd rect
		(at 19.75 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "164" smd rect
		(at 19.75 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "165" smd rect
		(at 20.25 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "166" smd rect
		(at 20.25 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "167" smd rect
		(at 20.75 3)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "168" smd rect
		(at 20.75 -3.05)
		(size 0.33 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MP" smd rect
		(at -23.974 -0.023 90)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MP" smd rect
		(at 23.925 -0.023 90)
		(size 3.2 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_fx10a_168s_sv.glb"
		(offset
			(xyz 6.476 -2.176 0.9)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 90)
		)
	)
)
