(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Socket_Hirose_FX10_2x84_FX10A-168S-SV"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 35.56 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Socket_Hirose_FX10_2x84_FX10A-168S-SV"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Socket_Hirose_FX10_2x84_FX10A-168S-SV"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/185/FX10_Catalog_D31650_en-2585888.pdf"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Board to Board & Mezzanine Connectors REC 168P W/POST SMT"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "FX10A-168S-SV"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Hirose Electric"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Pitch" "0.5 mm"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "CONNECTOR, B2B, SOCKET, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Socket_Hirose_FX10_2x84_FX10A-168S-SV_1_1"
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "")
					(number "1")
				)
				(pin passive line
					(at 13.97 0 180)
					(length 3.81)
					(name "")
					(number "2")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "")
					(number "3")
				)
				(pin passive line
					(at 13.97 -2.54 180)
					(length 3.81)
					(name "")
					(number "4")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "")
					(number "5")
				)
				(pin passive line
					(at 13.97 -5.08 180)
					(length 3.81)
					(name "")
					(number "6")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "")
					(number "7")
				)
				(pin passive line
					(at 13.97 -7.62 180)
					(length 3.81)
					(name "")
					(number "8")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "")
					(number "9")
				)
				(pin passive line
					(at 13.97 -10.16 180)
					(length 3.81)
					(name "")
					(number "10")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "")
					(number "11")
				)
				(pin passive line
					(at 13.97 -12.7 180)
					(length 3.81)
					(name "")
					(number "12")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "")
					(number "13")
				)
				(pin passive line
					(at 13.97 -15.24 180)
					(length 3.81)
					(name "")
					(number "14")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 3.81)
					(name "")
					(number "15")
				)
				(pin passive line
					(at 13.97 -17.78 180)
					(length 3.81)
					(name "")
					(number "16")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(name "")
					(number "17")
				)
				(pin passive line
					(at 13.97 -20.32 180)
					(length 3.81)
					(name "")
					(number "18")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 3.81)
					(name "")
					(number "19")
				)
				(pin passive line
					(at 13.97 -22.86 180)
					(length 3.81)
					(name "")
					(number "20")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(name "")
					(number "21")
				)
				(pin passive line
					(at 13.97 -25.4 180)
					(length 3.81)
					(name "")
					(number "22")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(name "")
					(number "23")
				)
				(pin passive line
					(at 13.97 -27.94 180)
					(length 3.81)
					(name "")
					(number "24")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(name "")
					(number "25")
				)
				(pin passive line
					(at 13.97 -30.48 180)
					(length 3.81)
					(name "")
					(number "26")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(name "")
					(number "27")
				)
				(pin passive line
					(at 13.97 -33.02 180)
					(length 3.81)
					(name "")
					(number "28")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 3.81)
					(name "")
					(number "29")
				)
				(pin passive line
					(at 13.97 -35.56 180)
					(length 3.81)
					(name "")
					(number "30")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 3.81)
					(name "")
					(number "31")
				)
				(pin passive line
					(at 13.97 -38.1 180)
					(length 3.81)
					(name "")
					(number "32")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(name "")
					(number "33")
				)
				(pin passive line
					(at 13.97 -40.64 180)
					(length 3.81)
					(name "")
					(number "34")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 3.81)
					(name "")
					(number "35")
				)
				(pin passive line
					(at 13.97 -43.18 180)
					(length 3.81)
					(name "")
					(number "36")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 3.81)
					(name "")
					(number "37")
				)
				(pin passive line
					(at 13.97 -45.72 180)
					(length 3.81)
					(name "")
					(number "38")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 3.81)
					(name "")
					(number "39")
				)
				(pin passive line
					(at 13.97 -48.26 180)
					(length 3.81)
					(name "")
					(number "40")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "")
					(number "41")
				)
				(pin passive line
					(at 13.97 -50.8 180)
					(length 3.81)
					(name "")
					(number "42")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 3.81)
					(name "")
					(number "43")
				)
				(pin passive line
					(at 13.97 -53.34 180)
					(length 3.81)
					(name "")
					(number "44")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(name "")
					(number "45")
				)
				(pin passive line
					(at 13.97 -55.88 180)
					(length 3.81)
					(name "")
					(number "46")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "")
					(number "47")
				)
				(pin passive line
					(at 13.97 -58.42 180)
					(length 3.81)
					(name "")
					(number "48")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 3.81)
					(name "")
					(number "49")
				)
				(pin passive line
					(at 13.97 -60.96 180)
					(length 3.81)
					(name "")
					(number "50")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 3.81)
					(name "")
					(number "51")
				)
				(pin passive line
					(at 13.97 -63.5 180)
					(length 3.81)
					(name "")
					(number "52")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "")
					(number "53")
				)
				(pin passive line
					(at 13.97 -66.04 180)
					(length 3.81)
					(name "")
					(number "54")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 3.81)
					(name "")
					(number "55")
				)
				(pin passive line
					(at 13.97 -68.58 180)
					(length 3.81)
					(name "")
					(number "56")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 3.81)
					(name "")
					(number "57")
				)
				(pin passive line
					(at 13.97 -71.12 180)
					(length 3.81)
					(name "")
					(number "58")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 3.81)
					(name "")
					(number "59")
				)
				(pin passive line
					(at 13.97 -73.66 180)
					(length 3.81)
					(name "")
					(number "60")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 3.81)
					(name "")
					(number "61")
				)
				(pin passive line
					(at 13.97 -76.2 180)
					(length 3.81)
					(name "")
					(number "62")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 3.81)
					(name "")
					(number "63")
				)
				(pin passive line
					(at 13.97 -78.74 180)
					(length 3.81)
					(name "")
					(number "64")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 3.81)
					(name "")
					(number "65")
				)
				(pin passive line
					(at 13.97 -81.28 180)
					(length 3.81)
					(name "")
					(number "66")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 3.81)
					(name "")
					(number "67")
				)
				(pin passive line
					(at 13.97 -83.82 180)
					(length 3.81)
					(name "")
					(number "68")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 3.81)
					(name "")
					(number "69")
				)
				(pin passive line
					(at 13.97 -86.36 180)
					(length 3.81)
					(name "")
					(number "70")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 3.81)
					(name "")
					(number "71")
				)
				(pin passive line
					(at 13.97 -88.9 180)
					(length 3.81)
					(name "")
					(number "72")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 3.81)
					(name "")
					(number "73")
				)
				(pin passive line
					(at 13.97 -91.44 180)
					(length 3.81)
					(name "")
					(number "74")
				)
				(pin passive line
					(at 0 -93.98 0)
					(length 3.81)
					(name "")
					(number "75")
				)
				(pin passive line
					(at 13.97 -93.98 180)
					(length 3.81)
					(name "")
					(number "76")
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 3.81)
					(name "")
					(number "77")
				)
				(pin passive line
					(at 13.97 -96.52 180)
					(length 3.81)
					(name "")
					(number "78")
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 3.81)
					(name "")
					(number "79")
				)
				(pin passive line
					(at 13.97 -99.06 180)
					(length 3.81)
					(name "")
					(number "80")
				)
				(pin passive line
					(at 0 -101.6 0)
					(length 3.81)
					(name "")
					(number "81")
				)
				(pin passive line
					(at 13.97 -101.6 180)
					(length 3.81)
					(name "")
					(number "82")
				)
				(pin passive line
					(at 0 -104.14 0)
					(length 3.81)
					(name "")
					(number "83")
				)
				(pin passive line
					(at 13.97 -104.14 180)
					(length 3.81)
					(name "")
					(number "84")
				)
				(pin passive line
					(at 0 -106.68 0)
					(length 3.81)
					(name "")
					(number "85")
				)
				(pin passive line
					(at 13.97 -106.68 180)
					(length 3.81)
					(name "")
					(number "86")
				)
				(pin passive line
					(at 0 -109.22 0)
					(length 3.81)
					(name "")
					(number "87")
				)
				(pin passive line
					(at 13.97 -109.22 180)
					(length 3.81)
					(name "")
					(number "88")
				)
				(pin passive line
					(at 0 -111.76 0)
					(length 3.81)
					(name "")
					(number "89")
				)
				(pin passive line
					(at 13.97 -111.76 180)
					(length 3.81)
					(name "")
					(number "90")
				)
				(pin passive line
					(at 0 -114.3 0)
					(length 3.81)
					(name "")
					(number "91")
				)
				(pin passive line
					(at 13.97 -114.3 180)
					(length 3.81)
					(name "")
					(number "92")
				)
				(pin passive line
					(at 0 -116.84 0)
					(length 3.81)
					(name "")
					(number "93")
				)
				(pin passive line
					(at 13.97 -116.84 180)
					(length 3.81)
					(name "")
					(number "94")
				)
				(pin passive line
					(at 0 -119.38 0)
					(length 3.81)
					(name "")
					(number "95")
				)
				(pin passive line
					(at 13.97 -119.38 180)
					(length 3.81)
					(name "")
					(number "96")
				)
				(pin passive line
					(at 0 -121.92 0)
					(length 3.81)
					(name "")
					(number "97")
				)
				(pin passive line
					(at 13.97 -121.92 180)
					(length 3.81)
					(name "")
					(number "98")
				)
				(pin passive line
					(at 0 -124.46 0)
					(length 3.81)
					(name "")
					(number "99")
				)
				(pin passive line
					(at 13.97 -124.46 180)
					(length 3.81)
					(name "")
					(number "100")
				)
				(pin passive line
					(at 0 -127 0)
					(length 3.81)
					(name "")
					(number "101")
				)
				(pin passive line
					(at 13.97 -127 180)
					(length 3.81)
					(name "")
					(number "102")
				)
				(pin passive line
					(at 0 -129.54 0)
					(length 3.81)
					(name "")
					(number "103")
				)
				(pin passive line
					(at 13.97 -129.54 180)
					(length 3.81)
					(name "")
					(number "104")
				)
				(pin passive line
					(at 0 -132.08 0)
					(length 3.81)
					(name "")
					(number "105")
				)
				(pin passive line
					(at 13.97 -132.08 180)
					(length 3.81)
					(name "")
					(number "106")
				)
				(pin passive line
					(at 0 -134.62 0)
					(length 3.81)
					(name "")
					(number "107")
				)
				(pin passive line
					(at 13.97 -134.62 180)
					(length 3.81)
					(name "")
					(number "108")
				)
				(pin passive line
					(at 0 -137.16 0)
					(length 3.81)
					(name "")
					(number "109")
				)
				(pin passive line
					(at 13.97 -137.16 180)
					(length 3.81)
					(name "")
					(number "110")
				)
				(pin passive line
					(at 0 -139.7 0)
					(length 3.81)
					(name "")
					(number "111")
				)
				(pin passive line
					(at 13.97 -139.7 180)
					(length 3.81)
					(name "")
					(number "112")
				)
				(pin passive line
					(at 0 -142.24 0)
					(length 3.81)
					(name "")
					(number "113")
				)
				(pin passive line
					(at 13.97 -142.24 180)
					(length 3.81)
					(name "")
					(number "114")
				)
				(pin passive line
					(at 0 -144.78 0)
					(length 3.81)
					(name "")
					(number "115")
				)
				(pin passive line
					(at 13.97 -144.78 180)
					(length 3.81)
					(name "")
					(number "116")
				)
				(pin passive line
					(at 0 -147.32 0)
					(length 3.81)
					(name "")
					(number "117")
				)
				(pin passive line
					(at 13.97 -147.32 180)
					(length 3.81)
					(name "")
					(number "118")
				)
				(pin passive line
					(at 0 -149.86 0)
					(length 3.81)
					(name "")
					(number "119")
				)
				(pin passive line
					(at 13.97 -149.86 180)
					(length 3.81)
					(name "")
					(number "120")
				)
				(pin passive line
					(at 0 -152.4 0)
					(length 3.81)
					(name "")
					(number "121")
				)
				(pin passive line
					(at 13.97 -152.4 180)
					(length 3.81)
					(name "")
					(number "122")
				)
				(pin passive line
					(at 0 -154.94 0)
					(length 3.81)
					(name "")
					(number "123")
				)
				(pin passive line
					(at 13.97 -154.94 180)
					(length 3.81)
					(name "")
					(number "124")
				)
				(pin passive line
					(at 0 -157.48 0)
					(length 3.81)
					(name "")
					(number "125")
				)
				(pin passive line
					(at 13.97 -157.48 180)
					(length 3.81)
					(name "")
					(number "126")
				)
				(pin passive line
					(at 0 -160.02 0)
					(length 3.81)
					(name "")
					(number "127")
				)
				(pin passive line
					(at 13.97 -160.02 180)
					(length 3.81)
					(name "")
					(number "128")
				)
				(pin passive line
					(at 0 -162.56 0)
					(length 3.81)
					(name "")
					(number "129")
				)
				(pin passive line
					(at 13.97 -162.56 180)
					(length 3.81)
					(name "")
					(number "130")
				)
				(pin passive line
					(at 0 -165.1 0)
					(length 3.81)
					(name "")
					(number "131")
				)
				(pin passive line
					(at 13.97 -165.1 180)
					(length 3.81)
					(name "")
					(number "132")
				)
				(pin passive line
					(at 0 -167.64 0)
					(length 3.81)
					(name "")
					(number "133")
				)
				(pin passive line
					(at 13.97 -167.64 180)
					(length 3.81)
					(name "")
					(number "134")
				)
				(pin passive line
					(at 0 -170.18 0)
					(length 3.81)
					(name "")
					(number "135")
				)
				(pin passive line
					(at 13.97 -170.18 180)
					(length 3.81)
					(name "")
					(number "136")
				)
				(pin passive line
					(at 0 -172.72 0)
					(length 3.81)
					(name "")
					(number "137")
				)
				(pin passive line
					(at 13.97 -172.72 180)
					(length 3.81)
					(name "")
					(number "138")
				)
				(pin passive line
					(at 0 -175.26 0)
					(length 3.81)
					(name "")
					(number "139")
				)
				(pin passive line
					(at 13.97 -175.26 180)
					(length 3.81)
					(name "")
					(number "140")
				)
				(pin passive line
					(at 0 -177.8 0)
					(length 3.81)
					(name "")
					(number "141")
				)
				(pin passive line
					(at 13.97 -177.8 180)
					(length 3.81)
					(name "")
					(number "142")
				)
				(pin passive line
					(at 0 -180.34 0)
					(length 3.81)
					(name "")
					(number "143")
				)
				(pin passive line
					(at 13.97 -180.34 180)
					(length 3.81)
					(name "")
					(number "144")
				)
				(pin passive line
					(at 0 -182.88 0)
					(length 3.81)
					(name "")
					(number "145")
				)
				(pin passive line
					(at 13.97 -182.88 180)
					(length 3.81)
					(name "")
					(number "146")
				)
				(pin passive line
					(at 0 -185.42 0)
					(length 3.81)
					(name "")
					(number "147")
				)
				(pin passive line
					(at 13.97 -185.42 180)
					(length 3.81)
					(name "")
					(number "148")
				)
				(pin passive line
					(at 0 -187.96 0)
					(length 3.81)
					(name "")
					(number "149")
				)
				(pin passive line
					(at 13.97 -187.96 180)
					(length 3.81)
					(name "")
					(number "150")
				)
				(pin passive line
					(at 0 -190.5 0)
					(length 3.81)
					(name "")
					(number "151")
				)
				(pin passive line
					(at 13.97 -190.5 180)
					(length 3.81)
					(name "")
					(number "152")
				)
				(pin passive line
					(at 0 -193.04 0)
					(length 3.81)
					(name "")
					(number "153")
				)
				(pin passive line
					(at 13.97 -193.04 180)
					(length 3.81)
					(name "")
					(number "154")
				)
				(pin passive line
					(at 0 -195.58 0)
					(length 3.81)
					(name "")
					(number "155")
				)
				(pin passive line
					(at 13.97 -195.58 180)
					(length 3.81)
					(name "")
					(number "156")
				)
				(pin passive line
					(at 0 -198.12 0)
					(length 3.81)
					(name "")
					(number "157")
				)
				(pin passive line
					(at 13.97 -198.12 180)
					(length 3.81)
					(name "")
					(number "158")
				)
				(pin passive line
					(at 0 -200.66 0)
					(length 3.81)
					(name "")
					(number "159")
				)
				(pin passive line
					(at 13.97 -200.66 180)
					(length 3.81)
					(name "")
					(number "160")
				)
				(pin passive line
					(at 0 -203.2 0)
					(length 3.81)
					(name "")
					(number "161")
				)
				(pin passive line
					(at 13.97 -203.2 180)
					(length 3.81)
					(name "")
					(number "162")
				)
				(pin passive line
					(at 0 -205.74 0)
					(length 3.81)
					(name "")
					(number "163")
				)
				(pin passive line
					(at 13.97 -205.74 180)
					(length 3.81)
					(name "")
					(number "164")
				)
				(pin passive line
					(at 0 -208.28 0)
					(length 3.81)
					(name "")
					(number "165")
				)
				(pin passive line
					(at 13.97 -208.28 180)
					(length 3.81)
					(name "")
					(number "166")
				)
				(pin passive line
					(at 0 -210.82 0)
					(length 3.81)
					(name "")
					(number "167")
				)
				(pin passive line
					(at 13.97 -210.82 180)
					(length 3.81)
					(name "")
					(number "168")
				)
				(pin passive line
					(at 13.97 -213.36 180)
					(length 3.81)
					(name "")
					(number "MP")
				)
			)
			(embedded_fonts no)
		)
)
