(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Socket_Amphenol_ME1016813401101"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 75.946 -2.286 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Socket_Amphenol_ME1016813401101"
				(at 75.946 -7.366 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Socket_Amphenol_ME1016813401101"
				(at 75.946 -9.906 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://cdn.amphenol-cs.com/media/wysiwyg/files/drawing/cme10168x340x10x.pdf"
				(at 75.946 -12.446 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Standard Card Edge Connectors Mini Cool Edge, Gen Z EDSFF OCP 30 168 pins SMT Straddle Mount"
				(at 75.946 -14.986 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Amphenol"
				(at 75.946 -17.526 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "ME1016813401101"
				(at 75.946 -4.826 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 75.946 -20.066 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 75.946 -22.606 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "EDGE, CONNECTOR, SOCKET, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Socket_Amphenol_ME1016813401101_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "P12V_AUX")
					(number "A1")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "P12V_AUX")
					(number "A2")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "P12V_AUX")
					(number "A3")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "P12V_AUX")
					(number "A4")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A5")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A6")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(name "PRSNT1_HPM_SCM_N")
					(number "A7")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "JTAG_SCMCNTRL_TCK")
					(number "A8")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "JTAG_SCMCNTRL_TDO")
					(number "A9")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(name "JTAG_SCMCNTRL_TDI")
					(number "A10")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "JTAG_SCMCNTRL_TMS")
					(number "A11")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "JTAG_SCMCNTRL_TRST_N")
					(number "A12")
					(alternate "GPIO" passive line)
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "SCM_HPM_STBY_RST_N")
					(number "A13")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "SCM_HPM_STBY_EN")
					(number "A14")
				)
				(pin power_in line
					(at 0 -43.18 0)
					(length 5.08)
					(name "GND")
					(number "A19")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A22")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A25")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A29")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A32")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A35")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A38")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A53")
				)
				(pin passive line
					(at 62.23 -13.97 180)
					(length 5.08)
					(name "GPIO")
					(number "A60")
					(alternate "SPI_SCMCNTRL_IRQ0_N" passive line)
				)
				(pin passive line
					(at 62.23 -22.86 180)
					(length 5.08)
					(name "UART0_HPM_SCM_DATA")
					(number "A63")
					(alternate "GPIO" passive line)
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A64")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A67")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "A70")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B11")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B19")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B22")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B25")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "HPM_SCM_STBY_RDY")
					(number "B26")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "HPM_SCM_INTRUSION_N")
					(number "B27")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "P3V0_HPM_SCM_BAT")
					(number "B28")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B29")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B32")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B35")
				)
				(pin passive line
					(at 62.23 -29.21 180)
					(length 5.08)
					(name "USB2_SCMHOST1_DN")
					(number "B36")
					(alternate "GPIO" passive line)
					(alternate "USB2_HPMHOST1_DN_" passive line)
				)
				(pin passive line
					(at 62.23 -26.67 180)
					(length 5.08)
					(name "USB2_SCMHOST1_DP")
					(number "B37")
					(alternate "GPIO" passive line)
					(alternate "USB2_HPMHOST1_DP_" passive line)
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B38")
				)
				(pin passive line
					(at 62.23 0 180)
					(length 5.08)
					(name "VCC_SCM_HPM_FRU")
					(number "B50")
				)
				(pin passive line
					(at 62.23 -20.32 180)
					(length 5.08)
					(name "UART0_SCM_HPM_DATA")
					(number "B51")
					(alternate "NCSI2_SCM_HPM_TX_EN" passive line)
					(alternate "PCIE_SCM_HPM_PERST_N" passive line)
					(alternate "_GPO" passive line)
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "PRSNT0_SCM_HPM_N")
					(number "B58")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B64")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B67")
				)
				(pin passive line
					(at 62.23 -35.56 180)
					(length 5.08)
					(name "USB2_SCMHOST2_DN")
					(number "B68")
					(alternate "GPIO" passive line)
					(alternate "USB2_HPMHOST2_DN_" passive line)
				)
				(pin passive line
					(at 62.23 -33.02 180)
					(length 5.08)
					(name "USB2_SCMHOST2_DP")
					(number "B69")
					(alternate "GPIO" passive line)
					(alternate "_USB2_HPMHOST2_DP" passive line)
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B70")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "OA1")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "OA4")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "OA7")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "OA10")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "OA13")
				)
				(pin passive line
					(at 62.23 -7.62 180)
					(length 5.08)
					(name "PECI_HPM_SCM")
					(number "OA14")
					(alternate "GPIO" passive line)
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "OB1")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "OB4")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "OB7")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "OB10")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "OB13")
				)
				(pin passive line
					(at 62.23 -5.08 180)
					(length 5.08)
					(name "PECI_VREF_HPM_SCM")
					(number "OB14")
					(alternate "GPI" passive line)
				)
			)
			(symbol "Socket_Amphenol_ME1016813401101_2_1"
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(name "I2C_3V3_0_SCL")
					(number "A15")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "I2C_3V3_0_SDA")
					(number "A16")
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 5.08)
					(name "I2C_3V3_1_SCL")
					(number "A17")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 5.08)
					(name "I2C_3V3_1_SDA")
					(number "A18")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "I2C_3V3_2_SCL")
					(number "A26")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "I2C_3V3_2_SDA")
					(number "A27")
				)
				(pin passive line
					(at 62.23 -38.1 180)
					(length 5.08)
					(name "I2C_I3C_1V0_18_SCL")
					(number "A39")
					(alternate "FSI_1V2_0_SCL" passive line)
				)
				(pin passive line
					(at 62.23 -40.64 180)
					(length 5.08)
					(name "I2C_I3C_1V0_18_SDA")
					(number "A40")
					(alternate "_FSI_1V2_0_SDA" passive line)
				)
				(pin passive line
					(at 62.23 -44.45 180)
					(length 5.08)
					(name "I2C_I3C_1V0_19_SCL")
					(number "A41")
					(alternate "FSI_1V2_1_SCL" passive line)
				)
				(pin passive line
					(at 62.23 -46.99 180)
					(length 5.08)
					(name "I2C_I3C_1V0_19_SDA")
					(number "A42")
					(alternate "FSI_1V2_1_SDA" passive line)
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 5.08)
					(name "I2C_3V3_3_SCL")
					(number "A43")
				)
				(pin passive line
					(at 0 -21.59 0)
					(length 5.08)
					(name "I2C_3V3_3_SDA")
					(number "A44")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "I2C_3V3_4_SCL")
					(number "A45")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "I2C_3V3_4_SDA")
					(number "A46")
				)
				(pin passive line
					(at 0 -31.75 0)
					(length 5.08)
					(name "I2C_3V3_5_SCL")
					(number "A47")
				)
				(pin passive line
					(at 0 -34.29 0)
					(length 5.08)
					(name "I2C_3V3_5_SDA")
					(number "A48")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "I2C_3V3_6_SCL")
					(number "A49")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(name "I2C_3V3_6_SDA")
					(number "A50")
				)
				(pin passive line
					(at 62.23 -27.94 180)
					(length 5.08)
					(name "I2C_I3C_1V8_16_SCL")
					(number "A51")
				)
				(pin passive line
					(at 62.23 -25.4 180)
					(length 5.08)
					(name "I2C_I3C_1V8_16_SDA")
					(number "A52")
				)
				(pin passive line
					(at 0 -64.77 0)
					(length 5.08)
					(name "SPI_HPMCNTRL_TPM_CLK")
					(number "A54")
					(alternate "I2C_I3C_1V8_10_SCL" passive line)
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 5.08)
					(name "SPI_HPMCNTRL_TPM_CS_N")
					(number "A55")
					(alternate "I2C_I3C_1V8_10_SDA_" passive line)
					(alternate "QSPI_HPMCNTRL_TPM_CS_N" passive line)
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 5.08)
					(name "SPI_HPMCNTRL_TPM_DI_IO0")
					(number "A56")
					(alternate "I2C_I3C_1V8_11_SCL" passive line)
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 5.08)
					(name "SPI_HPMCNTRL_TPM_DO_IO1")
					(number "A57")
					(alternate "I2C_I3C_1V8_11_SDA" passive line)
				)
				(pin passive line
					(at 62.23 0 180)
					(length 5.08)
					(name "I2C_I3C_1V8_12_SCL")
					(number "A58")
				)
				(pin passive line
					(at 62.23 -2.54 180)
					(length 5.08)
					(name "I2C_I3C_1V8_12_SDA")
					(number "A59")
				)
				(pin passive line
					(at 62.23 -6.35 180)
					(length 5.08)
					(name "I2C_I3C_1V8_13_SCL")
					(number "A61")
				)
				(pin passive line
					(at 62.23 -8.89 180)
					(length 5.08)
					(name "I2C_I3C_1V8_13_SDA")
					(number "A62")
				)
				(pin passive line
					(at 62.23 -31.75 180)
					(length 5.08)
					(name "I2C_I3C_1V8_17_SCL")
					(number "B9")
					(alternate "ESPI0_HPMCNTRL_CS1_N" passive line)
				)
				(pin passive line
					(at 62.23 -34.29 180)
					(length 5.08)
					(name "I2C_I3C_1V8_17_SDA")
					(number "B10")
					(alternate "ESPI0_HPMCNTRL_ALERT1_N" passive line)
				)
				(pin passive line
					(at 62.23 -12.7 180)
					(length 5.08)
					(name "I2C_I3C_1V8_14_SCL")
					(number "B39")
				)
				(pin passive line
					(at 62.23 -15.24 180)
					(length 5.08)
					(name "I2C_I3C_1V8_14_SDA")
					(number "B40")
				)
				(pin passive line
					(at 62.23 -19.05 180)
					(length 5.08)
					(name "I2C_I3C_1V8_15_SCL")
					(number "B41")
				)
				(pin passive line
					(at 62.23 -21.59 180)
					(length 5.08)
					(name "I2C_I3C_1V8_15_SDA")
					(number "B42")
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 5.08)
					(name "I2C_3V3_7_SCL")
					(number "B52")
					(alternate "NCSI2_HPM_SCM_CLK" passive line)
					(alternate "SGPIO_CLK" passive line)
				)
				(pin passive line
					(at 0 -46.99 0)
					(length 5.08)
					(name "I2C_3V3_7_SDA")
					(number "B53")
					(alternate "NCSI2_HPM_SCM_CRS_DV" passive line)
					(alternate "SGPIO_LD" passive line)
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 5.08)
					(name "I2C_3V3_8_SCL")
					(number "B54")
					(alternate "NCSI2_SCM_HPM_D0" passive line)
					(alternate "SGPIO_DATAOUT" passive line)
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 5.08)
					(name "I2C_3V3_8_SDA")
					(number "B55")
					(alternate "NCSI2_SCM_HPM_D1" passive line)
					(alternate "SGPIO_DATAIN" passive line)
				)
				(pin passive line
					(at 0 -57.15 0)
					(length 5.08)
					(name "I2C_3V3_9_SCL")
					(number "B56")
					(alternate "NCSI2_HPM_SCM_D0" passive line)
					(alternate "UART1_SCM_HPM_DATA_" passive line)
				)
				(pin passive line
					(at 0 -59.69 0)
					(length 5.08)
					(name "I2C_3V3_9_SDA")
					(number "B57")
					(alternate "NCSI2_HPM_SCM_D1" passive line)
					(alternate "UART1_HPM_SCM_DATA_" passive line)
				)
				(pin passive line
					(at 62.23 -67.31 180)
					(length 5.08)
					(name "SPI_SCMCNTRL_CS1_N")
					(number "B59")
					(alternate "GPIO" passive line)
				)
				(pin passive line
					(at 62.23 -62.23 180)
					(length 5.08)
					(name "SPI_SCMCNTRL_CLK")
					(number "B60")
				)
				(pin passive line
					(at 62.23 -71.12 180)
					(length 5.08)
					(name "SPI_SCMCNTRL_DO_IO1")
					(number "B61")
				)
				(pin passive line
					(at 62.23 -73.66 180)
					(length 5.08)
					(name "SPI_SCMCNTRL_DI_IO0")
					(number "B62")
				)
				(pin passive line
					(at 62.23 -64.77 180)
					(length 5.08)
					(name "SPI_SCMCNTRL_CS0_N")
					(number "B63")
				)
			)
			(symbol "Socket_Amphenol_ME1016813401101_3_1"
				(pin passive line
					(at 0 -46.99 0)
					(length 5.08)
					(name "LTPI_SCM_HPM_DATA_DN")
					(number "A20")
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 5.08)
					(name "LTPI_SCM_HPM_DATA_DP")
					(number "A21")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(name "LTPI_SCM_HPM_CLK_DN")
					(number "A23")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "LTPI_SCM_HPM_CLK_DP")
					(number "A24")
				)
				(pin passive line
					(at 62.23 0 180)
					(length 5.08)
					(name "ESPI_HPMCNTRL_CLK")
					(number "B1")
				)
				(pin passive line
					(at 62.23 -2.54 180)
					(length 5.08)
					(name "ESPI_HPMCNTRL_CS0_N")
					(number "B2")
				)
				(pin passive line
					(at 62.23 -5.08 180)
					(length 5.08)
					(name "ESPI_HPMCNTRL_RESET_N")
					(number "B3")
				)
				(pin passive line
					(at 62.23 -7.62 180)
					(length 5.08)
					(name "ESPI_HPMCNTRL_IO_0")
					(number "B4")
				)
				(pin passive line
					(at 62.23 -10.16 180)
					(length 5.08)
					(name "ESPI_HPMCNTRL_IO_1")
					(number "B5")
				)
				(pin passive line
					(at 62.23 -12.7 180)
					(length 5.08)
					(name "ESPI_HPMCNTRL_IO_2")
					(number "B6")
				)
				(pin passive line
					(at 62.23 -15.24 180)
					(length 5.08)
					(name "ESPI_HPMCNTRL_IO_3")
					(number "B7")
				)
				(pin passive line
					(at 62.23 -17.78 180)
					(length 5.08)
					(name "ESPI_HPMCNTRL_ALERT0_N")
					(number "B8")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "QSPI_HPMCNTRL_CLK")
					(number "B12")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(name "QSPI_HPMCNTRL_CS0_N")
					(number "B13")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "QSPI_HPMCNTRL_IO_0")
					(number "B14")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "QSPI_HPMCNTRL_IO_1")
					(number "B15")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "QSPI_HPMCNTRL_IO_2")
					(number "B16")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "QSPI_HPMCNTRL_IO_3")
					(number "B17")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "QSPI_HPMCNTRL_CS1_N")
					(number "B18")
					(alternate "GPIO" passive line)
				)
				(pin passive line
					(at 0 -34.29 0)
					(length 5.08)
					(name "LTPI_HPM_SCM_DATA_DN")
					(number "B20")
				)
				(pin passive line
					(at 0 -31.75 0)
					(length 5.08)
					(name "LTPI_HPM_SCM_DATA_DP")
					(number "B21")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "LTPI_HPM_SCM_CLK_DN")
					(number "B23")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "LTPI_HPM_SCM_CLK_DP")
					(number "B24")
				)
				(pin passive line
					(at 62.23 -31.75 180)
					(length 5.08)
					(name "NCSI_HPM_SCM_CLK")
					(number "B43")
					(alternate "GPIO" passive line)
				)
				(pin passive line
					(at 62.23 -34.29 180)
					(length 5.08)
					(name "NCSI_HPM_SCM_CRS_DV")
					(number "B44")
					(alternate "GPIO" passive line)
				)
				(pin passive line
					(at 62.23 -41.91 180)
					(length 5.08)
					(name "NCSI_SCM_HPM_TX_EN")
					(number "B45")
					(alternate "GPIO" passive line)
				)
				(pin passive line
					(at 62.23 -44.45 180)
					(length 5.08)
					(name "NCSI_SCM_HPM_D0")
					(number "B46")
					(alternate "GPIO" passive line)
				)
				(pin passive line
					(at 62.23 -46.99 180)
					(length 5.08)
					(name "NCSI_SCM_HPM_D1")
					(number "B47")
					(alternate "GPIO" passive line)
				)
				(pin passive line
					(at 62.23 -36.83 180)
					(length 5.08)
					(name "NCSI_HPM_SCM_D0")
					(number "B48")
					(alternate "GPIO" passive line)
				)
				(pin passive line
					(at 62.23 -39.37 180)
					(length 5.08)
					(name "NCSI_HPM_SCM_D1")
					(number "B49")
					(alternate "GPIO" passive line)
				)
			)
			(symbol "Socket_Amphenol_ME1016813401101_4_1"
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(name "PCIE_HPM_SCM_PERST_N")
					(number "A28")
				)
				(pin passive line
					(at 0 -85.09 0)
					(length 5.08)
					(name "PCIE_HPMROOT_SCM_HPM_4_DN")
					(number "A30")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 5.08)
					(name "PCIE_HPMROOT_SCM_HPM_4_DP")
					(number "A31")
				)
				(pin passive line
					(at 0 -107.95 0)
					(length 5.08)
					(name "PCIE_SCMROOT_SCM_HPM_DN")
					(number "A33")
					(alternate "SGMII_SCM_HPM_2_DN" passive line)
					(alternate "USB3_SCMHOST_SCM_HPM_1_DN" passive line)
				)
				(pin passive line
					(at 0 -105.41 0)
					(length 5.08)
					(name "PCIE_SCMROOT_SCM_HPM_DP")
					(number "A34")
					(alternate "SGMII_SCM_HPM_2_DP" passive line)
					(alternate "USB3_SCMHOST_SCM_HPM_1_DP" passive line)
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "PCIE_HPM_SCM_CLK_100M_0_DN")
					(number "A36")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "PCIE_HPM_SCM_CLK_100M_0_DP")
					(number "A37")
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 5.08)
					(name "PCIE_HPMROOT_SCM_HPM_5_DN")
					(number "A65")
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 5.08)
					(name "PCIE_HPMROOT_SCM_HPM_5_DP")
					(number "A66")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(name "PCIE_HPM_SCM_CLK_100M_1_S0_DN")
					(number "A68")
					(alternate "PCIE_HPM_SCM_CLK_100M_1_S5_DN" passive line)
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 5.08)
					(name "PCIE_HPM_SCM_CLK_100M_1_S0_DP")
					(number "A69")
					(alternate "PCIE_HPM_SCM_CLK_100M_1_S5_DP" passive line)
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 5.08)
					(name "PCIE_HPMROOT_HPM_SCM_4_DN")
					(number "B30")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 5.08)
					(name "PCIE_HPMROOT_HPM_SCM_4_DP")
					(number "B31")
				)
				(pin passive line
					(at 0 -114.3 0)
					(length 5.08)
					(name "PCIE_SCMROOT_HPM_SCM_DN")
					(number "B33")
					(alternate "SGMII_HPM_SCM_2_DN" passive line)
					(alternate "USB3_SCMHOST_HPM_SCM_1_DN" passive line)
				)
				(pin passive line
					(at 0 -111.76 0)
					(length 5.08)
					(name "PCIE_SCMROOT_HPM_SCM_DP")
					(number "B34")
					(alternate "SGMII_HPM_SCM_2_DP" passive line)
					(alternate "USB3_SCMHOST_HPM_SCM_1_DP" passive line)
				)
				(pin passive line
					(at 0 -92.71 0)
					(length 5.08)
					(name "PCIE_HPMROOT_HPM_SCM_5_DN")
					(number "B65")
				)
				(pin passive line
					(at 0 -90.17 0)
					(length 5.08)
					(name "PCIE_HPMROOT_HPM_SCM_5_DP")
					(number "B66")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 5.08)
					(name "PCIE_HPMROOT_SCM_HPM_0_DN")
					(number "OA2")
					(alternate "USB3_SCMHOST_SCM_HPM_2_DN" passive line)
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 5.08)
					(name "PCIE_HPMROOT_SCM_HPM_0_DP")
					(number "OA3")
					(alternate "USB3_SCMHOST_SCM_HPM_2_DP" passive line)
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(name "PCIE_HPMROOT_SCM_HPM_1_DN")
					(number "OA5")
					(alternate "DISPLAYPORT_SCM_HPM_LANE0_DN" passive line)
					(alternate "LTPI_SCM_HPM_CLK_2_DN" passive line)
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(name "PCIE_HPMROOT_SCM_HPM_1_DP")
					(number "OA6")
					(alternate "DISPLAYPORT_SCM_HPM_LANE0_DP" passive line)
					(alternate "LTPI_SCM_HPM_CLK_2_DP" passive line)
				)
				(pin passive line
					(at 0 -57.15 0)
					(length 5.08)
					(name "PCIE_HPMROOT_SCM_HPM_2_DN")
					(number "OA8")
					(alternate "SGMII_SCM_HPM_1_DN" passive line)
				)
				(pin passive line
					(at 0 -54.61 0)
					(length 5.08)
					(name "PCIE_HPMROOT_SCM_HPM_2_DP")
					(number "OA9")
					(alternate "SGMII_SCM_HPM_1_DP" passive line)
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 5.08)
					(name "PCIE_HPMROOT_SCM_HPM_3_DN")
					(number "OA11")
					(alternate "DISPLAYPORT_SCM_HPM_LANE1_DN" passive line)
					(alternate "LTPI_SCM_HPM_DATA_2_DN" passive line)
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 5.08)
					(name "PCIE_HPMROOT_SCM_HPM_3_DP")
					(number "OA12")
					(alternate "DISPLAYPORT_SCM_HPM_LANE1_DP" passive line)
					(alternate "LTPI_SCM_HPM_DATA_2_DP" passive line)
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(name "PCIE_HPMROOT_HPM_SCM_0_DN")
					(number "OB2")
					(alternate "USB3_SCMHOST_HPM_SCM_2_DN" passive line)
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "PCIE_HPMROOT_HPM_SCM_0_DP")
					(number "OB3")
					(alternate "USB3_SCMHOST_HPM_SCM_2_DP" passive line)
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(name "PCIE_HPMROOT_HPM_SCM_1_DN")
					(number "OB5")
					(alternate "DISPLAYPORT_AUX_DN" passive line)
					(alternate "LTPI_HPM_SCM_CLK_2_DN" passive line)
				)
				(pin passive line
					(at 0 -34.29 0)
					(length 5.08)
					(name "PCIE_HPMROOT_HPM_SCM_1_DP")
					(number "OB6")
					(alternate "DISPLAYPORT_AUX_DP" passive line)
					(alternate "LTPI_HPM_SCM_CLK_2_DP" passive line)
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 5.08)
					(name "PCIE_HPMROOT_HPM_SCM_2_DN")
					(number "OB8")
					(alternate "SGMII_HPM_SCM_1_DN" passive line)
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 5.08)
					(name "PCIE_HPMROOT_HPM_SCM_2_DP")
					(number "OB9")
					(alternate "SGMII_HPM_SCM_1_DP" passive line)
				)
				(pin passive line
					(at 0 -64.77 0)
					(length 5.08)
					(name "PCIE_HPMROOT_HPM_SCM_3_DN")
					(number "OB11")
					(alternate "LTPI_HPM_SCM_DATA_2_DN__" passive line)
					(alternate "USB2_SCMHOST_3_DN" passive line)
				)
				(pin passive line
					(at 0 -62.23 0)
					(length 5.08)
					(name "PCIE_HPMROOT_HPM_SCM_3_DP")
					(number "OB12")
					(alternate "LTPI_HPM_SCM_DATA_2_DP" passive line)
					(alternate "USB2_SCMHOST_3_DP" passive line)
				)
			)
			(embedded_fonts no)
		)
)
