(footprint "MicroSD_YL004-030-001"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -8.8 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "MicroSD_YL004-030-001"
		(at 0 9.9 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -8.25 12.4 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -8.25 13.6 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -8.25 14.8 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at 2.955 7.41)
		(size 0.8128 1.6764)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 1.855 7.41)
		(size 0.8128 1.6764)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 0.755 7.41)
		(size 0.8128 1.6764)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -0.345 7.41)
		(size 0.8128 1.6764)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -1.445 7.41)
		(size 0.8128 1.6764)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -2.545 7.41)
		(size 0.8128 1.6764)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -3.645 7.41)
		(size 0.8128 1.6764)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -4.745 7.41)
		(size 0.8128 1.6764)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at -6.805 -1.55)
		(size 1.2954 1.397)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at -6.8 5.85)
		(size 1.2954 1.2954)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at -6.695 -7.35)
		(size 1.4986 1.7018)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at -6.145 7.5)
		(size 1.6002 1.4986)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at 6.505 7.5)
		(size 1.7018 1.4986)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at 6.805 -7.35)
		(size 1.4986 1.7018)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_yl004_030_001.glb"
		(offset
			(xyz -3.445 -0.71 -0.35)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 180 0 0)
		)
	)
)
